


CVTXIM(4)           UNIX Programmer's Manual            CVTXIM(4)



NNAAMMEE
     cvt_xim_tbl - key conversion table of Input Manager of the X
     Window System Version 11 (xwnmo(1X))

SSYYNNOOPPSSIISS
     //uussrr//llooccaall//lliibb//wwnnnn//ccvvtt__xxiimm__ttbbll (Default)

DDEESSCCRRIIPPTTIIOONN
     Converts a key code(_K_e_y_S_y_m) generated by _X_L_o_o_k_u_p_S_t_r_i_n_g() to
     a one-byte character(_W_n_n _c_o_d_e) according to preset data.

     CCooddiinngg ffoorrmmaatt::
             [ _S_t_a_t_e-_o_r-_K_e_y_S_y_m <space_character> _W_n_n-_c_o_d_e ]
             _S_t_a_t_e-_o_r-_K_e_y_S_y_m = [_S_t_a_t_e_s]_K_e_y_S_y_m-_n_a_m_e
             _S_t_a_t_e_s = _S_t_a_t_e-_n_a_m_e'|'[_S_t_a_t_e_s]

     Lines that start with a semicolon (;) are comments.

     KeySym-name is a string declarated in keysymdef.h (except
     the prefix "XA_").

     State-name is one between the following string.
             "Shift"   ---> means ShiftMask
             "Ctrl"    ---> means ControlMask
             "Meta"    ---> means Mod1Mask
             "Meta1"   ---> means Mod1Mask (same as "Meta")
             "Meta2"   ---> means Mod2Mask
             "Meta3"   ---> means Mod3Mask
             "Meta4"   ---> means Mod4Mask
             "Meta5"   ---> means Mod5Mask

     CCooddee nnoottaattiioonn::
             0??             ---> Octal
             0x?? or 0X??    ---> Hexadecimal
             ??              ---> Decimal

EEXXAAMMPPLLEE
     Meta|Left            0x9A
     Meta|Up              0x99
     Meta|F11             0x95
     Meta|minus           0x81
     Meta|asciicircum     0x82
     Kanji                0x81
     F1                   0x91
     F2                   0x90
     Meta|Shift|F1        0x91

NNOOTTEESS
     In case of old version _x_w_n_m_o, key codes are converted with
     _c_v_t__f_u_n__t_b_l and _c_v_t__m_e_t_a__t_b_l. For compatibility, those files
     are available if those are specified by option or resource.
     In this case, those two files are loaded before the loading
     of _c_v_t__x_i_m__t_b_l. If duplicate definition is occurred, a warn-
     ing message will be printed and the definition in those two
     files will be taken precedence.

     Codes converted according to this table will be evaluated by
     _2_A__C_T_R_L (default), which is an alphanumeric-phonetic conver-
     sion automation table. After which, they are evaluated by
     _u_u_m_k_e_y.

SSEEEE AALLSSOO
     xwnmo(1X), 2A_CTRL(4_JT), uumkey(4_JT)

CCOOPPYYRRIIGGHHTT
     Copyright 1992 by OMRON Corporation
     Copyright 1992 by Massachusetts Institute of Technology

AAUUTTHHOORR
     Seiji Kuwari (OMRON Corporation)

EEXXAAMMPPLLEE
Printed 12/1/92             Release 5                           2






















































































































