<?xml version="1.0" encoding="utf-8"?>
<!-- $Revision$ -->
<chapter id="encoding-guide">
<title>Encoding with <application>MEncoder</application></title>

<sect1 id="menc-feat-dvd-mpeg4">
<title>Making a high quality MPEG-4 ("DivX")
  rip of a DVD movie</title>

<para>
One frequently asked question is "How do I make the highest quality rip
for a given size?". Another question is "How do I make the highest
quality DVD rip possible? I do not care about file size, I just want the best
quality."
</para>

<para>
The latter question is perhaps at least somewhat wrongly posed. After all, if
you do not care about file size, why not simply copy the entire MPEG-2 video
stream from the the DVD? Sure, your AVI will end up being 5GB, give
or take, but if you want the best quality and do not care about size,
this is certainly your best option.
</para>

<para>
In fact, the reason you want to transcode a DVD into MPEG-4 is
specifically because you <emphasis role="bold">do</emphasis> care about
file size.
</para>

<para>
It is difficult to offer a cookbook recipe on how to create a very high
quality DVD rip. There are several factors to consider, and you should
understand these details or else you are likely to end up disappointed
with your results. Below we will investigate some of these issues, and
then have a look at an example. We assume you are using
<systemitem class="library">libavcodec</systemitem> to encode the video,
although the theory applies to other codecs as well.
</para>

<para>
If this seems to be too much for you, you should probably use one of the
many fine frontends that are listed in the
<ulink url="http://www.mplayerhq.hu/design7/projects.html#mencoder_frontends">MEncoder section</ulink>
of our related projects page.
That way, you should be able to achieve high quality rips without too much
thinking, because most of those tools are designed to take clever decisions
for you.
</para>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-preparing-encode">
<title>Preparing to encode: Identifying source material and framerate</title>

<para>
Before you even think about encoding a movie, you need to take
several preliminary steps.
</para>

<para>
The first and most important step before you encode should be
determining what type of content you are dealing with.
If your source material comes from DVD or broadcast/cable/satellite
TV, it will be stored in one of two formats: NTSC for North
America and Japan, PAL for Europe, etc.
It is important to realize, however, that this is just the formatting for
presentation on a television, and often does
<emphasis role="bold">not</emphasis> correspond to the
original format of the movie.
Experience shows that NTSC material is a lot more difficult to encode,
because there more elements to identify in the source.
In order to produce a suitable encode, you need to know the original
format.
Failure to take this into account will result in various flaws in your
encode, including ugly combing (interlacing) artifacts and duplicated
or even lost frames.
Besides being ugly, the artifacts also harm coding efficiency:
You will get worse quality per unit bitrate.
</para>


<sect3 id="menc-feat-dvd-mpeg4-preparing-encode-fps">
<title>Identifying source framerate</title>

<para>
Here is a list of common types of source material, where you are
likely to find them, and their properties:
</para>

<itemizedlist>
<listitem><para>
  <emphasis role="bold">Standard Film</emphasis>: Produced for
  theatrical display at 24fps.
</para></listitem>
<listitem><para>
  <emphasis role="bold">PAL video</emphasis>: Recorded with a PAL
  video camera at 50 fields per second.
  A field consists of just the odd- or even-numbered lines of a
  frame.
  Television was designed to refresh these in alternation as a
  cheap form of analog compression.
  The human eye supposedly compensates for this, but once you
  understand interlacing you will learn to see it on TV too and
  never enjoy TV again.
  Two fields do <emphasis role="bold">not</emphasis> make a
  complete frame, because they are captured 1/50 of a second apart
  in time, and thus they do not line up unless there is no motion.
</para></listitem>
<listitem><para>
  <emphasis role="bold">NTSC Video</emphasis>: Recorded with an
  NTSC video camera at 60000/1001 fields per second, or 60 fields per
  second in the pre-color era.
  Otherwise similar to PAL.
</para></listitem>
<listitem><para>
  <emphasis role="bold">Animation</emphasis>: Usually drawn at
  24fps, but also comes in mixed-framerate varieties.
</para></listitem>
<listitem><para>
  <emphasis role="bold">Computer Graphics (CG)</emphasis>: Can be
  any framerate, but some are more common than others; 24 and
  30 frames per second are typical for NTSC, and 25fps is typical
  for PAL.
</para></listitem>
<listitem><para>
  <emphasis role="bold">Old Film</emphasis>: Various lower
  framerates.
</para></listitem>
</itemizedlist>
</sect3>


<sect3 id="menc-feat-dvd-mpeg4-preparing-encode-material">
<title>Identifying source material</title>

<para>
Movies consisting of frames are referred to as progressive,
while those consisting of independent fields are called
either interlaced or video - though this latter term is
ambiguous.
</para>

<para>
To further complicate matters, some movies will be a mix of
several of the above.
</para>

<para>
The most important distinction to make between all of these
formats is that some are frame-based, while others are
field-based.
<emphasis role="bold">Whenever</emphasis> a movie is prepared
for display on television (including DVD), it is converted to a
field-based format.
The various methods by which this can be done are collectively
referred to as "telecine", of which the infamous NTSC
"3:2 pulldown" is one variety.
Unless the original material was also field-based (and the same
fieldrate), you are getting the movie in a format other than the
original.
</para>

<itemizedlist>
<title>There are several common types of pulldown:</title>
<listitem><para>
  <emphasis role="bold">PAL 2:2 pulldown</emphasis>: The nicest of
  them all.
  Each frame is shown for the duration of two fields, by extracting the
  even and odd lines and showing them in alternation.
  If the original material is 24fps, this process speeds up the
  movie by 4%.
</para></listitem>
<listitem><para>
  <emphasis role="bold">PAL 2:2:2:2:2:2:2:2:2:2:2:3 pulldown</emphasis>:
  Every 12th frame is shown for the duration of three fields, instead of
  just two.
  This avoids the 4% speedup issue, but makes the process much
  more difficult to reverse.
  It is usually seen in musical productions where adjusting the
  speed by 4% would seriously damage the musical score.
</para></listitem>
<listitem><para>
  <emphasis role="bold">NTSC 3:2 telecine</emphasis>: Frames are
  shown alternately for the duration of 3 fields or 2 fields.
  This gives a fieldrate 2.5 times the original framerate.
  The result is also slowed down very slightly from 60 fields per
  second to 60000/1001 fields per second to maintain NTSC fieldrate.
</para></listitem>
<listitem><para>
  <emphasis role="bold">NTSC 2:2 pulldown</emphasis>: Used for
  showing 30fps material on NTSC.
  Nice, just like 2:2 PAL pulldown.
</para></listitem>
</itemizedlist>

<para>
There are also methods for converting between NTSC and PAL video,
but such topics are beyond the scope of this guide.
If you encounter such a movie and want to encode it, your best
bet is to find a copy in the original format.
Conversion between these two formats is highly destructive and
cannot be reversed cleanly, so your encode will greatly suffer
if it is made from a converted source.
</para>

<para>
When video is stored on DVD, consecutive pairs of fields are
grouped as a frame, even though they are not intended to be shown
at the same moment in time.
The MPEG-2 standard used on DVD and digital TV provides a
way both to encode the original progressive frames and to store
the number of fields for which a frame should be shown in the
header of that frame.
If this method has been used, the movie will often be described
as "soft-telecined", since the process only directs the
DVD player to apply pulldown to the movie rather than altering
the movie itself.
This case is highly preferable since it can easily be reversed
(actually ignored) by the encoder, and since it preserves maximal
quality.
However, many DVD and broadcast production studios do not use
proper encoding techniques but instead produce movies with
"hard telecine", where fields are actually duplicated in the
encoded MPEG-2.
</para>

<para>
The procedures for dealing with these cases will be covered
<link linkend="menc-feat-telecine">later in this guide</link>.
For now, we leave you with some guides to identifying which type
of material you are dealing with:
</para>

<itemizedlist>
<title>NTSC regions:</title>
<listitem><para>
  If <application>MPlayer</application> prints that the framerate
  has changed to 24000/1001 when watching your movie, and never changes
  back, it is almost certainly progressive content that has been
  "soft telecined".
</para></listitem>
<listitem><para>
  If <application>MPlayer</application> shows the framerate
  switching back and forth between 24000/1001 and 30000/1001, and you see
  "combing" at times, then there are several possibilities.
  The 24000/1001 fps segments are almost certainly progressive
  content, "soft telecined", but the 30000/1001 fps parts could be
  either hard-telecined 24000/1001 fps content or 60000/1001 fields per second
  NTSC video.
  Use the same guidelines as the following two cases to determine which.
</para></listitem>
<listitem><para>
  If <application>MPlayer</application> never shows the framerate
  changing, and every single frame with motion appears combed, your
  movie is NTSC video at 60000/1001 fields per second.
</para></listitem>
<listitem><para>
  If <application>MPlayer</application> never shows the framerate
  changing, and two frames out of every five appear combed, your
  movie is "hard telecined" 24000/1001fps content.
</para></listitem>
</itemizedlist>

<itemizedlist>
<title>PAL regions:</title>
<listitem><para>
  If you never see any combing, your movie is 2:2 pulldown.
</para></listitem>
<listitem><para>
  If you see combing alternating in and out every half second,
  then your movie is 2:2:2:2:2:2:2:2:2:2:2:3 pulldown.
</para></listitem>
<listitem><para>
  If you always see combing during motion, then your movie is PAL
  video at 50 fields per second.
</para></listitem>
</itemizedlist>

<note><title>Hint:</title>
<para>
  <application>MPlayer</application> can slow down movie playback
  with the -speed option or play it frame-by-frame.
  Try using <option>-speed</option> 0.2 to watch the movie very
  slowly or press the "<keycap>.</keycap>" key repeatedly to play one frame at
  a time and identify the pattern, if you cannot see it at full speed.
</para>
</note>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-2pass">
<title>Constant quantizer vs. multipass</title>

<para>
It is possible to encode your movie at a wide range of qualities.
With modern video encoders and a bit of pre-codec compression
(downscaling and denoising), it is possible to achieve very good
quality at 700 MB, for a 90-110 minute widescreen movie.
Furthermore, all but the longest movies can be encoded with near-perfect
quality at 1400 MB.
</para>

<para>
There are three approaches to encoding the video: constant bitrate
(CBR), constant quantizer, and multipass (ABR, or average bitrate).
</para>

<para>
The complexity of the frames of a movie, and thus the number of bits
required to compress them, can vary greatly from one scene to another.
Modern video encoders can adjust to these needs as they go and vary
the bitrate.
In simple modes such as CBR, however, the encoders do not know the
bitrate needs of future scenes and so cannot exceed the requested
average bitrate for long stretches of time.
More advanced modes, such as multipass encode, can take into account
the statistics from previous passes; this fixes the problem mentioned
above.
</para>

<note><title>Note:</title>
<para>
Most codecs which support ABR encode only support two pass encode
while some others such as <systemitem class="library">x264</systemitem>,
<systemitem class="library">Xvid</systemitem>
and <systemitem class="library">libavcodec</systemitem> support
multipass, which slightly improves quality at each pass,
yet this improvement is no longer measurable nor noticeable after the
4th or so pass.
Therefore, in this section, two pass and multipass will be used
interchangeably.
</para>
</note>

<para>
In each of these modes, the video codec (such as
<systemitem class="library">libavcodec</systemitem>)
breaks the video frame into 16x16 pixel macroblocks and then applies a
quantizer to each macroblock. The lower the quantizer, the better the
quality and higher the bitrate.
The method the movie encoder uses to determine
which quantizer to use for a given macroblock varies and is highly
tunable. (This is an extreme over-simplification of the actual
process, but the basic concept is useful to understand.)
</para>

<para>
When you specify a constant bitrate, the video codec will encode the video,
discarding
detail as much as necessary and as little as possible in order to remain
lower than the given bitrate. If you truly do not care about file size,
you could as well use CBR and specify a bitrate of infinity. (In
practice, this means a value high enough so that it poses no limit, like
10000Kbit.) With no real restriction on bitrate, the result is that
the codec will use the lowest
possible quantizer for each macroblock (as specified by
<option>vqmin</option> for
<systemitem class="library">libavcodec</systemitem>, which is 2 by default).
As soon as you specify a
low enough bitrate that the codec
is forced to use a higher quantizer, then you are almost certainly ruining
the quality of your video.
In order to avoid that, you should probably downscale your video, according
to the method described later on in this guide.
In general, you should avoid CBR altogether if you care about quality.
</para>

<para>
With constant quantizer, the codec uses the same quantizer, as
specified by the <option>vqscale</option> option (for
<systemitem class="library">libavcodec</systemitem>), on every macroblock.
If you want the highest quality rip possible, again ignoring bitrate,
you can use <option>vqscale=2</option>.
This will yield the same bitrate and PSNR (peak signal-to-noise ratio)
as CBR with
<option>vbitrate</option>=infinity and the default <option>vqmin</option>
of 2.
</para>

<para>
The problem with constant quantizing is that it uses the given quantizer
whether the macroblock needs it or not. That is, it might be possible
to use a higher quantizer on a macroblock without sacrificing visual
quality. Why waste the bits on an unnecessarily low quantizer? Your
CPU has as many cycles as there is time, but there is only so many bits
on your hard disk.
</para>

<para>
With a two pass encode, the first pass will rip the movie as though it
were CBR, but it will keep a log of properties for each frame. This
data is then used during the second pass in order to make intelligent
decisions about which quantizers to use. During fast action or high
detail scenes, higher quantizers will likely be used, and during
slow moving or low detail scenes, lower quantizers will be used.
Normally, the amount of motion is much more important than the
amount of detail.
</para>

<para>
If you use <option>vqscale=2</option>, then you are wasting bits. If you
use <option>vqscale=3</option>, then you are not getting the highest
quality rip. Suppose you rip a DVD at <option>vqscale=3</option>, and
the result is 1800Kbit. If you do a two pass encode with
<option>vbitrate=1800</option>, the resulting video will have
<emphasis role="bold">higher quality</emphasis> for the
<emphasis role="bold">same bitrate</emphasis>.
</para>

<para>
Since you are now convinced that two pass is the way to go, the real
question now is what bitrate to use? The answer is that there is no
single answer. Ideally you want to choose a bitrate that yields the
best balance between quality and file size. This is going to vary
depending on the source video.
</para>

<para>
If size does not matter, a good starting point for a very high quality
rip is about 2000Kbit plus or minus 200Kbit.
For fast action or high detail source video, or if you just have a very
critical eye, you might decide on 2400 or 2600.
For some DVDs, you might not notice a difference at 1400Kbit. It is a
good idea to experiment with scenes at different bitrates to get a feel.
</para>

<para>
If you aim at a certain size, you will have to somehow calculate the bitrate.
But before that, you need to know how much space you should reserve for the
audio track(s), so you should
<link linkend="menc-feat-dvd-mpeg4-audio">rip those</link> first.
You can compute the bitrate with the following equation:
<systemitem>bitrate = (target_size_in_Mbytes - sound_size_in_Mbytes) *
1024 * 1024 / length_in_secs * 8 / 1000</systemitem>
For instance, to squeeze a two-hour movie onto a 702MB CD, with 60MB
of audio track, the video bitrate will have to be:
<systemitem>(702 - 60) * 1024 * 1024 / (120*60) * 8 / 1000
= 740kbps</systemitem>
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-constraints">
<title>Constraints for efficient encoding</title>

<para>
Due to the nature of MPEG-type compression, there are various
constraints you should follow for maximal quality.
MPEG splits the video up into 16x16 squares called macroblocks,
each composed of 4 8x8 blocks of luma (intensity) information and two
half-resolution 8x8 chroma (color) blocks (one for red-cyan axis and
the other for the blue-yellow axis).
Even if your movie width and height are not multiples of 16, the
encoder will use enough 16x16 macroblocks to cover the whole picture
area, and the extra space will go to waste.
So in the interests of maximizing quality at a fixed file size, it is
a bad idea to use dimensions that are not multiples of 16.
</para>

<para>
Most DVDs also have some degree of black borders at the edges. Leaving
these in place will hurt quality <emphasis role="bold">a lot</emphasis>
in several ways.
</para>

<orderedlist>
<listitem>
  <para>
  MPEG-type compression is highly dependent on frequency domain
  transformations, in particular the Discrete Cosine Transform (DCT),
  which is similar to the Fourier transform. This sort of encoding is
  efficient for representing patterns and smooth transitions, but it
  has a hard time with sharp edges. In order to encode them it must
  use many more bits, or else an artifact known as ringing will
  appear.
  </para>

  <para>
  The frequency transform (DCT) takes place separately on each
  macroblock (actually each block), so this problem only applies when
  the sharp edge is inside a block. If your black borders begin
  exactly at multiple-of-16 pixel boundaries, this is not a problem.
  However, the black borders on DVDs rarely come nicely aligned, so
  in practice you will always need to crop to avoid this penalty.
  </para>
</listitem>
</orderedlist>

<para>
In addition to frequency domain transforms, MPEG-type compression uses
motion vectors to represent the change from one frame to the next.
Motion vectors naturally work much less efficiently for new content
coming in from the edges of the picture, because it is not present in
the previous frame. As long as the picture extends all the way to the
edge of the encoded region, motion vectors have no problem with
content moving out the edges of the picture. However, in the presence
of black borders, there can be trouble:
</para>

<orderedlist continuation="continues">
<listitem>
  <para>
  For each macroblock, MPEG-type compression stores a vector
  identifying which part of the previous frame should be copied into
  this macroblock as a base for predicting the next frame. Only the
  remaining differences need to be encoded. If a macroblock spans the
  edge of the picture and contains part of the black border, then
  motion vectors from other parts of the picture will overwrite the
  black border. This means that lots of bits must be spent either
  re-blackening the border that was overwritten, or (more likely) a
  motion vector will not be used at all and all the changes in this
  macroblock will have to be coded explicitly. Either way, encoding
  efficiency is greatly reduced.
  </para>

  <para>
  Again, this problem only applies if black borders do not line up on
  multiple-of-16 boundaries.
  </para>
</listitem>

<listitem>
  <para>
  Finally, suppose we have a macroblock in the interior of the
  picture, and an object is moving into this block from near the edge
  of the image. MPEG-type coding cannot say "copy the part that is
  inside the picture but not the black border." So the black border
  will get copied inside too, and lots of bits will have to be spent
  encoding the part of the picture that is supposed to be there.
  </para>

  <para>
  If the picture runs all the way to the edge of the encoded area,
  MPEG has special optimizations to repeatedly copy the pixels at the
  edge of the picture when a motion vector comes from outside the
  encoded area. This feature becomes useless when the movie has black
  borders. Unlike problems 1 and 2, aligning the borders at multiples
  of 16 does not help here.
  </para>
</listitem>

<listitem><para>
  Despite the borders being entirely black and never changing, there
  is at least a minimal amount of overhead involved in having more
  macroblocks.
</para></listitem>
</orderedlist>

<para>
For all of these reasons, it is recommended to fully crop black
borders. Further, if there is an area of noise/distortion at the edge
of the picture, cropping this will improve encoding efficiency as
well. Videophile purists who want to preserve the original as close as
possible may object to this cropping, but unless you plan to encode at
constant quantizer, the quality you gain from cropping will
considerably exceed the amount of information lost at the edges.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-crop">
<title>Cropping and Scaling</title>

<para>
Recall from the previous section that the final picture size you
encode should be a multiple of 16 (in both width and height).
This can be achieved by cropping, scaling, or a combination of both.
</para>

<para>
When cropping, there are a few guidelines that must be followed to
avoid damaging your movie.
The normal YUV format, 4:2:0, stores chroma (color) information
subsampled, i.e. chroma is only sampled half as often in each
direction as luma (intensity) information.
Observe this diagram, where L indicates luma sampling points and C
chroma.
</para>

<informaltable>
<?dbhtml table-width="40%" ?>
<?dbfo table-width="40%" ?>
<tgroup cols="8" align="center">
<colspec colnum="1" colname="col1"/>
<colspec colnum="2" colname="col2"/>
<colspec colnum="3" colname="col3"/>
<colspec colnum="4" colname="col4"/>
<colspec colnum="5" colname="col5"/>
<colspec colnum="6" colname="col6"/>
<colspec colnum="7" colname="col7"/>
<colspec colnum="8" colname="col8"/>
<spanspec spanname="spa1-2" namest="col1" nameend="col2"/>
<spanspec spanname="spa3-4" namest="col3" nameend="col4"/>
<spanspec spanname="spa5-6" namest="col5" nameend="col6"/>
<spanspec spanname="spa7-8" namest="col7" nameend="col8"/>
  <tbody>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
    <row>
      <entry spanname="spa1-2">C</entry>
      <entry spanname="spa3-4">C</entry>
      <entry spanname="spa5-6">C</entry>
      <entry spanname="spa7-8">C</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
    <row>
      <entry spanname="spa1-2">C</entry>
      <entry spanname="spa3-4">C</entry>
      <entry spanname="spa5-6">C</entry>
      <entry spanname="spa7-8">C</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
  </tbody>
</tgroup>
</informaltable>

<para>
As you can see, rows and columns of the image naturally come in pairs.
Thus your crop offsets and dimensions <emphasis>must</emphasis> be
even numbers.
If they are not, the chroma will no longer line up correctly with the
luma.
In theory, it is possible to crop with odd offsets, but it requires
resampling the chroma which is potentially a lossy operation and not
supported by the crop filter.
</para>

<para>
Further, interlaced video is sampled as follows:
</para>

<informaltable>
<?dbhtml table-width="80%" ?>
<?dbfo table-width="80%" ?>
<tgroup cols="16" align="center">
<colspec colnum="1"  colname="col1"/>
<colspec colnum="2"  colname="col2"/>
<colspec colnum="3"  colname="col3"/>
<colspec colnum="4"  colname="col4"/>
<colspec colnum="5"  colname="col5"/>
<colspec colnum="6"  colname="col6"/>
<colspec colnum="7"  colname="col7"/>
<colspec colnum="8"  colname="col8"/>
<colspec colnum="9"  colname="col9"/>
<colspec colnum="10" colname="col10"/>
<colspec colnum="11" colname="col11"/>
<colspec colnum="12" colname="col12"/>
<colspec colnum="13" colname="col13"/>
<colspec colnum="14" colname="col14"/>
<colspec colnum="15" colname="col15"/>
<colspec colnum="16" colname="col16"/>
<spanspec spanname="spa1-2"   namest="col1" nameend="col2"/>
<spanspec spanname="spa3-4"   namest="col3" nameend="col4"/>
<spanspec spanname="spa5-6"   namest="col5" nameend="col6"/>
<spanspec spanname="spa7-8"   namest="col7" nameend="col8"/>
<spanspec spanname="spa9-10"  namest="col9" nameend="col10"/>
<spanspec spanname="spa11-12" namest="col11" nameend="col12"/>
<spanspec spanname="spa13-14" namest="col13" nameend="col14"/>
<spanspec spanname="spa15-16" namest="col15" nameend="col16"/>
  <tbody>
    <row>
      <entry namest="col1" nameend="col8">Top field</entry>
      <entry namest="col9" nameend="col16">Bottom field</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry spanname="spa1-2">C</entry>
      <entry spanname="spa3-4">C</entry>
      <entry spanname="spa5-6">C</entry>
      <entry spanname="spa7-8">C</entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry spanname="spa9-10">C</entry>
      <entry spanname="spa11-12">C</entry>
      <entry spanname="spa13-14">C</entry>
      <entry spanname="spa15-16">C</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry spanname="spa1-2">C</entry>
      <entry spanname="spa3-4">C</entry>
      <entry spanname="spa5-6">C</entry>
      <entry spanname="spa7-8">C</entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
    <row>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry spanname="spa9-10">C</entry>
      <entry spanname="spa11-12">C</entry>
      <entry spanname="spa13-14">C</entry>
      <entry spanname="spa15-16">C</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry></entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
      <entry>L</entry>
    </row>
  </tbody>
</tgroup>
</informaltable>

<para>
As you can see, the pattern does not repeat until after 4 lines.
So for interlaced video, your y-offset and height for cropping must
be multiples of 4.
</para>

<para>
Native DVD resolution is 720x480 for NTSC, and 720x576 for PAL, but
there is an aspect flag that specifies whether it is full-screen (4:3) or
wide-screen (16:9). Many (if not most) widescreen DVDs are not strictly
16:9, and will be either 1.85:1 or 2.35:1 (cinescope). This means that
there will be black bands in the video that will need to be cropped out.
</para>

<para>
<application>MPlayer</application> provides a crop detection filter that
will determine the crop rectangle (<option>-vf cropdetect</option>).
Run <application>MPlayer</application> with
<option>-vf cropdetect</option> and it will print out the crop
settings to remove the borders.
You should let the movie run long enough that the whole picture
area is used, in order to get accurate crop values.
</para>

<para>
Then, test the values you get with <application>MPlayer</application>,
using the command line which was printed by
<option>cropdetect</option>, and adjust the rectangle as needed.
The <option>rectangle</option> filter can help by allowing you to
interactively position the crop rectangle over your movie.
Remember to follow the above divisibility guidelines so that you
do not misalign the chroma planes.
</para>

<para>
In certain cases, scaling may be undesirable.
Scaling in the vertical direction is difficult with interlaced
video, and if you wish to preserve the interlacing, you should
usually refrain from scaling.
If you will not be scaling but you still want to use multiple-of-16
dimensions, you will have to overcrop.
Do not undercrop, since black borders are very bad for encoding!
</para>

<para>
Because MPEG-4 uses 16x16 macroblocks, you will want to make sure that each
dimension of the video you are encoding is a multiple of 16 or else you
will be degrading quality, especially at lower bitrates. You can do this
by rounding the width and height of the crop rectangle down to the nearest
multiple of 16.
As stated earlier, when cropping, you will want to increase the Y offset by
half the difference of the old and the new height so that the resulting
video is taken from the center of the frame. And because of the way DVD
video is sampled, make sure the offset is an even number. (In fact, as a
rule, never use odd values for any parameter when you are cropping and
scaling video.) If you are not comfortable throwing a few extra pixels
away, you might prefer to scale the video instead. We will look
at this in our example below.
You can actually let the <option>cropdetect</option> filter do all of the
above for you, as it has an optional <option>round</option> parameter that
is equal to 16 by default.
</para>

<para>
Also, be careful about "half black" pixels at the edges. Make sure you
crop these out too, or else you will be wasting bits there that
are better spent elsewhere.
</para>

<para>
After all is said and done, you will probably end up with video whose pixels
are not quite 1.85:1 or 2.35:1, but rather something close to that. You
could calculate the new aspect ratio manually, but
<application>MEncoder</application> offers an option for <systemitem
class="library">libavcodec</systemitem> called <option>autoaspect</option>
that will do this for you. Absolutely do not scale this video up in order to
square the pixels unless you like to waste your hard disk space. Scaling
should be done on playback, and the player will use the aspect stored in
the AVI to determine the correct resolution.
Unfortunately, not all players enforce this auto-scaling information,
therefore you may still want to rescale.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-resolution-bitrate">
<title>Choosing resolution and bitrate</title>

<para>
If you will not be encoding in constant quantizer mode, you need to
select a bitrate.
The concept of bitrate is quite simple.
It is the (average) number of bits that will be consumed to store your
movie, per second.
Normally bitrate is measured in kilobits (1000 bits) per second.
The size of your movie on disk is the bitrate times the length of the
movie in time, plus a small amount of "overhead" (see the section on
<link linkend="menc-feat-dvd-mpeg4-muxing-avi-limitations">the AVI container</link>
for instance).
Other parameters such as scaling, cropping, etc. will
<emphasis role="bold">not</emphasis> alter the file size unless you
change the bitrate as well!
</para>

<para>
Bitrate does <emphasis role="bold">not</emphasis> scale proportionally
to resolution.
That is to say, a 320x240 file at 200 kbit/sec will not be the same
quality as the same movie at 640x480 and 800 kbit/sec!
There are two reasons for this:
<orderedlist>
<listitem><para>
  <emphasis role="bold">Perceptual</emphasis>: You notice MPEG
  artifacts more if they are scaled up bigger!
  Artifacts appear on the scale of blocks (8x8).
  Your eye will not see errors in 4800 small blocks as easily as it
  sees errors in 1200 large blocks (assuming you will be scaling both
  to fullscreen).
</para></listitem>
<listitem><para>
  <emphasis role="bold">Theoretical</emphasis>: When you scale down
  an image but still use the same size (8x8) blocks for the frequency
  space transform, you move more data to the high frequency bands.
  Roughly speaking, each pixel contains more of the detail than it
  did before.
  So even though your scaled-down picture contains 1/4 the information
  in the spacial directions, it could still contain a large portion
  of the information in the frequency domain (assuming that the high
  frequencies were underutilized in the original 640x480 image).
</para></listitem>
</orderedlist>
</para>

<para>
Past guides have recommended choosing a bitrate and resolution based
on a "bits per pixel" approach, but this is usually not valid due to
the above reasons.
A better estimate seems to be that bitrates scale proportional to the
square root of resolution, so that 320x240 and 400 kbit/sec would be
comparable to 640x480 at 800 kbit/sec.
However this has not been verified with theoretical or empirical
rigor.
Further, given that movies vary greatly with regard to noise, detail,
degree of motion, etc., it is futile to make general recommendations
for bits per length-of-diagonal (the analog of bits per pixel,
using the square root).
</para>
<para>
So far we have discussed the difficulty of choosing a bitrate and
resolution.
</para>


<sect3 id="menc-feat-dvd-mpeg4-resolution-bitrate-compute">
<title>Computing the resolution</title>

<para>
The following steps will guide you in computing the resolution of your
encode without distorting the video too much, by taking into account several
types of information about the source video.
First, you should compute the encoded aspect ratio:
<systemitem>ARc = (Wc x (ARa / PRdvd )) / Hc</systemitem>

<itemizedlist>
<title>where:</title>
<listitem><para>
  Wc and Hc are the width and height of the cropped video,
</para></listitem>
<listitem><para>
  ARa is the displayed aspect ratio, which usually is 4/3 or 16/9,
</para></listitem>
<listitem><para>
  PRdvd is the pixel ratio of the DVD which is equal to 1.25=(720/576) for PAL
  DVDs and 1.5=(720/480) for NTSC DVDs.
</para></listitem>
</itemizedlist>
</para>

<para>
Then, you can compute the X and Y resolution, according to a certain
Compression Quality (CQ) factor:
<systemitem>ResY = INT(SQRT( 1000*Bitrate/25/ARc/CQ )/16) * 16</systemitem>
and
<systemitem>ResX = INT( ResY * ARc / 16) * 16</systemitem>
</para>

<para>
Okay, but what is the CQ?
The CQ represents the number of bits per pixel and per frame of the encode.
Roughly speaking, the greater the CQ, the less the likelihood to see
encoding artifacts.
However, if you have a target size for your movie (1 or 2 CDs for instance),
there is a limited total number of bits that you can spend; therefore it is
necessary to find a good tradeoff between compressibility and quality.
</para>

<para>
The CQ depends on the bitrate, the video codec efficiency and the
movie resolution.
In order to raise the CQ, typically you would downscale the movie given that the
bitrate is computed in function of the target size and the length of the
movie, which are constant.
With MPEG-4 ASP codecs such as <systemitem class="library">Xvid</systemitem>
and <systemitem class="library">libavcodec</systemitem>, a CQ below 0.18
usually results in a pretty blocky picture, because there
are not enough bits to code the information of each macroblock. (MPEG4, like
many other codecs, groups pixels by blocks of several pixels to compress the
image; if there are not enough bits, the edges of those blocks are
visible.)
It is therefore wise to take a CQ ranging from 0.20 to 0.22 for a 1 CD rip,
and 0.26-0.28 for 2 CDs rip with standard encoding options.
More advanced encoding options such as those listed here for
<link linkend="menc-feat-mpeg4-lavc-example-settings"><systemitem class="library">libavcodec</systemitem></link>
and
<link linkend="menc-feat-xvid-example-settings"><systemitem class="library">Xvid</systemitem></link>
should make it possible to get the same quality with CQ ranging from
0.18 to 0.20 for a 1 CD rip, and 0.24 to 0.26 for a 2 CD rip.
With MPEG-4 AVC codecs such as <systemitem class="library">x264</systemitem>,
you can use a CQ ranging from 0.14 to 0.16 with standard encoding options,
and should be able to go as low as 0.10 to 0.12 with
<link linkend="menc-feat-x264-example-settings"><systemitem class="library">x264</systemitem>'s advanced encoding settings</link>.
</para>

<para>
Please take note that the CQ is just an indicative figure, as depending on
the encoded content, a CQ of 0.18 may look just fine for a Bergman, contrary
to a movie such as The Matrix, which contains many high-motion scenes.
On the other hand, it is worthless to raise CQ higher than 0.30 as you would
be wasting bits without any noticeable quality gain.
Also note that as mentioned earlier in this guide, low resolution videos
need a bigger CQ (compared to, for instance, DVD resolution) to look good.
</para>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-filtering">
<title>Filtering</title>

<para>
Learning how to use <application>MEncoder</application>'s video filters
is essential to producing good encodes.
All video processing is performed through the filters -- cropping,
scaling, color adjustment, noise removal, sharpening, deinterlacing,
telecine, inverse telecine, and deblocking, just to name a few.
Along with the vast number of supported input formats, the variety of
filters available in <application>MEncoder</application> is one of its
main advantages over other similar programs.
</para>

<para>
Filters are loaded in a chain using the -vf option:

<screen>-vf filter1=options,filter2=options,...</screen>

Most filters take several numeric options separated by colons, but
the syntax for options varies from filter to filter, so read the man
page for details on the filters you wish to use.
</para>

<para>
Filters operate on the video in the order they are loaded.
For example, the following chain:

<screen>-vf crop=688:464:12:4,scale=640:464</screen>

will first crop the 688x464 region of the picture with upper-left
corner at (12,4), and then scale the result down to 640x464.
</para>

<para>
Certain filters need to be loaded at or near the beginning of the
filter chain, in order to take advantage of information from the
video decoder that will be lost or invalidated by other filters.
The principal examples are <option>pp</option> (postprocessing, only
when it is performing deblock or dering operations),
<option>spp</option> (another postprocessor to remove MPEG artifacts),
<option>pullup</option> (inverse telecine), and
<option>softpulldown</option> (for converting soft telecine to hard telecine).
</para>

<para>
In general, you want to do as little filtering as possible to the movie
in order to remain close to the original DVD source. Cropping is often
necessary (as described above), but avoid to scale the video. Although
scaling down is sometimes preferred to using higher quantizers, we want
to avoid both these things: remember that we decided from the start to
trade bits for quality.
</para>

<para>
Also, do not adjust gamma, contrast, brightness, etc. What looks good
on your display may not look good on others. These adjustments should
be done on playback only.
</para>

<para>
One thing you might want to do, however, is pass the video through a
very light denoise filter, such as <option>-vf hqdn3d=2:1:2</option>.
Again, it is a matter of putting those bits to better use: why waste them
encoding noise when you can just add that noise back in during playback?
Increasing the parameters for <option>hqdn3d</option> will further
improve compressibility, but if you increase the values too much, you
risk degrading the image visibly. The suggested values above
(<option>2:1:2</option>) are quite conservative; you should feel free to
experiment with higher values and observe the results for yourself.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-interlacing">
<title>Interlacing and Telecine</title>

<para>
Almost all movies are shot at 24 fps. Because NTSC is 30000/1001 fps, some
processing must be done to this 24 fps video to make it run at the correct
NTSC framerate. The process is called 3:2 pulldown, commonly referred to
as telecine (because pulldown is often applied during the telecine
process), and, naively described, it works by slowing the film down to
24000/1001 fps, and repeating every fourth frame.
</para>

<para>
No special processing, however, is done to the video for PAL DVDs, which
run at 25 fps. (Technically, PAL can be telecined, called 2:2 pulldown,
but this does not become an issue in practice.) The 24 fps film is simply
played back at 25 fps. The result is that the movie runs slightly faster,
but unless you are an alien, you probably will not notice the difference.
Most PAL DVDs have pitch-corrected audio, so when they are played back at
25 fps things will sound right, even though the audio track (and hence the
whole movie) has a running time that is 4% less than NTSC DVDs.
</para>

<para>
Because the video in a PAL DVD has not been altered, you need not worry
much about framerate. The source is 25 fps, and your rip will be 25
fps. However, if you are ripping an NTSC DVD movie, you may need to
apply inverse telecine.
</para>

<para>
For movies shot at 24 fps, the video on the NTSC DVD is either telecined
30000/1001, or else it is progressive 24000/1001 fps and intended to be
telecined on-the-fly by a DVD player. On the other hand, TV series are usually
only interlaced, not telecined. This is not a hard rule: some TV series
are interlaced (such as Buffy the Vampire Slayer) whereas some are a
mixture of progressive and interlaced (such as Angel, or 24).
</para>

<para>
It is highly recommended that you read the section on
<link linkend="menc-feat-telecine">How to deal with telecine and interlacing in NTSC DVDs</link>
to learn how to handle the different possibilities.
</para>

<para>
However, if you are mostly just ripping movies, likely you are either
dealing with 24 fps progressive or telecined video, in which case you can
use the <option>pullup</option> filter <option>-vf
pullup,softskip</option>.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-encoding-interlaced">
<title>Encoding interlaced video</title>

<para>
If the movie you want to encode is interlaced (NTSC video or
PAL video), you will need to choose whether you want to
deinterlace or not.
While deinterlacing will make your movie usable on progressive
scan displays such a computer monitors and projectors, it comes
at a cost: The fieldrate of 50 or 60000/1001 fields per second
is halved to 25 or 30000/1001 frames per second, and roughly half of
the information in your movie will be lost during scenes with
significant motion.
</para>

<para>
Therefore, if you are encoding for high quality archival purposes,
it is recommended not to deinterlace.
You can always deinterlace the movie at playback time when
displaying it on progressive scan devices.
The power of currently available computers forces players to use a
deinterlacing filter, which results in a slight degradation in
image quality.
But future players will be able to mimic the interlaced display of
a TV, deinterlacing to full fieldrate and interpolating 50 or
60000/1001 entire frames per second from the interlaced video.
</para>

<para>
Special care must be taken when working with interlaced video:
</para>

<orderedlist>
<listitem><para>
  Crop height and y-offset must be multiples of 4.
</para></listitem>
<listitem><para>
  Any vertical scaling must be performed in interlaced mode.
</para></listitem>
<listitem><para>
  Postprocessing and denoising filters may not work as expected
  unless you take special care to operate them a field at a time,
  and they may damage the video if used incorrectly.
</para></listitem>
</orderedlist>

<para>
With these things in mind, here is our first example:
<screen>
mencoder <replaceable>capture.avi</replaceable> -mc 0 -oac lavc -ovc lavc -lavcopts \
    vcodec=mpeg2video:vbitrate=6000:ilme:ildct:acodec=mp2:abitrate=224
</screen>
Note the <option>ilme</option> and <option>ildct</option> options.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-av-sync">
<title>Notes on Audio/Video synchronization</title>

<para>
<application>MEncoder</application>'s audio/video synchronization
algorithms were designed with the intention of recovering files with
broken sync.
However, in some cases they can cause unnecessary skipping and duplication of
frames, and possibly slight A/V desync, when used with proper input
(of course, A/V sync issues apply only if you process or copy the
audio track while transcoding the video, which is strongly encouraged).
Therefore, you may have to switch to basic A/V sync with
the <option>-mc 0</option> option, or put this in your
<systemitem>~/.mplayer/mencoder</systemitem> config file, as long as
you are only working with good sources (DVD, TV capture, high quality
MPEG-4 rips, etc) and not broken ASF/RM/MOV files.
</para>

<para>
If you want to further guard against strange frame skips and
duplication, you can use both <option>-mc 0</option> and
<option>-noskip</option>.
This will prevent <emphasis>all</emphasis> A/V sync, and copy frames
one-to-one, so you cannot use it if you will be using any filters that
unpredictably add or drop frames, or if your input file has variable
framerate!
Therefore, using <option>-noskip</option> is not in general recommended.
</para>

<para>
The so-called "three-pass" audio encoding which
<application>MEncoder</application> supports has been reported to cause A/V
desync.
This will definitely happen if it is used in conjunction with certain
filters, therefore, it is now recommended <emphasis>not</emphasis> to
use three-pass audio mode.
This feature is only left for compatibility purposes and for expert
users who understand when it is safe to use and when it is not.
If you have never heard of three-pass mode before, forget that we
even mentioned it!
</para>

<para>
There have also been reports of A/V desync when encoding from stdin
with <application>MEncoder</application>.
Do not do this! Always use a file or CD/DVD/etc device as input.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-codec">
<title>Choosing the video codec</title>

<para>
Which video codec is best to choose depends on several factors,
like size, quality, streamability, usability and popularity, some of
which widely depend on personal taste and technical constraints.
</para>
<itemizedlist>
<listitem>
  <para>
  <emphasis role="bold">Compression efficiency</emphasis>:
  It is quite easy to understand that most newer-generation codecs are
  made to increase quality and compression.
  Therefore, the authors of this guide and many other people suggest that
  you cannot go wrong
  <footnote id='fn-menc-feat-dvd-mpeg4-codec-cpu'><para>
  Be careful, however: Decoding DVD-resolution MPEG-4 AVC videos
  requires a fast machine (i.e. a Pentium 4 over 1.5GHz or a Pentium M
  over 1GHz).
  </para></footnote>
  when choosing MPEG-4 AVC codecs like
  <systemitem class="library">x264</systemitem> instead of MPEG-4 ASP codecs
  such as <systemitem class="library">libavcodec</systemitem> MPEG-4 or
  <systemitem class="library">Xvid</systemitem>.
  (Advanced codec developers may be interested in reading Michael
  Niedermayer's opinion on
  "<ulink url="http://guru.multimedia.cx/?p=10">why MPEG4-ASP sucks</ulink>".)
  Likewise, you should get better quality using MPEG-4 ASP than you
  would with MPEG-2 codecs.
  </para>

  <para>
  However, newer codecs which are in heavy development can suffer from
  bugs which have not yet been noticed and which can ruin an encode.
  This is simply the tradeoff for using bleeding-edge technology.
  </para>

  <para>
  What is more, beginning to use a new codec requires that you spend some
  time becoming familiar with its options, so that you know what
  to adjust to achieve a desired picture quality.
  </para>
</listitem>

<listitem><para>
  <emphasis role="bold">Hardware compatibility</emphasis>:
  It usually takes a long time for standalone video players to begin to
  include support for the latest video codecs.
  As a result, most only support MPEG-1 (like VCD, XVCD and KVCD), MPEG-2
  (like DVD, SVCD and KVCD) and MPEG-4 ASP (like DivX,
  <systemitem class="library">libavcodec</systemitem>'s LMP4 and
  <systemitem class="library">Xvid</systemitem>)
  (Beware: Usually, not all MPEG-4 ASP features are supported).
  Please refer to the technical specs of your player (if they are available),
  or google around for more information.
</para></listitem>

<listitem>
  <para>
  <emphasis role="bold">Best quality per encoding time</emphasis>:
  Codecs that have been around for some time (such as
  <systemitem class="library">libavcodec</systemitem> MPEG-4 and
  <systemitem class="library">Xvid</systemitem>) are usually heavily
  optimized with all kinds of smart algorithms and SIMD assembly code.
  That is why they tend to yield the best quality per encoding time ratio.
  However, they may have some very advanced options that, if enabled,
  will make the encode really slow for marginal gains.
  </para>

  <para>
  If you are after blazing speed you should stick around the default
  settings of the video codec (although you should still try the other
  options which are mentioned in other sections of this guide).
  </para>

  <para>
  You may also consider choosing a codec which can do multi-threaded
  processing, though this is only useful for users of machines with
  several CPUs.
  <systemitem class="library">libavcodec</systemitem> MPEG-4 does
  allow that, but speed gains are limited, and there is a slight
  negative effect on picture quality.
  <systemitem class="library">Xvid</systemitem>'s multi-threaded encoding,
  activated by the <option>threads</option> option, can be used to
  boost encoding speed &mdash; by about 40-60% in typical cases &mdash;
  with little if any picture degradation.
  <systemitem class="library">x264</systemitem> also allows multi-threaded
  encoding, which currently speeds up encoding by 94% per CPU core while
  lowering PSNR between 0.005dB and 0.01dB on a typical setup.
  </para>
</listitem>

<listitem>
  <para>
  <emphasis role="bold">Personal taste</emphasis>:
  This is where it gets almost irrational: For the same reason that some
  hung on to DivX&nbsp;3 for years when newer codecs were already doing wonders,
  some folks will prefer <systemitem class="library">Xvid</systemitem>
  or <systemitem class="library">libavcodec</systemitem> MPEG-4 over
  <systemitem class="library">x264</systemitem>.
  </para>
  <para>
  You should make your own judgement; do not take advice from people who
  swear by one codec.
  Take a few sample clips from raw sources and compare different
  encoding options and codecs to find one that suits you best.
  The best codec is the one you master, and the one that looks
  best to your eyes on your display
  <footnote id='fn-menc-feat-dvd-mpeg4-codec-playback'><para>
  The same encode may not look the same on someone else's monitor or
  when played back by a different decoder, so future-proof your encodes by
  playing them back on different setups.
  </para></footnote>!
  </para>
</listitem>
</itemizedlist>

<para>
Please refer to the section
<link linkend="menc-feat-selecting-codec">selecting codecs and container formats</link>
to get a list of supported codecs.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-audio">
<title>Audio</title>

<para>
Audio is a much simpler problem to solve: if you care about quality, just
leave it as is.
Even AC-3 5.1 streams are at most 448Kbit/s, and they are worth every bit.
You might be tempted to transcode the audio to high quality Vorbis, but
just because you do not have an A/V receiver for AC-3 pass-through today
does not mean you will not have one tomorrow. Future-proof your DVD rips by
preserving the AC-3 stream.
You can keep the AC-3 stream either by copying it directly into the video
stream <link linkend="menc-feat-mpeg4">during the encoding</link>.
You can also extract the AC-3 stream in order to mux it into containers such
as NUT or Matroska.
<screen>
mplayer <replaceable>source_file.vob</replaceable> -aid 129 -dumpaudio -dumpfile <replaceable>sound.ac3</replaceable>
</screen>
will dump into the file <replaceable>sound.ac3</replaceable> the
audio track number 129 from the file
<replaceable>source_file.vob</replaceable> (NB: DVD VOB files
usually use a different audio numbering,
which means that the VOB audio track 129 is the 2nd audio track of the file).
</para>

<para>
But sometimes you truly have no choice but to further compress the
sound so that more bits can be spent on the video.
Most people choose to compress audio with either MP3 or Vorbis audio codecs.
While the latter is a very space-efficient codec, MP3 is better supported
by hardware players, although this trend is changing.
</para>

<para>
Do <emphasis>not</emphasis> use <option>-nosound</option> when encoding
a file with audio, even if you will be encoding and muxing audio
separately later.
Though it may work in ideal cases, using <option>-nosound</option> is
likely to hide some problems in your encoding command line setting.
In other words, having a soundtrack during your encode assures you that,
provided you do not see messages such as
<quote>Too many audio packets in the buffer</quote>, you will be able
to get proper sync.
</para>

<para>
You need to have <application>MEncoder</application> process the sound.
You can for example copy the original soundtrack during the encode with
<option>-oac copy</option> or convert it to a "light" 4 kHz mono WAV
PCM with <option>-oac pcm -channels 1 -srate 4000</option>.
Otherwise, in some cases, it will generate a video file that will not sync
with the audio.
Such cases are when the number of video frames in the source file does
not match up to the total length of audio frames or whenever there
are discontinuities/splices where there are missing or extra audio frames.
The correct way to handle this kind of problem is to insert silence or
cut audio at these points.
However <application>MPlayer</application> cannot do that, so if you
demux the AC-3 audio and encode it with a separate app (or dump it to PCM with
<application>MPlayer</application>), the splices will be left incorrect
and the only way to correct them is to drop/duplicate video frames at the
splice.
As long as <application>MEncoder</application> sees the audio when it is
encoding the video, it can do this dropping/duping (which is usually OK
since it takes place at full black/scene change), but if
<application>MEncoder</application> cannot see the audio, it will just
process all frames as-is and they will not fit the final audio stream when
you for example merge your audio and video track into a Matroska file.
</para>

<para>
First of all, you will have to convert the DVD sound into a WAV file that the
audio codec can use as input.
For example:
<screen>
mplayer <replaceable>source_file.vob</replaceable> -ao pcm:file=<replaceable>destination_sound.wav</replaceable> \
    -vc dummy -aid 1 -vo null
</screen>
will dump the second audio track from the file
<replaceable>source_file.vob</replaceable> into the file
<replaceable>destination_sound.wav</replaceable>.
You may want to normalize the sound before encoding, as DVD audio tracks
are commonly recorded at low volumes.
You can use the tool <application>normalize</application> for instance,
which is available in most distributions.
If you are using Windows, a tool such as <application>BeSweet</application>
can do the same job.
You will compress in either Vorbis or MP3.
For example:
<screen>oggenc -q1 <replaceable>destination_sound.wav</replaceable></screen>
will encode <replaceable>destination_sound.wav</replaceable> with
the encoding quality 1, which is roughly equivalent to 80Kb/s, and
is the minimum quality at which you should encode if you care about
quality.
Please note that <application>MEncoder</application> currently cannot
mux Vorbis audio tracks
into the output file because it only supports AVI and MPEG
containers as an output, each of which may lead to audio/video
playback synchronization problems with some players when the AVI file
contain VBR audio streams such as Vorbis.
Do not worry, this document will show you how you can do that with third
party programs.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-muxing">
<title>Muxing</title>

<para>
Now that you have encoded your video, you will most likely want
to mux it with one or more audio tracks into a movie container, such
as AVI, MPEG, Matroska or NUT.
<application>MEncoder</application> is currently only able to natively output
audio and video into MPEG and AVI container formats.
for example:
<screen>
mencoder -oac copy -ovc copy  -o <replaceable>output_movie.avi</replaceable> \
    -audiofile <replaceable>input_audio.mp2</replaceable> <replaceable>input_video.avi</replaceable>
</screen>
This would merge the video file <replaceable>input_video.avi</replaceable>
and the audio file <replaceable>input_audio.mp2</replaceable>
into the AVI file <replaceable>output_movie.avi</replaceable>.
This command works with MPEG-1 layer I, II and III (more commonly known
as MP3) audio, WAV and a few other audio formats too.
</para>

<para>
<application>MEncoder</application> features experimental support for
<systemitem class="library">libavformat</systemitem>, which is a
library from the FFmpeg project that supports muxing and demuxing
a variety of containers.
For example:
<screen>
mencoder -oac copy -ovc copy -o <replaceable>output_movie.asf</replaceable> -audiofile <replaceable>input_audio.mp2</replaceable> \
    <replaceable>input_video.avi</replaceable> -of lavf -lavfopts format=asf
</screen>
This will do the same thing as the previous example, except that
the output container will be ASF.
Please note that this support is highly experimental (but getting
better every day), and will only work if you compiled
<application>MPlayer</application> with the support for
<systemitem class="library">libavformat</systemitem> enabled (which
means that a pre-packaged binary version will not work in most cases).
</para>


<sect3 id="menc-feat-dvd-mpeg4-muxing-filter-issues">
<title>Improving muxing and A/V sync reliability</title>

<para>
You may experience some serious A/V sync problems while trying to mux
your video and some audio tracks, where no matter how you adjust the
audio delay, you will never get proper sync.
That may happen when you use some video filters that will drop or
duplicate some frames, like the inverse telecine filters.
It is strongly encouraged to append the <option>harddup</option> video
filter at the end of the filter chain to avoid this kind of problem.
</para>

<para>
Without <option>harddup</option>, if <application>MEncoder</application>
wants to duplicate a frame, it relies on the muxer to put a mark on the
container so that the last frame will be displayed again to maintain
sync while writing no actual frame.
With <option>harddup</option>, <application>MEncoder</application>
will instead just push the last frame displayed again into the filter
chain.
This means that the encoder receives the <emphasis>exact</emphasis>
same frame twice, and compresses it.
This will result in a slightly bigger file, but will not cause problems
when demuxing or remuxing into other container formats.
</para>

<para>
You may also have no choice but to use <option>harddup</option> with
container formats that are not too tightly linked with
<application>MEncoder</application> such as the ones supported through
<systemitem class="library">libavformat</systemitem>, which may not
support frame duplication at the container level.
</para>
</sect3>


<sect3 id="menc-feat-dvd-mpeg4-muxing-avi-limitations">
<title>Limitations of the AVI container</title>

<para>
Although it is the most widely-supported container format after MPEG-1,
AVI also has some major drawbacks.
Perhaps the most obvious is the overhead.
For each chunk of the AVI file, 24 bytes are wasted on headers and index.
This translates into a little over 5 MB per hour, or 1-2.5%
overhead for a 700 MB movie. This may not seem like much, but it could
mean the difference between being able to use 700 kbit/sec video or
714 kbit/sec, and every bit of quality counts.
</para>

<para>
In addition this gross inefficiency, AVI also has the following major
limitations:
</para>

<orderedlist>
<listitem><para>
  Only fixed-fps content can be stored. This is particularly limiting
  if the original material you want to encode is mixed content, for
  example a mix of NTSC video and film material.
  Actually there are hacks that can be used to store mixed-framerate
  content in AVI, but they increase the (already huge) overhead
  fivefold or more and so are not practical.
</para></listitem>
<listitem><para>
  Audio in AVI files must be either constant-bitrate (CBR) or
  constant-framesize (i.e. all frames decode to the same number of
  samples).
  Unfortunately, the most efficient codec, Vorbis, does not meet
  either of these requirements.
  Therefore, if you plan to store your movie in AVI, you will have to
  use a less efficient codec such as MP3 or AC-3.
</para></listitem>
</orderedlist>

<para>
Having said all that, <application>MEncoder</application> does not
currently support variable-fps output or Vorbis encoding.
Therefore, you may not see these as limitations if
<application>MEncoder</application> is the
only tool you will be using to produce your encodes.
However, it is possible to use <application>MEncoder</application>
only for video encoding, and then use external tools to encode
audio and mux it into another container format.
</para>
</sect3>


<sect3 id="menc-feat-dvd-mpeg4-muxing-matroska">
<title>Muxing into the Matroska container</title>

<para>
Matroska is a free, open standard container format, aiming
to offer a lot of advanced features, which older containers
like AVI cannot handle.
For example, Matroska supports variable bitrate audio content
(VBR), variable framerates (VFR), chapters, file attachments,
error detection code (EDC) and modern A/V Codecs like "Advanced Audio
Coding" (AAC), "Vorbis" or "MPEG-4 AVC" (H.264), next to nothing
handled by AVI.
</para>

<para>
The tools required to create Matroska files are collectively called
<application>mkvtoolnix</application>, and are available for most
Unix platforms as well as <application>Windows</application>.
Because Matroska is an open standard you may find other
tools that suit you better, but since mkvtoolnix is the most
common, and is supported by the Matroska team itself, we will
only cover its usage.
</para>

<para>
Probably the easiest way to get started with Matroska is to use
<application>MMG</application>, the graphical frontend shipped with
<application>mkvtoolnix</application>, and follow the
<ulink url="http://www.bunkus.org/videotools/mkvtoolnix/doc/mkvmerge-gui.html">guide to mkvmerge GUI (mmg)</ulink>
</para>

<para>
You may also mux audio and video files using the command line:
<screen>
mkvmerge -o <replaceable>output.mkv</replaceable> <replaceable>input_video.avi</replaceable> <replaceable>input_audio1.mp3</replaceable> <replaceable>input_audio2.ac3</replaceable>
</screen>
This would merge the video file <replaceable>input_video.avi</replaceable>
and the two audio files <replaceable>input_audio1.mp3</replaceable>
and <replaceable>input_audio2.ac3</replaceable> into the Matroska
file <replaceable>output.mkv</replaceable>.
Matroska, as mentioned earlier, is able to do much more than that, like
multiple audio tracks (including fine-tuning of audio/video
synchronization), chapters, subtitles, splitting, etc...
Please refer to the documentation of those applications for
more details.
</para>
</sect3>
</sect2>
</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-telecine">
<title>How to deal with telecine and interlacing within NTSC DVDs</title>

<sect2 id="menc-feat-telecine-intro">
<title>Introduction</title>

<formalpara>
<title>What is telecine?</title>
<para>
If you do not understand much of what is written in this document, read the
<ulink url="http://en.wikipedia.org/wiki/Telecine">Wikipedia entry on telecine</ulink>.
It is an understandable and reasonably comprehensive
description of what telecine is.
</para></formalpara>

<formalpara>
<title>A note about the numbers.</title>
<para>
Many documents, including the article linked above, refer to the fields
per second value of NTSC video as 59.94 and the corresponding frames
per second values as 29.97 (for telecined and interlaced) and 23.976
(for progressive). For simplicity, some documents even round these
numbers to 60, 30, and 24.
</para></formalpara>

<para>
Strictly speaking, all those numbers are approximations. Black and
white NTSC video was exactly 60 fields per second, but 60000/1001
was later chosen to accommodate color data while remaining compatible
with contemporary black and white televisions. Digital NTSC video
(such as on a DVD) is also 60000/1001 fields per second. From this,
interlaced and telecined video are derived to be 30000/1001 frames
per second; progressive video is 24000/1001 frames per second.
</para>

<para>
Older versions of the <application>MEncoder</application> documentation
and many archived mailing list posts refer to 59.94, 29.97, and 23.976.
All <application>MEncoder</application> documentation has been updated
to use the fractional values, and you should use them too.
</para>

<para>
<option>-ofps 23.976</option> is incorrect.
<option>-ofps 24000/1001</option> should be used instead.
</para>

<formalpara>
<title>How telecine is used.</title>
<para>
All video intended to be displayed on an NTSC
television set must be 60000/1001 fields per second. Made-for-TV movies
and shows are often filmed directly at 60000/1001 fields per second, but
the majority of cinema is filmed at 24 or 24000/1001 frames per
second. When cinematic movie DVDs are mastered, the video is then
converted for television using a process called telecine.
</para></formalpara>

<para>
On a DVD, the video is never actually stored as 60000/1001 fields per
second. For video that was originally 60000/1001, each pair of fields is
combined to form a frame, resulting in 30000/1001 frames per
second. Hardware DVD players then read a flag embedded in the video
stream to determine whether the odd- or even-numbered lines should
form the first field.
</para>

<para>
Usually, 24000/1001 frames per second content stays as it is when
encoded for a DVD, and the DVD player must perform telecining
on-the-fly. Sometimes, however, the video is telecined
<emphasis>before</emphasis> being stored on the DVD; even though it
was originally 24000/1001 frames per second, it becomes 60000/1001 fields per
second. When it is stored on the DVD, pairs of fields are combined to form
30000/1001 frames per second.
</para>

<para>
When looking at individual frames formed from 60000/1001 fields per
second video, telecined or otherwise, interlacing is clearly visible
wherever there is any motion, because one field (say, the
even-numbered lines) represents a moment in time 1/(60000/1001)
seconds later than the other. Playing interlaced video on a computer
looks ugly both because the monitor is higher resolution and because
the video is shown frame-after-frame instead of field-after-field.
</para>

<itemizedlist>
<title>Notes:</title>
<listitem><para>
  This section only applies to NTSC DVDs, and not PAL.
</para></listitem>
<listitem><para>
  The example <application>MEncoder</application> lines throughout the
  document are <emphasis role="bold">not</emphasis> intended for
  actual use. They are simply the bare minimum required to encode the
  pertaining video category. How to make good DVD rips or fine-tune
  <systemitem class="library">libavcodec</systemitem> for maximal
  quality is not within the scope of this section; refer to other
  sections within the <link linkend="encoding-guide">MEncoder encoding
  guide</link>.
</para></listitem>
<listitem><para>
  There are a couple footnotes specific to this guide, linked like this:
  <link linkend="menc-feat-telecine-footnotes">[1]</link>
</para></listitem>
</itemizedlist>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-telecine-ident">
<title>How to tell what type of video you have</title>

<sect3 id="menc-feat-telecine-ident-progressive">
<title>Progressive</title>

<para>
Progressive video was originally filmed at 24000/1001 fps, and stored
on the DVD without alteration.
</para>

<para>
When you play a progressive DVD in <application>MPlayer</application>,
<application>MPlayer</application> will print the following line as
soon as the movie begins to play:
<screen>
demux_mpg: 24000/1001 fps progressive NTSC content detected, switching framerate.
</screen>
From this point forward, demux_mpg should never say it finds
"30000/1001 fps NTSC content."
</para>

<para>
When you watch progressive video, you should never see any
interlacing. Beware, however, because sometimes there is a tiny bit
of telecine mixed in where you would not expect. I have encountered TV
show DVDs that have one second of telecine at every scene change, or
at seemingly random places. I once watched a DVD that had a
progressive first half, and the second half was telecined. If you
want to be <emphasis>really</emphasis> thorough, you can scan the
entire movie:
<screen>mplayer dvd://1 -nosound -vo null -benchmark</screen>
Using <option>-benchmark</option> makes
<application>MPlayer</application> play the movie as quickly as it
possibly can; still, depending on your hardware, it can take a
while. Every time demux_mpg reports a framerate change, the line
immediately above will show you the time at which the change
occurred.
</para>

<para>
Sometimes progressive video on DVDs is referred to as
"soft-telecine" because it is intended to
be telecined by the DVD player.
</para>
</sect3>


<sect3 id="menc-feat-telecine-ident-telecined">
<title>Telecined</title>

<para>
Telecined video was originally filmed at 24000/1001, but was telecined
<emphasis>before</emphasis> it was written to the DVD.
</para>

<para>
<application>MPlayer</application> does not (ever) report any
framerate changes when it plays telecined video.
</para>

<para>
Watching a telecined video, you will see interlacing artifacts that
seem to "blink": they repeatedly appear and disappear.
You can look closely at this by
<orderedlist>
<listitem><screen>mplayer dvd://1</screen></listitem>
<listitem><para>
  Seek to a part with motion.
</para></listitem>
<listitem><para>
  Use the <keycap>.</keycap> key to step forward one frame at a time.
</para></listitem>
<listitem><para>
  Look at the pattern of interlaced-looking and progressive-looking
  frames. If the pattern you see is PPPII,PPPII,PPPII,... then the
  video is telecined. If you see some other pattern, then the video
  may have been telecined using some non-standard method;
  <application>MEncoder</application> cannot losslessly convert
  non-standard telecine to progressive. If you do not see any
  pattern at all, then it is most likely interlaced.
</para></listitem>
</orderedlist>
</para>

<para>
Sometimes telecined video on DVDs is referred to as
"hard-telecine". Since hard-telecine is already 60000/1001 fields
per second, the DVD player plays the video without any manipulation.
</para>

<para>
Another way to tell if your source is telecined or not is to play
the source with the <option>-vf pullup</option> and <option>-v</option>
command line options to see how <option>pullup</option> matches frames.
If the source is telecined, you should see on the console a 3:2 pattern
with <systemitem>0+.1.+2</systemitem> and <systemitem>0++1</systemitem>
alternating.
This technique has the advantage that you do not need to watch the
source to identify it, which could be useful if you wish to automate
the encoding procedure, or to carry out said procedure remotely via
a slow connection.
</para>
</sect3>


<sect3 id="menc-feat-telecine-ident-interlaced">
<title>Interlaced</title>

<para>
Interlaced video was originally filmed at 60000/1001 fields per second,
and stored on the DVD as 30000/1001 frames per second. The interlacing effect
(often called "combing") is a result of combining pairs of
fields into frames. Each field is supposed to be 1/(60000/1001) seconds apart,
and when they are displayed simultaneously the difference is apparent.
</para>

<para>
As with telecined video, <application>MPlayer</application> should
not ever report any framerate changes when playing interlaced content.
</para>

<para>
When you view an interlaced video closely by frame-stepping with the
<keycap>.</keycap> key, you will see that every single frame is interlaced.
</para>
</sect3>


<sect3 id="menc-feat-telecine-ident-mixedpt">
<title>Mixed progressive and telecine</title>

<para>
All of a "mixed progressive and telecine" video was originally
24000/1001 frames per second, but some parts of it ended up being telecined.
</para>

<para>
When <application>MPlayer</application> plays this category, it will
(often repeatedly) switch back and forth between "30000/1001 fps NTSC"
and "24000/1001 fps progressive NTSC". Watch the bottom of
<application>MPlayer</application>'s output to see these messages.
</para>

<para>
You should check the "30000/1001 fps NTSC" sections to make sure
they are actually telecine, and not just interlaced.
</para>
</sect3>


<sect3 id="menc-feat-telecine-ident-mixedpi">
<title>Mixed progressive and interlaced</title>

<para>
In "mixed progressive and interlaced" content, progressive
and interlaced video have been spliced together.
</para>

<para>
This category looks just like "mixed progressive and telecine",
until you examine the 30000/1001 fps sections and see that they do not have the
telecine pattern.
</para>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-telecine-encode">
<title>How to encode each category</title>
<para>
As I mentioned in the beginning, example <application>MEncoder</application>
lines below are <emphasis role="bold">not</emphasis> meant to actually be used;
they only demonstrate the minimum parameters to properly encode each category.
</para>


<sect3 id="menc-feat-telecine-encode-progressive">
<title>Progressive</title>
<para>
Progressive video requires no special filtering to encode. The only
parameter you need to be sure to use is <option>-ofps 24000/1001</option>.
Otherwise, <application>MEncoder</application>
will try to encode at 30000/1001 fps and will duplicate frames.
</para>

<para>
<screen>mencoder dvd://1 -oac copy -ovc lavc -ofps 24000/1001</screen>
</para>

<para>
It is often the case, however, that a video that looks progressive
actually has very short parts of telecine mixed in. Unless you are
sure, it is safest to treat the video as
<link linkend="menc-feat-telecine-encode-mixedpt">mixed progressive and telecine</link>.
The performance loss is small
<link linkend="menc-feat-telecine-footnotes">[3]</link>.
</para>
</sect3>


<sect3 id="menc-feat-telecine-encode-telecined">
<title>Telecined</title>

<para>
Telecine can be reversed to retrieve the original 24000/1001 content,
using a process called inverse-telecine.
<application>MPlayer</application> contains several filters to
accomplish this; the best filter, <option>pullup</option>, is described
in the <link linkend="menc-feat-telecine-encode-mixedpt">mixed
progressive and telecine</link> section.
</para>
</sect3>


<sect3 id="menc-feat-telecine-encode-interlaced">
<title>Interlaced</title>

<para>
For most practical cases it is not possible to retrieve a complete
progressive video from interlaced content. The only way to do so
without losing half of the vertical resolution is to double the
framerate and try to "guess" what ought to make up the
corresponding lines for each field (this has drawbacks - see method 3).
</para>

<orderedlist>
<listitem><para>
  Encode the video in interlaced form. Normally, interlacing wreaks
  havoc with the encoder's ability to compress well, but
  <systemitem class="library">libavcodec</systemitem> has two
  parameters specifically for dealing with storing interlaced video a
  bit better: <option>ildct</option> and <option>ilme</option>. Also,
  using <option>mbd=2</option> is strongly recommended
  <link linkend="menc-feat-telecine-footnotes">[2] </link> because it
  will encode macroblocks as non-interlaced in places where there is
  no motion. Note that <option>-ofps</option> is NOT needed here.
  <screen>mencoder dvd://1 -oac copy -ovc lavc -lavcopts ildct:ilme:mbd=2</screen>
</para></listitem>
<listitem><para>
  Use a deinterlacing filter before encoding. There are several of
  these filters available to choose from, each with its own advantages
  and disadvantages. Consult <option>mplayer -pphelp</option> and
  <option>mplayer -vf help</option> to see what is available
  (grep for "deint"), read Michael Niedermayer's
  <ulink url="http://guru.multimedia.cx/deinterlacing-filters/">Deinterlacing filters comparison</ulink>,
  and search the
  <ulink url="http://www.mplayerhq.hu/design7/mailing_lists.html">
  MPlayer mailing lists</ulink> to find many discussions about the
  various filters.
  Again, the framerate is not changing, so no
  <option>-ofps</option>. Also, deinterlacing should be done after
  cropping <link linkend="menc-feat-telecine-footnotes">[1]</link> and
  before scaling.
  <screen>mencoder dvd://1 -oac copy -vf yadif -ovc lavc</screen>
</para></listitem>
<listitem><para>
  Unfortunately, this option is buggy with
  <application>MEncoder</application>; it ought to work well with
  <application>MEncoder G2</application>, but that is not here yet. You
  might experience crashes. Anyway, the purpose of <option> -vf
  tfields</option> is to create a full frame out of each field, which
  makes the framerate 60000/1001. The advantage of this approach is that no
  data is ever lost; however, since each frame comes from only one
  field, the missing lines have to be interpolated somehow. There are
  no very good methods of generating the missing data, and so the
  result will look a bit similar to when using some deinterlacing
  filters. Generating the missing lines creates other issues, as well,
  simply because the amount of data doubles. So, higher encoding
  bitrates are required to maintain quality, and more CPU power is
  used for both encoding and decoding. tfields has several different
  options for how to create the missing lines of each frame. If you
  use this method, then Reference the manual, and chose whichever
  option looks best for your material. Note that when using
  <option>tfields</option> you
  <emphasis role="bold">have to</emphasis> specify both
  <option>-fps</option> and <option>-ofps</option> to be twice the
  framerate of your original source.
  <screen>
mencoder dvd://1 -oac copy -vf tfields=2 -ovc lavc \
    -fps 60000/1001 -ofps 60000/1001<!--
  --></screen>
</para></listitem>
<listitem><para>
  If you plan on downscaling dramatically, you can extract and encode
  only one of the two fields. Of course, you will lose half the vertical
  resolution, but if you plan on downscaling to at most 1/2 of the
  original, the loss will not matter much. The result will be a
  progressive 30000/1001 frames per second file. The procedure is to use
  <option>-vf field</option>, then crop
  <link linkend="menc-feat-telecine-footnotes">[1]</link> and scale
  appropriately. Remember that you will have to adjust the scale to
  compensate for the vertical resolution being halved.
  <screen>mencoder dvd://1 -oac copy -vf field=0 -ovc lavc</screen>
</para></listitem>
</orderedlist>
</sect3>


<sect3 id="menc-feat-telecine-encode-mixedpt">
<title>Mixed progressive and telecine</title>

<para>
In order to turn mixed progressive and telecine video into entirely
progressive video, the telecined parts have to be
inverse-telecined. There are three ways to accomplish this,
described below. Note that you should
<emphasis role="bold">always</emphasis> inverse-telecine before any
rescaling; unless you really know what you are doing,
inverse-telecine before cropping, too
<link linkend="menc-feat-telecine-footnotes">[1]</link>.
<option>-ofps 24000/1001</option> is needed here because the output video
will be 24000/1001 frames per second.
</para>

<itemizedlist>
<listitem><para>
  <option>-vf pullup</option> is designed to inverse-telecine
  telecined material while leaving progressive data alone. In order to
  work properly, <option>pullup</option> <emphasis role="bold">must</emphasis>
  be followed by the <option>softskip</option> filter or
  else <application>MEncoder</application> will crash.
  <option>pullup</option> is, however, the cleanest and most
  accurate method available for encoding both telecine and
  "mixed progressive and telecine".
  <screen>
mencoder dvd://1 -oac copy -vf pullup,softskip
    -ovc lavc -ofps 24000/1001<!--
  --></screen>
</para></listitem>
<listitem><para>
  <option>-vf filmdint</option> is similar to
  <option>-vf pullup</option>: both filters attempt to match a pair of
  fields to form a complete frame. <option>filmdint</option> will
  deinterlace individual fields that it cannot match, however, whereas
  <option>pullup</option> will simply drop them. Also, the two filters
  have separate detection code, and <option>filmdint</option> may tend to match fields a
  bit less often. Which filter works better may depend on the input
  video and personal taste; feel free to experiment with fine-tuning
  the filters' options if you encounter problems with either one (see
  the man page for details). For most well-mastered input video,
  however, both filters work quite well, so either one is a safe choice
  to start with.
  <screen>
mencoder dvd://1 -oac copy -vf filmdint -ovc lavc -ofps 24000/1001<!--
  --></screen>
</para></listitem>
<listitem><para>
  An older method
  is to, rather than inverse-telecine the telecined parts, telecine
  the non-telecined parts and then inverse-telecine the whole
  video. Sound confusing? softpulldown is a filter that goes through
  a video and makes the entire file telecined. If we follow
  softpulldown with either <option>detc</option> or
  <option>ivtc</option>, the final result will be entirely
  progressive. <option>-ofps 24000/1001</option> is needed.
  <screen>
mencoder dvd://1 -oac copy -vf softpulldown,ivtc=1 -ovc lavc -ofps 24000/1001
  </screen>
</para></listitem>

</itemizedlist>
</sect3>


<sect3 id="menc-feat-telecine-encode-mixedpi">
<title>Mixed progressive and interlaced</title>

<para>
There are two options for dealing with this category, each of
which is a compromise. You should decide based on the
duration/location of each type.
</para>

<itemizedlist>
<listitem>
  <para>
  Treat it as progressive. The interlaced parts will look interlaced,
  and some of the interlaced fields will have to be dropped, resulting
  in a bit of uneven jumpiness. You can use a postprocessing filter if
  you want to, but it may slightly degrade the progressive parts.
  </para>

  <para>
  This option should definitely not be used if you want to eventually
  display the video on an interlaced device (with a TV card, for
  example). If you have interlaced frames in a 24000/1001 frames per
  second video, they will be telecined along with the progressive
  frames. Half of the interlaced "frames" will be displayed for three
  fields' duration (3/(60000/1001) seconds), resulting in a flicking
  "jump back in time" effect that looks quite bad. If you
  even attempt this, you <emphasis role="bold">must</emphasis> use a
  deinterlacing filter like <option>lb</option> or
  <option>l5</option>.
  </para>

  <para>
  It may also be a bad idea for progressive display, too. It will drop
  pairs of consecutive interlaced fields, resulting in a discontinuity
  that can be more visible than with the second method, which shows
  some progressive frames twice. 30000/1001 frames per second interlaced
  video is already a bit choppy because it really should be shown at
  60000/1001 fields per second, so the duplicate frames do not stand out as
  much.
  </para>

  <para>
  Either way, it is best to consider your content and how you intend to
  display it. If your video is 90% progressive and you never intend to
  show it on a TV, you should favor a progressive approach. If it is
  only half progressive, you probably want to encode it as if it is all
  interlaced.
  </para>
</listitem>

<listitem><para>
  Treat it as interlaced. Some frames of the progressive parts will
  need to be duplicated, resulting in uneven jumpiness. Again,
  deinterlacing filters may slightly degrade the progressive parts.
</para></listitem>
</itemizedlist>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-telecine-footnotes">
<title>Footnotes</title>

<orderedlist>
<listitem>
  <formalpara>
  <title>About cropping:</title>
  <para>
  Video data on DVDs are stored in a format called YUV 4:2:0. In YUV
  video, luma ("brightness") and chroma ("color")
  are stored separately. Because the human eye is somewhat less
  sensitive to color than it is to brightness, in a YUV 4:2:0 picture
  there is only one chroma pixel for every four luma pixels. In a
  progressive picture, each square of four luma pixels (two on each
  side) has one common chroma pixel. You must crop progressive YUV
  4:2:0 to even resolutions, and use even offsets. For example,
  <option>crop=716:380:2:26</option> is OK but
  <option>crop=716:380:3:26 </option> is not.
  </para>
  </formalpara>

  <para>
  When you are dealing with interlaced YUV 4:2:0, the situation is a
  bit more complicated. Instead of every four luma pixels in the
  <emphasis>frame</emphasis> sharing a chroma pixel, every four luma
  pixels in each <emphasis> field</emphasis> share a chroma
  pixel. When fields are interlaced to form a frame, each scanline is
  one pixel high. Now, instead of all four luma pixels being in a
  square, there are two pixels side-by-side, and the other two pixels
  are side-by-side two scanlines down. The two luma pixels in the
  intermediate scanline are from the other field, and so share a
  different chroma pixel with two luma pixels two scanlines away. All
  this confusion makes it necessary to have vertical crop dimensions
  and offsets be multiples of four. Horizontal can stay even.
  </para>

  <para>
  For telecined video, I recommend that cropping take place after
  inverse telecining. Once the video is progressive you only need to
  crop by even numbers. If you really want to gain the slight speedup
  that cropping first may offer, you must crop vertically by multiples
  of four or else the inverse-telecine filter will not have proper data.
  </para>

  <para>
  For interlaced (not telecined) video, you must always crop
  vertically by multiples of four unless you use <option>-vf
  field</option> before cropping.
  </para>
</listitem>

<listitem><formalpara>
  <title>About encoding parameters and quality:</title>
  <para>
  Just because I recommend <option>mbd=2</option> here does not mean it
  should not be used elsewhere. Along with <option>trell</option>,
  <option>mbd=2</option> is one of the two
   <systemitem class="library">libavcodec</systemitem> options that
  increases quality the most, and you should always use at least those
  two unless the drop in encoding speed is prohibitive (e.g. realtime
  encoding). There are many other options to
  <systemitem class="library">libavcodec</systemitem> that increase
  encoding quality (and decrease encoding speed) but that is beyond
  the scope of this document.
  </para>
</formalpara></listitem>

<listitem><formalpara>
  <title>About the performance of pullup:</title>
  <para>
  It is safe to use <option>pullup</option> (along with <option>softskip
  </option>) on progressive video, and is usually a good idea unless
  the source has been definitively verified to be entirely progressive.
  The performance loss is small for most cases. On a bare-minimum encode,
  <option>pullup</option> causes <application>MEncoder</application> to
  be 50% slower. Adding sound processing and advanced <option>lavcopts
  </option> overshadows that difference, bringing the performance
  decrease of using <option>pullup</option> down to 2%.
  </para>
</formalpara></listitem>
</orderedlist>
</sect2>
</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-enc-libavcodec">
<title>Encoding with the <systemitem class="library">libavcodec</systemitem>
  codec family</title>

<para>
<systemitem class="library">libavcodec</systemitem>
provides simple encoding to a lot of interesting video and audio formats.
You can encode to the following codecs (more or less up to date):
</para>

<!-- ********** -->

<sect2 id="menc-feat-enc-libavcodec-video-codecs">
<title><systemitem class="library">libavcodec</systemitem>'s
  video codecs</title>

<para>
<informaltable frame="all">
<tgroup cols="2">
<thead>
  <row><entry>Video codec name</entry><entry>Description</entry></row>
</thead>
<tbody>
<row>
  <entry>mjpeg</entry>
  <entry>Motion JPEG</entry>
</row>
<row>
  <entry>ljpeg</entry>
  <entry>lossless JPEG</entry>
</row>
<row>
  <entry>jpegls</entry>
  <entry>JPEG LS</entry>
</row>
<row>
  <entry>targa</entry>
  <entry>Targa image</entry>
</row>
<row>
  <entry>gif</entry>
  <entry>GIF image</entry>
</row>
<row>
  <entry>bmp</entry>
  <entry>BMP image</entry>
</row>
<row>
  <entry>png</entry>
  <entry>PNG image</entry>
</row>
<row>
  <entry>h261</entry>
  <entry>H.261</entry>
</row>
<row>
  <entry>h263</entry>
  <entry>H.263 </entry>
</row>
<row>
  <entry>h263p</entry>
  <entry>H.263+</entry>
</row>
<row>
  <entry>mpeg4</entry>
  <entry>ISO standard MPEG-4 (DivX, Xvid compatible)</entry>
</row>
<row>
  <entry>msmpeg4</entry>
  <entry>pre-standard MPEG-4 variant by MS, v3 (AKA DivX3)</entry>
</row>
<row>
  <entry>msmpeg4v2</entry>
  <entry>pre-standard MPEG-4 by MS, v2 (used in old ASF files)</entry>
</row>
<row>
  <entry>wmv1</entry>
  <entry>Windows Media Video, version 1 (AKA WMV7)</entry>
</row>
<row>
  <entry>wmv2</entry>
  <entry>Windows Media Video, version 2 (AKA WMV8)</entry>
</row>
<row>
  <entry>rv10</entry>
  <entry>RealVideo 1.0</entry>
</row>
<row>
  <entry>rv20</entry>
  <entry>RealVideo 2.0</entry>
</row>
<row>
  <entry>mpeg1video</entry>
  <entry>MPEG-1 video</entry>
</row>
<row>
  <entry>mpeg2video</entry>
  <entry>MPEG-2 video</entry>
</row>
<row>
  <entry>huffyuv</entry>
  <entry>lossless compression</entry>
</row>
<row>
  <entry>ffvhuff</entry>
  <entry>FFmpeg modified huffyuv lossless</entry>
</row>
<row>
  <entry>asv1</entry>
  <entry>ASUS Video v1</entry>
</row>
<row>
  <entry>asv2</entry>
  <entry>ASUS Video v2</entry>
</row>
<row>
  <entry>ffv1</entry>
  <entry>FFmpeg's lossless video codec</entry>
</row>
<row>
  <entry>svq1</entry>
  <entry>Sorenson video 1</entry>
</row>
<row>
  <entry>flv</entry>
  <entry>Sorenson H.263 used in Flash Video</entry>
</row>
<row>
  <entry>flashsv</entry>
  <entry>Flash Screen Video</entry>
</row>
<row>
  <entry>dvvideo</entry>
  <entry>Sony Digital Video</entry>
</row>
<row>
  <entry>snow</entry>
  <entry>FFmpeg's experimental wavelet-based codec</entry>
</row>
<row>
  <entry>zmbv</entry>
  <entry>Zip Motion Blocks Video</entry>
</row>
<row>
  <entry>dnxhd</entry>
  <entry>AVID DNxHD</entry>
</row>
</tbody>
</tgroup>
</informaltable>

The first column contains the codec names that should be passed after the
<literal>vcodec</literal> config,
like: <option>-lavcopts vcodec=msmpeg4</option>
</para>

<informalexample><para>
An example with MJPEG compression:
<screen>
mencoder dvd://2 -o <replaceable>title2.avi</replaceable> -ovc lavc -lavcopts vcodec=mjpeg -oac copy
</screen>
</para></informalexample>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-enc-libavcodec-audio-codecs">
<title><systemitem class="library">libavcodec</systemitem>'s
  audio codecs</title>

<para>
<informaltable frame="all">
<tgroup cols="2">
<thead>
<row><entry>Audio codec name</entry><entry>Description</entry></row>
</thead>
<tbody>
<row>
  <entry>ac3</entry>
  <entry>Dolby Digital (AC-3)</entry>
</row>
<row>
  <entry>adpcm_*</entry>
  <entry>Adaptive PCM formats - see supplementary table</entry>
</row>
<row>
  <entry>flac</entry>
  <entry>Free Lossless Audio Codec (FLAC)</entry>
</row>
<row>
  <entry>g726</entry>
  <entry>G.726 ADPCM</entry>
</row>
<row>
  <entry>libfaac</entry>
  <entry>Advanced Audio Coding (AAC) - using FAAC</entry>
</row>
<row>
  <entry>libgsm</entry>
  <entry>ETSI GSM 06.10 full rate</entry>
</row>
<row>
  <entry>libgsm_ms</entry>
  <entry>Microsoft GSM</entry>
</row>
<row>
  <entry>libmp3lame</entry>
  <entry>MPEG-1 audio layer 3 (MP3) - using LAME</entry>
</row>
<row>
  <entry>mp2</entry>
  <entry>MPEG-1 audio layer 2 (MP2)</entry>
</row>
<row>
  <entry>pcm_*</entry>
  <entry>PCM formats - see supplementary table</entry>
</row>
<row>
  <entry>roq_dpcm</entry>
  <entry>Id Software RoQ DPCM</entry>
</row>
<row>
  <entry>sonic</entry>
  <entry>experimental FFmpeg lossy codec</entry>
</row>
<row>
  <entry>sonicls</entry>
  <entry>experimental FFmpeg lossless codec</entry>
</row>
<row>
  <entry>vorbis</entry>
  <entry>Vorbis</entry>
</row>
<row>
  <entry>wmav1</entry>
  <entry>Windows Media Audio v1</entry>
</row>
<row>
  <entry>wmav2</entry>
  <entry>Windows Media Audio v2</entry>
</row>
</tbody>
</tgroup>
</informaltable>

The first column contains the codec names that should be passed after the
<literal>acodec</literal> option, like: <option>-lavcopts acodec=ac3</option>
</para>

<informalexample><para>
An example with AC-3 compression:
<screen>
mencoder dvd://2 -o <replaceable>title2.avi</replaceable> -oac lavc -lavcopts acodec=ac3 -ovc copy
</screen>
</para></informalexample>

<para>
Contrary to <systemitem class="library">libavcodec</systemitem>'s video
codecs, its audio codecs do not make a wise usage of the bits they are
given as they lack some minimal psychoacoustic model (if at all)
which most other codec implementations feature.
However, note that all these audio codecs are very fast and work
out-of-the-box everywhere <application>MEncoder</application> has been
compiled with <systemitem class="library">libavcodec</systemitem> (which
is the case most of time), and do not depend on external libraries.
</para>

<sect3 id="menc-feat-enc-libavcodec-audio-codecs-pcmadpcm">
<title>PCM/ADPCM format supplementary table</title>

<para>
<informaltable frame="all">
<tgroup cols="2">
<thead>
<row><entry>PCM/ADPCM codec name</entry><entry>Description</entry></row>
</thead>
<tbody>
<row>
  <entry>pcm_s32le</entry>
  <entry>signed 32-bit little-endian</entry>
</row>
<row>
  <entry>pcm_s32be</entry>
  <entry>signed 32-bit big-endian</entry>
</row>
<row>
  <entry>pcm_u32le</entry>
  <entry>unsigned 32-bit little-endian</entry>
</row>
<row>
  <entry>pcm_u32be</entry>
  <entry>unsigned 32-bit big-endian</entry>
</row>
<row>
  <entry>pcm_s24le</entry>
  <entry>signed 24-bit little-endian</entry>
</row>
<row>
  <entry>pcm_s24be</entry>
  <entry>signed 24-bit big-endian</entry>
</row>
<row>
  <entry>pcm_u24le</entry>
  <entry>unsigned 24-bit little-endian</entry>
</row>
<row>
  <entry>pcm_u24be</entry>
  <entry>unsigned 24-bit big-endian</entry>
</row>
<row>
  <entry>pcm_s16le</entry>
  <entry>signed 16-bit little-endian</entry>
</row>
<row>
  <entry>pcm_s16be</entry>
  <entry>signed 16-bit big-endian</entry>
</row>
<row>
  <entry>pcm_u16le</entry>
  <entry>unsigned 16-bit little-endian</entry>
</row>
<row>
  <entry>pcm_u16be</entry>
  <entry>unsigned 16-bit big-endian</entry>
</row>
<row>
  <entry>pcm_s8</entry>
  <entry>signed 8-bit</entry>
</row>
<row>
  <entry>pcm_u8</entry>
  <entry>unsigned 8-bit</entry>
</row>
<row>
  <entry>pcm_alaw</entry>
  <entry>G.711 A-LAW </entry>
</row>
<row>
  <entry>pcm_mulaw</entry>
  <entry>G.711 &mu;-LAW</entry>
</row>
<row>
  <entry>pcm_s24daud</entry>
  <entry>signed 24-bit D-Cinema Audio format</entry>
</row>
<row>
  <entry>pcm_zork</entry>
  <entry>Activision Zork Nemesis</entry>
</row>
<row>
  <entry>adpcm_ima_qt</entry>
  <entry>Apple QuickTime</entry>
</row>
<row>
  <entry>adpcm_ima_wav</entry>
  <entry>Microsoft/IBM WAVE</entry>
</row>
<row>
  <entry>adpcm_ima_dk3</entry>
  <entry>Duck DK3</entry>
</row>
<row>
  <entry>adpcm_ima_dk4</entry>
  <entry>Duck DK4</entry>
</row>
<row>
  <entry>adpcm_ima_ws</entry>
  <entry>Westwood Studios</entry>
</row>
<row>
  <entry>adpcm_ima_smjpeg</entry>
  <entry>SDL Motion JPEG</entry>
</row>
<row>
  <entry>adpcm_ms</entry>
  <entry>Microsoft</entry>
</row>
<row>
  <entry>adpcm_4xm</entry>
  <entry>4X Technologies</entry>
</row>
<row>
  <entry>adpcm_xa</entry>
  <entry>Phillips Yellow Book CD-ROM eXtended Architecture</entry>
</row>
<row>
  <entry>adpcm_ea</entry>
  <entry>Electronic Arts</entry>
</row>
<row>
  <entry>adpcm_ct</entry>
  <entry>Creative 16->4-bit</entry>
</row>
<row>
  <entry>adpcm_swf</entry>
  <entry>Adobe Shockwave Flash</entry>
</row>
<row>
  <entry>adpcm_yamaha</entry>
  <entry>Yamaha</entry>
</row>
<row>
  <entry>adpcm_sbpro_4</entry>
  <entry>Creative VOC SoundBlaster Pro 8->4-bit</entry>
</row>
<row>
  <entry>adpcm_sbpro_3</entry>
  <entry>Creative VOC SoundBlaster Pro 8->2.6-bit</entry>
</row>
<row>
  <entry>adpcm_sbpro_2</entry>
  <entry>Creative VOC SoundBlaster Pro 8->2-bit</entry>
</row>
<row>
  <entry>adpcm_thp</entry>
  <entry>Nintendo GameCube FMV THP</entry>
</row>
<row>
  <entry>adpcm_adx</entry>
  <entry>Sega/CRI ADX</entry>
</row>
</tbody>
</tgroup>
</informaltable>
</para>
</sect3>

</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-lavc-encoding-options">
<title>Encoding options of libavcodec</title>

<para>
Ideally, you would probably want to be able to just tell the encoder to switch
into "high quality" mode and move on.
That would probably be nice, but unfortunately hard to implement as different
encoding options yield different quality results depending on the source
material. That is because compression depends on the visual properties of the
video in question.
For example, Anime and live action have very different properties and
thus require different options to obtain optimum encoding.
The good news is that some options should never be left out, like
<option>mbd=2</option>, <option>trell</option>, and <option>v4mv</option>.
See below for a detailed description of common encoding options.
</para>

<itemizedlist>
<title>Options to adjust:</title>
<listitem><para>
  <emphasis role="bold">vmax_b_frames</emphasis>: 1 or 2 is good, depending on
  the movie.
  Note that if you need to have your encode be decodable by DivX5, you
  need to activate closed GOP support, using
  <systemitem class="library">libavcodec</systemitem>'s <option>cgop</option>
  option, but you need to deactivate scene detection, which
  is not a good idea as it will hurt encode efficiency a bit.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vb_strategy=1</emphasis>: helps in high-motion scenes.
  On some videos, vmax_b_frames may hurt quality, but vmax_b_frames=2 along
  with vb_strategy=1 helps.
</para></listitem>
<listitem><para>
  <emphasis role="bold">dia</emphasis>: motion search range. Bigger is better
  and slower.
  Negative values are a completely different scale.
  Good values are -1 for a fast encode, or 2-4 for slower.
</para></listitem>
<listitem><para>
  <emphasis role="bold">predia</emphasis>: motion search pre-pass.
  Not as important as dia. Good values are 1 (default) to 4. Requires preme=2
  to really be useful.
</para></listitem>
<listitem><para>
  <emphasis role="bold">cmp, subcmp, precmp</emphasis>: Comparison function for
  motion estimation.
  Experiment with values of 0 (default), 2 (hadamard), 3 (dct), and 6 (rate
  distortion).
  0 is fastest, and sufficient for precmp.
  For cmp and subcmp, 2 is good for Anime, and 3 is good for live action.
  6 may or may not be slightly better, but is slow.
</para></listitem>
<listitem><para>
  <emphasis role="bold">last_pred</emphasis>: Number of motion predictors to
  take from the previous frame.
  1-3 or so help at little speed cost.
  Higher values are slow for no extra gain.
</para></listitem>
<listitem><para>
  <emphasis role="bold">cbp, mv0</emphasis>: Controls the selection of
  macroblocks. Small speed cost for small quality gain.
</para></listitem>
<listitem><para>
  <emphasis role="bold">qprd</emphasis>: adaptive quantization based on the
  macroblock's complexity.
  May help or hurt depending on the video and other options.
  This can cause artifacts unless you set vqmax to some reasonably small value
  (6 is good, maybe as low as 4); vqmin=1 should also help.
</para></listitem>
<listitem><para>
  <emphasis role="bold">qns</emphasis>: very slow, especially when combined
  with qprd.
  This option will make the encoder minimize noise due to compression
  artifacts instead of making the encoded video strictly match the source.
  Do not use this unless you have already tweaked everything else as far as it
  will go and the results still are not good enough.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vqcomp</emphasis>: Tweak ratecontrol.
  What values are good depends on the movie.
  You can safely leave this alone if you want.
  Reducing vqcomp puts more bits on low-complexity scenes, increasing it puts
  them on high-complexity scenes (default: 0.5, range: 0-1. recommended range:
  0.5-0.7).
</para></listitem>
<listitem><para>
  <emphasis role="bold">vlelim, vcelim</emphasis>: Sets the single coefficient
  elimination threshold for luminance and chroma planes.
  These are encoded separately in all MPEG-like algorithms.
  The idea behind these options is to use some good heuristics to determine
  when the change in a block is less than the threshold you specify, and in
  such a case, to just  encode the block as "no change".
  This saves bits and perhaps speeds up encoding. vlelim=-4 and vcelim=9
  seem to be good for live movies, but seem not to help with Anime;
  when encoding animation, you should probably leave them unchanged.
</para></listitem>
<listitem><para>
  <emphasis role="bold">qpel</emphasis>: Quarter pixel motion estimation.
  MPEG-4 uses half pixel precision for its motion search by default,
  therefore this option comes with an overhead as more information will be
  stored in the encoded file.
  The compression gain/loss depends on the movie, but it is usually not very
  effective on Anime.
  qpel always incurs a significant cost in CPU decode time (+25% in
  practice).
</para></listitem>
<listitem><para>
  <emphasis role="bold">psnr</emphasis>: does not affect the actual encoding,
  but writes a log file giving the type/size/quality of each frame, and
  prints a summary of PSNR (Peak Signal to Noise Ratio) at the end.
</para></listitem>
</itemizedlist>

<itemizedlist>
<title>Options not recommended to play with:</title>
<listitem><para>
  <emphasis role="bold">vme</emphasis>: The default is best.
</para></listitem>
<listitem><para>
  <emphasis role="bold">lumi_mask, dark_mask</emphasis>: Psychovisual adaptive
  quantization.
  You do not want to play with those options if you care about quality.
  Reasonable values may be effective in your case, but be warned this is very
  subjective.
</para></listitem>
<listitem><para>
  <emphasis role="bold">scplx_mask</emphasis>: Tries to prevent blocky
  artifacts, but postprocessing is better.
</para></listitem>
</itemizedlist>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-mpeg4-lavc-example-settings">
<title>Encoding setting examples</title>

<para>
The following settings are examples of different encoding
option combinations that affect the speed vs quality tradeoff
at the same target bitrate.
</para>

<para>
All the encoding settings were tested on a 720x448 @30000/1001 fps
video sample, the target bitrate was 900kbps, and the machine was an
AMD-64 3400+ at 2400 MHz in 64 bits mode.
Each encoding setting features the measured encoding speed (in
frames per second) and the PSNR loss (in dB) compared to the "very
high quality" setting.
Please understand that depending on your source, your machine type
and development advancements, you may get very different results.
</para>

<para>
<informaltable frame="all">
<tgroup cols="4">
<thead>
<row>
  <entry>Description</entry>
  <entry>Encoding options</entry>
  <entry>speed (in fps)</entry>
  <entry>Relative PSNR loss (in dB)</entry>
</row>
</thead>
<tbody>
<row>
  <entry>Very high quality</entry>
  <entry><option>vcodec=mpeg4:mbd=2:mv0:trell:v4mv:cbp:last_pred=3:predia=2:dia=2:vmax_b_frames=2:vb_strategy=1:precmp=2:cmp=2:subcmp=2:preme=2:qns=2</option></entry>
  <entry>6fps</entry>
  <entry>0dB</entry>
</row>
<row>
  <entry>High quality</entry>
  <entry><option>vcodec=mpeg4:mbd=2:trell:v4mv:last_pred=2:dia=-1:vmax_b_frames=2:vb_strategy=1:cmp=3:subcmp=3:precmp=0:vqcomp=0.6:turbo</option></entry>
  <entry>15fps</entry>
  <entry>-0.5dB</entry>
</row>
<row>
  <entry>Fast</entry>
  <entry><option>vcodec=mpeg4:mbd=2:trell:v4mv:turbo</option></entry>
  <entry>42fps</entry>
  <entry>-0.74dB</entry>
</row>
<row>
  <entry>Realtime</entry>
  <entry><option>vcodec=mpeg4:mbd=2:turbo</option></entry>
  <entry>54fps</entry>
  <entry>-1.21dB</entry>
</row>
</tbody>
</tgroup>
</informaltable>
</para>
</sect2>

<!-- ********** -->

<sect2 id="custommatrices">
<title>Custom inter/intra matrices</title>

<para>
With this feature of
<systemitem class="library">libavcodec</systemitem>
you are able to set custom inter (I-frames/keyframes) and intra
(P-frames/predicted frames) matrices. It is supported by many of the codecs:
<systemitem>mpeg1video</systemitem> and <systemitem>mpeg2video</systemitem>
are reported as working.
</para>

<para>
A typical usage of this feature is to set the matrices preferred by the
<ulink url="http://www.kvcd.net/">KVCD</ulink> specifications.
</para>

<para>
The <emphasis role="bold">KVCD "Notch" Quantization Matrix:</emphasis>
</para>

<para>
Intra:
<screen>
 8  9 12 22 26 27 29 34
 9 10 14 26 27 29 34 37
12 14 18 27 29 34 37 38
22 26 27 31 36 37 38 40
26 27 29 36 39 38 40 48
27 29 34 37 38 40 48 58
29 34 37 38 40 48 58 69
34 37 38 40 48 58 69 79
</screen>

Inter:
<screen>
16 18 20 22 24 26 28 30
18 20 22 24 26 28 30 32
20 22 24 26 28 30 32 34
22 24 26 30 32 32 34 36
24 26 28 32 34 34 36 38
26 28 30 32 34 36 38 40
28 30 32 34 36 38 42 42
30 32 34 36 38 40 42 44
</screen>
</para>

<para>
Usage:
<screen>
mencoder <replaceable>input.avi</replaceable> -o <replaceable>output.avi</replaceable> -oac copy -ovc lavc \
    -lavcopts inter_matrix=...:intra_matrix=...
</screen>
</para>

<para>
<screen>
mencoder <replaceable>input.avi</replaceable> -ovc lavc -lavcopts \
vcodec=mpeg2video:intra_matrix=8,9,12,22,26,27,29,34,9,10,14,26,27,29,34,37,\
12,14,18,27,29,34,37,38,22,26,27,31,36,37,38,40,26,27,29,36,39,38,40,48,27,\
29,34,37,38,40,48,58,29,34,37,38,40,48,58,69,34,37,38,40,48,58,69,79\
:inter_matrix=16,18,20,22,24,26,28,30,18,20,22,24,26,28,30,32,20,22,24,26,\
28,30,32,34,22,24,26,30,32,32,34,36,24,26,28,32,34,34,36,38,26,28,30,32,34,\
36,38,40,28,30,32,34,36,38,42,42,30,32,34,36,38,40,42,44 -oac copy -o svcd.mpg
</screen>
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-dvd-mpeg4-example">
<title>Example</title>

<para>
So, you have just bought your shiny new copy of Harry Potter and the Chamber
of Secrets (widescreen edition, of course), and you want to rip this DVD
so that you can add it to your Home Theatre PC. This is a region 1 DVD,
so it is NTSC. The example below will still apply to PAL, except you will
omit <option>-ofps 24000/1001</option> (because the output framerate is the
same as the input framerate), and of course the crop dimensions will be
different.
</para>

<para>
After running <option>mplayer dvd://1</option>, we follow the process
detailed in the section <link linkend="menc-feat-telecine">How to deal
with telecine and interlacing in NTSC DVDs</link> and discover that it is
24000/1001 fps progressive video, which means that we need not use an inverse
telecine filter, such as <option>pullup</option> or
<option>filmdint</option>.
</para>

<para id="menc-feat-dvd-mpeg4-example-crop">
Next, we want to determine the appropriate crop rectangle, so we use the
cropdetect filter:
<screen>mplayer dvd://1 -vf cropdetect</screen>
Make sure you seek to a fully filled frame (such as a bright scene,
past the opening credits and logos), and
you will see in <application>MPlayer</application>'s console output:
<screen>crop area: X: 0..719  Y: 57..419  (-vf crop=720:362:0:58)</screen>
We then play the movie back with this filter to test its correctness:
<screen>mplayer dvd://1 -vf crop=720:362:0:58</screen>
And we see that it looks perfectly fine. Next, we ensure the width and
height are a multiple of 16. The width is fine, however the height is
not. Since we did not fail 7th grade math, we know that the nearest
multiple of 16 lower than 362 is 352.
</para>

<para>
We could just use <option>crop=720:352:0:58</option>, but it would be nice
to take a little off the top and a little off the bottom so that we
retain the center. We have shrunk the height by 10 pixels, but we do not
want to increase the y-offset by 5-pixels since that is an odd number and
will adversely affect quality. Instead, we will increase the y-offset by
4 pixels:
<screen>mplayer dvd://1 -vf crop=720:352:0:62</screen>
Another reason to shave pixels from both the top and the bottom is that we
ensure we have eliminated any half-black pixels if they exist. Note that if
your video is telecined, make sure the <option>pullup</option> filter (or
whichever inverse telecine filter you decide to use) appears in the filter
chain before you crop. If it is interlaced, deinterlace before cropping.
(If you choose to preserve the interlaced video, then make sure your
vertical crop offset is a multiple of 4.)
</para>

<para>
If you are really concerned about losing those 10 pixels, you might
prefer instead to scale the dimensions down to the nearest multiple of 16.
The filter chain would look like:
<screen>-vf crop=720:362:0:58,scale=720:352</screen>
Scaling the video down like this will mean that some small amount of
detail is lost, though it probably will not be perceptible. Scaling up will
result in lower quality (unless you increase the bitrate). Cropping
discards those pixels altogether. It is a tradeoff that you will want to
consider for each circumstance. For example, if the DVD video was made
for television, you might want to avoid vertical scaling, since the line
sampling corresponds to the way the content was originally recorded.
</para>

<para>
On inspection, we see that our movie has a fair bit of action and high
amounts of detail, so we pick 2400Kbit for our bitrate.
</para>

<para>
We are now ready to do the two pass encode. Pass one:
<screen>
mencoder dvd://1 -ofps 24000/1001 -oac copy -o <replaceable>Harry_Potter_2.avi</replaceable> -ovc lavc \
    -lavcopts vcodec=mpeg4:vbitrate=2400:v4mv:mbd=2:trell:cmp=3:subcmp=3:autoaspect:vpass=1 \
    -vf pullup,softskip,crop=720:352:0:62,hqdn3d=2:1:2
</screen>
And pass two is the same, except that we specify <option>vpass=2</option>:
<screen>
mencoder dvd://1 -ofps 24000/1001 -oac copy -o <replaceable>Harry_Potter_2.avi</replaceable> -ovc lavc \
    -lavcopts vcodec=mpeg4:vbitrate=2400:v4mv:mbd=2:trell:cmp=3:subcmp=3:autoaspect:vpass=2 \
    -vf pullup,softskip,crop=720:352:0:62,hqdn3d=2:1:2
</screen>
</para>

<para>
The options <option>v4mv:mbd=2:trell</option> will greatly increase the
quality at the expense of encoding time. There is little reason to leave
these options out when the primary goal is quality. The options
<option>cmp=3:subcmp=3</option> select a comparison function that
yields higher quality than the defaults. You might try experimenting with
this parameter (refer to the man page for the possible values) as
different functions can have a large impact on quality depending on the
source material. For example, if you find
<systemitem class="library">libavcodec</systemitem> produces too much
blocky artifacts, you could try selecting the experimental NSSE as
comparison function via <option>*cmp=10</option>.
</para>

<para>
For this movie, the resulting AVI will be 138 minutes long and nearly
3GB. And because you said that file size does not matter, this is a
perfectly acceptable size. However, if you had wanted it smaller, you
could try a lower bitrate. Increasing bitrates have diminishing
returns, so while we might clearly see an improvement from 1800Kbit to
2000Kbit, it might not be so noticeable above 2000Kbit. Feel
free to experiment until you are happy.
</para>

<para>
Because we passed the source video through a denoise filter, you may want
to add some of it back during playback. This, along with the
<option>spp</option> post-processing filter, drastically improves the
perception of quality and helps eliminate blocky artifacts in the video.
With <application>MPlayer</application>'s <option>autoq</option> option,
you can vary the amount of post-processing done by the spp filter
depending on available CPU. Also, at this point, you may want to apply
gamma and/or color correction to best suit your display. For example:
<screen>
mplayer <replaceable>Harry_Potter_2.avi</replaceable> -vf spp,noise=9ah:5ah,eq2=1.2 -autoq 3
</screen>
</para>
</sect2>
</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-xvid">
<title>Encoding with the <systemitem class="library">Xvid</systemitem>
  codec</title>

<para>
<systemitem class="library">Xvid</systemitem> is a free library for
encoding MPEG-4 ASP video streams.
Before starting to encode, you need to <link linkend="xvid">
set up <application>MEncoder</application> to support it</link>.
</para>

<para>
This guide mainly aims at featuring the same kind of information
as x264's encoding guide.
Therefore, please begin by reading
<link linkend="menc-feat-x264-encoding-options-intro">the first part</link>
of that guide.
</para>

<!-- ********** -->

<sect2 id="menc-feat-xvid-intro">
<title>What options should I use to get the best results?</title>

<para>
Please begin by reviewing the
<systemitem class="library">Xvid</systemitem> section of
<application>MPlayer</application>'s man page.
This section is intended to be a supplement to the man page.
</para>

<para>
The Xvid default settings are already a good tradeoff between
speed and quality, therefore you can safely stick to them if
the following section puzzles you.
</para>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-xvid-encoding-options">
<title>Encoding options of <systemitem class="library">Xvid</systemitem></title>

<itemizedlist>
<listitem><para>
  <emphasis role="bold">vhq</emphasis>
  This setting affects the macroblock decision algorithm, where the
  higher the setting, the wiser the decision.
  The default setting may be safely used for every encode, while
  higher settings always help PSNR but are significantly slower.
  Please note that a better PSNR does not necessarily mean
  that the picture will look better, but tells you that it is
  closer to the original.
  Turning it off will noticeably speed up encoding; if speed is
  critical for you, the tradeoff may be worth it.
</para></listitem>
<listitem><para>
  <emphasis role="bold">bvhq</emphasis>
  This does the same job as vhq, but does it on B-frames.
  It has a negligible impact on speed, and slightly improves quality
  (around +0.1dB PSNR).
</para></listitem>
<listitem><para>
  <emphasis role="bold">max_bframes</emphasis>
  A higher number of consecutive allowed B-frames usually improves
  compressibility, although it may also lead to more blocking artifacts.
  The default setting is a good tradeoff between compressibility and
  quality, but you may increase it up to 3 if you are bitrate-starved.
  You may also decrease it to 1 or 0 if you are aiming at perfect
  quality, though in that case you should make sure your
  target bitrate is high enough to ensure that the encoder does not
  have to increase quantizers to reach it.
</para></listitem>
<listitem><para>
  <emphasis role="bold">bf_threshold</emphasis>
  This controls the B-frame sensitivity of the encoder, where a higher
  value leads to more B-frames being used (and vice versa).
  This setting is to be used together with <option>max_bframes</option>;
  if you are bitrate-starved, you should increase both
  <option>max_bframes</option> and <option>bf_threshold</option>,
  while you may increase <option>max_bframes</option> and reduce
  <option>bf_threshold</option> so that the encoder may use more
  B-frames in places that only <emphasis role="bold">really</emphasis>
  need them.
  A low number of <option>max_bframes</option> and a high value of
  <option>bf_threshold</option> is probably not a wise choice as it
  will force the encoder to put B-frames in places that would not
  benefit from them, therefore reducing visual quality.
  However, if you need to be compatible with standalone players that
  only support old DivX profiles (which only supports up to 1
  consecutive B-frame), this would be your only way to
  increase compressibility through using B-frames.
</para></listitem>
<listitem><para>
  <emphasis role="bold">trellis</emphasis>
  Optimizes the quantization process to get an optimal tradeoff
  between PSNR and bitrate, which allows significant bit saving.
  These bits will in return be spent elsewhere on the video,
  raising overall visual quality.
  You should always leave it on as its impact on quality is huge.
  Even if you are looking for speed, do not disable it until you
  have turned down <option>vhq</option> and all other more
  CPU-hungry options to the minimum.
</para></listitem>
<listitem><para>
  <emphasis role="bold">hq_ac</emphasis>
  Activates a better coefficient cost estimation method, which slightly
  reduces file size by around 0.15 to 0.19% (which corresponds to less
  than 0.01dB PSNR increase), while having a negligible impact on speed.
  It is therefore recommended to always leave it on.
</para></listitem>
<listitem><para>
 <emphasis role="bold">cartoon</emphasis>
  Designed to better encode cartoon content, and has no impact on
  speed as it just tunes the mode decision heuristics for this type
  of content.
</para></listitem>
<listitem>
  <para>
  <emphasis role="bold">me_quality</emphasis>
  This setting is to control the precision of the motion estimation.
  The higher <option>me_quality</option>, the more
  precise the estimation of the original motion will be, and the
  better the resulting clip will capture the original motion.
  </para>
  <para>
  The default setting is best in all cases;
  thus it is not recommended to turn it down unless you are
  really looking for speed, as all the bits saved by a good motion
  estimation would be spent elsewhere, raising overall quality.
  Therefore, do not go any lower than 5, and even that only as a last
  resort.
  </para>
</listitem>
<listitem><para>
  <emphasis role="bold">chroma_me</emphasis>
  Improves motion estimation by also taking the chroma (color)
  information into account, whereas <option>me_quality</option>
  alone only uses luma (grayscale).
  This slows down encoding by 5-10% but improves visual quality
  quite a bit by reducing blocking effects and reduces file size by
  around 1.3%.
  If you are looking for speed, you should disable this option before
  starting to consider reducing <option>me_quality</option>.
</para></listitem>
<listitem><para>
  <emphasis role="bold">chroma_opt</emphasis>
  Is intended to increase chroma image quality around pure
  white/black edges, rather than improving compression.
  This can help to reduce the "red stairs" effect.
</para></listitem>
<listitem><para>
  <emphasis role="bold">lumi_mask</emphasis>
  Tries to give less bitrate to part of the picture that the
  human eye cannot see very well, which should allow the encoder
  to spend the saved bits on more important parts of the picture.
  The quality of the encode yielded by this option highly depends
  on personal preferences and on the type and monitor settings
  used to watch it (typically, it will not look as good if it is
  bright or if it is a TFT monitor).
</para></listitem>
<listitem>
  <para>
  <emphasis role="bold">qpel</emphasis>
  Raise the number of candidate motion vectors by increasing
  the precision of the motion estimation from halfpel to
  quarterpel.
  The idea is to find better motion vectors which will in return
  reduce bitrate (hence increasing quality).
  However, motion vectors with quarterpel precision require a
  few extra bits to code, but the candidate vectors do not always
  give (much) better results.
  Quite often, the codec still spends bits on the extra precision,
  but little or no extra quality is gained in return.
  Unfortunately, there is no way to foresee the possible gains of
  <option>qpel</option>, so you need to actually encode with and
  without it to know for sure.
  </para>
  <para>
  <option>qpel</option> can be almost double encoding time, and
  requires as much as 25% more processing power to decode.
  It is not supported by all standalone players.
  </para>
</listitem>
<listitem><para>
  <emphasis role="bold">gmc</emphasis>
  Tries to save bits on panning scenes by using a single motion
  vector for the whole frame.
  This almost always raises PSNR, but significantly slows down
  encoding (as well as decoding).
  Therefore, you should only use it when you have turned
  <option>vhq</option> to the maximum.
  <systemitem class="library">Xvid</systemitem>'s GMC is more
  sophisticated than DivX's, but is only supported by few
  standalone players.
</para></listitem>
</itemizedlist>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-xvid-encoding-profiles">
<title>Encoding profiles</title>

<para>
Xvid supports encoding profiles through the <option>profile</option> option,
which are used to impose restrictions on the properties of the Xvid video
stream such that it will be playable on anything which supports the
chosen profile.
The restrictions relate to resolutions, bitrates and certain MPEG-4
features.
The following table shows what each profile supports.
</para>

<informaltable>
<tgroup cols="16" align="center">
<colspec colnum="1"  colname="col1"/>
<colspec colnum="2"  colname="col2"/>
<colspec colnum="3"  colname="col3"/>
<colspec colnum="4"  colname="col4"/>
<colspec colnum="5"  colname="col5"/>
<colspec colnum="6"  colname="col6"/>
<colspec colnum="7"  colname="col7"/>
<colspec colnum="8"  colname="col8"/>
<colspec colnum="9"  colname="col9"/>
<colspec colnum="10" colname="col10"/>
<colspec colnum="11" colname="col11"/>
<colspec colnum="12" colname="col12"/>
<colspec colnum="13" colname="col13"/>
<colspec colnum="14" colname="col14"/>
<colspec colnum="15" colname="col15"/>
<colspec colnum="16" colname="col16"/>
<colspec colnum="17" colname="col17"/>
<spanspec spanname="spa2-5"   namest="col2" nameend="col5"/>
<spanspec spanname="spa6-11"  namest="col6" nameend="col11"/>
<spanspec spanname="spa12-17" namest="col12" nameend="col17"/>
<tbody>
<row>
  <entry></entry>
  <entry spanname="spa2-5">Simple</entry>
  <entry spanname="spa6-11">Advanced Simple</entry>
  <entry spanname="spa12-17">DivX</entry>
</row>
<row>
  <entry>Profile name</entry>
  <entry>0</entry>
  <entry>1</entry>
  <entry>2</entry>
  <entry>3</entry>
  <entry>0</entry>
  <entry>1</entry>
  <entry>2</entry>
  <entry>3</entry>
  <entry>4</entry>
  <entry>5</entry>
  <entry>Handheld</entry>
  <entry>Portable NTSC</entry>
  <entry>Portable PAL</entry>
  <entry>Home Theater NTSC</entry>
  <entry>Home Theater PAL</entry>
  <entry>HDTV</entry>
</row>
<row>
  <entry>Width [pixels]</entry>
  <entry>176</entry>
  <entry>176</entry>
  <entry>352</entry>
  <entry>352</entry>
  <entry>176</entry>
  <entry>176</entry>
  <entry>352</entry>
  <entry>352</entry>
  <entry>352</entry>
  <entry>720</entry>
  <entry>176</entry>
  <entry>352</entry>
  <entry>352</entry>
  <entry>720</entry>
  <entry>720</entry>
  <entry>1280</entry>
</row>
<row>
  <entry>Height [pixels]</entry>
  <entry>144</entry>
  <entry>144</entry>
  <entry>288</entry>
  <entry>288</entry>
  <entry>144</entry>
  <entry>144</entry>
  <entry>288</entry>
  <entry>288</entry>
  <entry>576</entry>
  <entry>576</entry>
  <entry>144</entry>
  <entry>240</entry>
  <entry>288</entry>
  <entry>480</entry>
  <entry>576</entry>
  <entry>720</entry>
</row>
<row>
  <entry>Frame rate [fps]</entry>
  <entry>15</entry>
  <entry>15</entry>
  <entry>15</entry>
  <entry>15</entry>
  <entry>30</entry>
  <entry>30</entry>
  <entry>15</entry>
  <entry>30</entry>
  <entry>30</entry>
  <entry>30</entry>
  <entry>15</entry>
  <entry>30</entry>
  <entry>25</entry>
  <entry>30</entry>
  <entry>25</entry>
  <entry>30</entry>
</row>
<row>
  <entry>Max average bitrate [kbps]</entry>
  <entry>64</entry>
  <entry>64</entry>
  <entry>128</entry>
  <entry>384</entry>
  <entry>128</entry>
  <entry>128</entry>
  <entry>384</entry>
  <entry>768</entry>
  <entry>3000</entry>
  <entry>8000</entry>
  <entry>537.6</entry>
  <entry>4854</entry>
  <entry>4854</entry>
  <entry>4854</entry>
  <entry>4854</entry>
  <entry>9708.4</entry>
</row>
<row>
  <entry>Peak average bitrate over 3 secs [kbps]</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>800</entry>
  <entry>8000</entry>
  <entry>8000</entry>
  <entry>8000</entry>
  <entry>8000</entry>
  <entry>16000</entry>
</row>
<row>
  <entry>Max. B-frames</entry>
  <entry>0</entry>
  <entry>0</entry>
  <entry>0</entry>
  <entry>0</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>0</entry>
  <entry>1</entry>
  <entry>1</entry>
  <entry>1</entry>
  <entry>1</entry>
  <entry>2</entry>
</row>
<row>
  <entry>MPEG quantization</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
</row>
<row>
  <entry>Adaptive quantization</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
</row>
<row>
  <entry>Interlaced encoding</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
</row>
<row>
  <entry>Quarterpixel</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
</row>
<row>
  <entry>Global motion compensation</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry>X</entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
  <entry></entry>
</row>
</tbody>
</tgroup>
</informaltable>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-xvid-example-settings">
<title>Encoding setting examples</title>

<para>
The following settings are examples of different encoding
option combinations that affect the speed vs quality tradeoff
at the same target bitrate.
</para>

<para>
All the encoding settings were tested on a 720x448 @30000/1001 fps
video sample, the target bitrate was 900kbps, and the machine was an
AMD-64 3400+ at 2400 MHz in 64 bits mode.
Each encoding setting features the measured encoding speed (in
frames per second) and the PSNR loss (in dB) compared to the "very
high quality" setting.
Please understand that depending on your source, your machine type
and development advancements, you may get very different results.
</para>

<informaltable frame="all">
<tgroup cols="4">
<thead>
<row><entry>Description</entry><entry>Encoding options</entry><entry>speed (in fps)</entry><entry>Relative PSNR loss (in dB)</entry></row>
</thead>
<tbody>
<row>
  <entry>Very high quality</entry>
  <entry><option>chroma_opt:vhq=4:bvhq=1:quant_type=mpeg</option></entry>
  <entry>16fps</entry>
  <entry>0dB</entry>
</row>
<row>
  <entry>High quality</entry>
  <entry><option>vhq=2:bvhq=1:chroma_opt:quant_type=mpeg</option></entry>
  <entry>18fps</entry>
  <entry>-0.1dB</entry>
</row>
<row>
  <entry>Fast</entry>
  <entry><option>turbo:vhq=0</option></entry>
  <entry>28fps</entry>
  <entry>-0.69dB</entry>
</row>
<row>
  <entry>Realtime</entry>
  <entry><option>turbo:nochroma_me:notrellis:max_bframes=0:vhq=0</option></entry>
  <entry>38fps</entry>
  <entry>-1.48dB</entry>
</row>
</tbody>
</tgroup>
</informaltable>
</sect2>
</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-x264">
<title>Encoding with the
  <systemitem class="library">x264</systemitem> codec</title>

<para>
<systemitem class="library">x264</systemitem> is a free library for
encoding H.264/AVC video streams.
Before starting to encode, you need to
<link linkend="x264">set up <application>MEncoder</application> to support it</link>.
</para>

<!-- ********** -->

<sect2 id="menc-feat-x264-encoding-options">
<title>Encoding options of x264</title>

<para>
Please begin by reviewing the
<systemitem class="library">x264</systemitem> section of
<application>MPlayer</application>'s man page.
This section is intended to be a supplement to the man page.
Here you will find quick hints about which options are most
likely to interest most people. The man page is more terse,
but also more exhaustive, and it sometimes offers much better
technical detail.
</para>


<sect3 id="menc-feat-x264-encoding-options-intro">
<title>Introduction</title>

<para>
This guide considers two major categories of encoding options:
</para>

<orderedlist>
<listitem><para>
  Options which mainly trade off encoding time vs. quality
</para></listitem>
<listitem><para>
  Options which may be useful for fulfilling various personal
  preferences and special requirements
</para></listitem>
</orderedlist>

<para>
Ultimately, only you can decide which options are best for your
purposes. The decision for the first class of options is the simplest:
you only have to decide whether you think the quality differences
justify the speed differences. For the second class of options,
preferences may be far more subjective, and more factors may be
involved. Note that some of the "personal preferences and special
requirements" options can still have large impacts on speed or quality,
but that is not what they are primarily useful for. A couple of the
"personal preference" options may even cause changes that look better
to some people, but look worse to others.
</para>

<para>
Before continuing, you need to understand that this guide uses only one
quality metric: global PSNR.
For a brief explanation of what PSNR is, see
<ulink url="http://en.wikipedia.org/wiki/PSNR">the Wikipedia article on PSNR</ulink>.
Global PSNR is the last PSNR number reported when you include
the <option>psnr</option> option in <option>x264encopts</option>.
Any time you read a claim about PSNR, one of the assumptions
behind the claim is that equal bitrates are used.
</para>

<para>
Nearly all of this guide's comments assume you are using two pass.
When comparing options, there are two major reasons for using
two pass encoding.
First, using two pass often gains around 1dB PSNR, which is a
very big difference.
Secondly, testing options by doing direct quality comparisons
with one pass encodes introduces a major confounding
factor: bitrate often varies significantly with each encode.
It is not always easy to tell whether quality changes are due
mainly to changed options, or if they mostly reflect essentially
random differences in the achieved bitrate.
</para>
</sect3>


<sect3 id="menc-feat-x264-encoding-options-speedvquality">
<title>Options which primarily affect speed and quality</title>

<itemizedlist>
<listitem>
  <para>
  <emphasis role="bold">subq</emphasis>:
  Of the options which allow you to trade off speed for quality,
  <option>subq</option> and <option>frameref</option> (see below) are usually
  by far the most important.
  If you are interested in tweaking either speed or quality, these
  are the first options you should consider.
  On the speed dimension, the <option>frameref</option> and
  <option>subq</option> options interact with each other fairly
  strongly.
  Experience shows that, with one reference frame,
  <option>subq=5</option> (the default setting) takes about 35% more time than
  <option>subq=1</option>.
  With 6 reference frames, the penalty grows to over 60%.
  <option>subq</option>'s effect on PSNR seems fairly constant
  regardless of the number of reference frames.
  Typically, <option>subq=5</option> achieves 0.2-0.5 dB higher global
  PSNR in comparison <option>subq=1</option>.
  This is usually enough to be visible.
  </para>
  <para>
  <option>subq=6</option> is slower and yields better quality at a reasonable
  cost.
  In comparison to <option>subq=5</option>, it usually gains 0.1-0.4 dB
  global PSNR with speed costs varying from 25%-100%.
  Unlike other levels of <option>subq</option>, the behavior of
  <option>subq=6</option> does not depend much on <option>frameref</option>
  and <option>me</option>.  Instead, the effectiveness of <option>subq=6
  </option> depends mostly upon the number of B-frames used. In normal
  usage, this means <option>subq=6</option> has a large impact on both speed
  and quality in complex, high motion scenes, but it may not have much effect
  in low-motion scenes. Note that it is still recommended to always set
  <option>bframes</option> to something other than zero (see below).
  </para>
  <para>
  <option>subq=7</option> is the slowest, highest quality mode.
  In comparison to <option>subq=6</option>, it usually gains 0.01-0.05 dB
  global PSNR with speed costs varying from 15%-33%.
  Since the tradeoff encoding time vs. quality is quite low, you should
  only use it if you are after every bit saving and if encoding time is
  not an issue.
  </para>
</listitem>
<listitem>
  <para>
  <emphasis role="bold">frameref</emphasis>:
  <option>frameref</option> is set to 1 by default, but this
  should not be taken to imply that it is reasonable to set it to 1.
  Merely raising <option>frameref</option> to 2 gains around
  0.15dB PSNR with a 5-10% speed penalty; this seems like a good tradeoff.
  <option>frameref=3</option> gains around 0.25dB PSNR over
  <option>frameref=1</option>, which should be a visible difference.
  <option>frameref=3</option> is around 15% slower than
  <option>frameref=1</option>.
  Unfortunately, diminishing returns set in rapidly.
  <option>frameref=6</option> can be expected to gain only
  0.05-0.1 dB over <option>frameref=3</option> at an additional
  15% speed penalty.
  Above <option>frameref=6</option>, the quality gains are
  usually very small (although you should keep in mind throughout
  this whole discussion that it can vary quite a lot depending on your source).
  In a fairly typical case, <option>frameref=12</option>
  will improve global PSNR by a tiny 0.02dB over
  <option>frameref=6</option>, at a speed cost of 15%-20%.
  At such high <option>frameref</option> values, the only really
  good thing that can be said is that increasing it even further will
  almost certainly never <emphasis role="bold">harm</emphasis>
  PSNR, but the additional quality benefits are barely even
  measurable, let alone perceptible.
  </para>
  <note><title>Note:</title>
  <para>
  Raising <option>frameref</option> to unnecessarily high values
  <emphasis role="bold">can</emphasis> and
  <emphasis role="bold">usually does</emphasis>
  hurt coding efficiency if you turn CABAC off.
  With CABAC on (the default behavior), the possibility of setting
  <option>frameref</option> "too high" currently seems too remote
  to even worry about, and in the future, optimizations may remove
  the possibility altogether.
  </para></note>
  <para>
  If you care about speed, a reasonable compromise is to use low
  <option>subq</option> and <option>frameref</option> values on
  the first pass, and then raise them on the second pass.
  Typically, this has a negligible negative effect on the final
  quality: You will probably lose well under 0.1dB PSNR, which
  should be much too small of a difference to see.
  However, different values of <option>frameref</option> can
  occasionally affect frame type decision.
  Most likely, these are rare outlying cases, but if you want to
  be pretty sure, consider whether your video has either
  fullscreen repetitive flashing patterns or very large temporary
  occlusions which might force an I-frame.
  Adjust the first-pass <option>frameref</option> so it is large
  enough to contain the duration of the flashing cycle (or occlusion).
  For example, if the scene flashes back and forth between two images
  over a duration of three frames, set the first pass
  <option>frameref</option> to 3 or higher.
  This issue is probably extremely rare in live action video material,
  but it does sometimes come up in video game captures.
  </para>
</listitem>
<listitem>
  <para>
  <emphasis role="bold">me</emphasis>:
  This option is for choosing the motion estimation search method.
  Altering this option provides a straightforward quality-vs-speed
  tradeoff. <option>me=dia</option> is only a few percent faster than
  the default search, at a cost of under 0.1dB global PSNR. The
  default setting (<option>me=hex</option>) is a reasonable tradeoff
  between speed and quality. <option>me=umh</option> gains a little under
  0.1dB global PSNR, with a speed penalty that varies depending on
  <option>frameref</option>.  At high values of
  <option>frameref</option> (e.g. 12 or so), <option>me=umh</option>
  is about 40% slower than the default <option> me=hex</option>. With
  <option>frameref=3</option>, the speed penalty incurred drops to
  25%-30%.
  </para>
  <para>
  <option>me=esa</option> uses an exhaustive search that is too slow for
  practical use.
  </para>
</listitem>
<listitem><para>
  <emphasis role="bold">partitions=all</emphasis>:
  This option enables the use of 8x4, 4x8 and 4x4 subpartitions in
  predicted macroblocks (in addition to the default partitions).
  Enabling it results in a fairly consistent
  10%-15% loss of speed. This option is rather useless in source
  containing only low motion, however in some high-motion source,
  particularly source with lots of small moving objects, gains of
  about 0.1dB can be expected.
</para></listitem>
<listitem>
  <para>
  <emphasis role="bold">bframes</emphasis>:
  If you are used to encoding with other codecs, you may have found
  that B-frames are not always useful.
  In H.264, this has changed: there are new techniques and block
  types that are possible in B-frames.
  Usually, even a naive B-frame choice algorithm can have a
  significant PSNR benefit.
  It is interesting to note that using B-frames usually speeds up
  the second pass somewhat, and may also speed up a single
  pass encode if adaptive B-frame decision is turned off.
  </para>
  <para>
  With adaptive B-frame decision turned off
  (<option>x264encopts</option>'s <option>nob_adapt</option>),
  the optimal value for this setting is usually no more than
  <option>bframes=1</option>, or else high-motion scenes can suffer.
  With adaptive B-frame decision on (the default behavior), it is
  safe to use higher values; the encoder will reduce the use of
  B-frames in scenes where they would hurt compression.
  The encoder rarely chooses to use more than 3 or 4 B-frames;
  setting this option any higher will have little effect.
  </para>
</listitem>
<listitem>
  <para>
  <emphasis role="bold">b_adapt</emphasis>:
  Note: This is on by default.
  </para>
  <para>
  With this option enabled, the encoder will use a reasonably fast
  decision process to reduce the number of B-frames used in scenes that
  might not benefit from them as much.
  You can use <option>b_bias</option> to tweak how B-frame-happy
  the encoder is.
  The speed penalty of adaptive B-frames is currently rather modest,
  but so is the potential quality gain.
  It usually does not hurt, however.
  Note that this only affects speed and frame type decision on the
  first pass.
  <option>b_adapt</option> and <option>b_bias</option> have no
  effect on subsequent passes.
  </para>
</listitem>
<listitem><para>
  <emphasis role="bold">b_pyramid</emphasis>:
  You might as well enable this option if you are using >=2 B-frames;
  as the man page says, you get a little quality improvement at no
  speed cost.
  Note that these videos cannot be read by libavcodec-based decoders
  older than about March 5, 2005.
</para></listitem>
<listitem>
  <para>
  <emphasis role="bold">weight_b</emphasis>:
  In typical cases, there is not much gain with this option.
  However, in crossfades or fade-to-black scenes, weighted
  prediction gives rather large bitrate savings.
  In MPEG-4 ASP, a fade-to-black is usually best coded as a series
  of expensive I-frames; using weighted prediction in B-frames
  makes it possible to turn at least some of these into much smaller
  B-frames.
  Encoding time cost is minimal, as no extra decisions need to be made.
  Also, contrary to what some people seem to guess, the decoder
  CPU requirements are not much affected by weighted prediction,
  all else being equal.
  </para>
  <para>
  Unfortunately, the current adaptive B-frame decision algorithm
  has a strong tendency to avoid B-frames during fades.
  Until this changes, it may be a good idea to add
  <option>nob_adapt</option> to your x264encopts, if you expect
  fades to have a large effect in your particular video
  clip.
  </para>
</listitem>
<listitem id="menc-feat-x264-encoding-options-speedvquality-threads">
  <para>
  <emphasis role="bold">threads</emphasis>:
  This option allows to spawn threads to encode in parallel on multiple CPUs.
  You can manually select the number of threads to be created or, better, set
  <option>threads=auto</option> and let
  <systemitem class="library">x264</systemitem> detect how many CPUs are
  available and pick an appropriate number of threads.
  If you have a multi-processor machine, you should really consider using it
  as it can to increase encoding speed linearly with the number of CPU cores
  (about 94% per CPU core), with very little quality reduction (about 0.005dB
  for dual processor, about 0.01dB for a quad processor machine).
  </para>
</listitem>
</itemizedlist>
</sect3>


<sect3 id="menc-feat-x264-encoding-options-misc-preferences">
<title>Options pertaining to miscellaneous preferences</title>

<itemizedlist>
<listitem>
  <para>
  <emphasis role="bold">Two pass encoding</emphasis>:
  Above, it was suggested to always use two pass encoding, but there
  are still reasons for not using it. For instance, if you are capturing
  live TV and encoding in realtime, you are forced to use single-pass.
  Also, one pass is obviously faster than two passes; if you use the
  exact same set of options on both passes, two pass encoding is almost
  twice as slow.
  </para>
  <para>
  Still, there are very good reasons for using two pass encoding. For
  one thing, single pass ratecontrol is not psychic, and it often makes
  unreasonable choices because it cannot see the big picture. For example,
  suppose you have a two minute long video consisting of two distinct
  halves.  The first half is a very high-motion scene lasting 60 seconds
  which, in isolation, requires about 2500kbps in order to look decent.
  Immediately following it is a much less demanding 60-second scene
  that looks good at 300kbps. Suppose you ask for 1400kbps on the theory
  that this is enough to accommodate both scenes. Single pass ratecontrol
  will make a couple of "mistakes" in such a case. First of all, it
  will target 1400kbps in both segments. The first segment may end up
  heavily overquantized, causing it to look unacceptably and unreasonably
  blocky. The second segment will be heavily underquantized; it may look
  perfect, but the bitrate cost of that perfection will be completely
  unreasonable. What is even harder to avoid is the problem at the
  transition between the two scenes. The first seconds of the low motion
  half will be hugely over-quantized, because the ratecontrol is still
  expecting the kind of bitrate requirements it met in the first half
  of the video. This "error period" of heavily over-quantized low motion
  will look jarringly bad, and will actually use less than the 300kbps
  it would have taken to make it look decent. There are ways to
  mitigate the pitfalls of single-pass encoding, but they may tend to
  increase bitrate misprediction.
  </para>
  <para>
  Multipass ratecontrol can offer huge advantages over a single pass.
  Using the statistics gathered from the first pass encode, the encoder
  can estimate, with reasonable accuracy, the "cost" (in bits) of
  encoding any given frame, at any given quantizer. This allows for
  a much more rational, better planned allocation of bits between the
  expensive (high-motion) and cheap (low-motion) scenes. See
  <option>qcomp</option> below for some ideas on how to tweak this
  allocation to your liking.
  </para>
  <para>
  Moreover, two passes need not take twice as long as one pass. You can
  tweak the options in the first pass for higher speed and lower quality.
  If you choose your options well, you can get a very fast first pass.
  The resulting quality in the second pass will be slightly lower because size
  prediction is less accurate, but the quality difference is normally much
  too small to be visible. Try, for example, adding
  <option>subq=1:frameref=1</option> to the first pass
  <option>x264encopts</option>. Then, on the second pass, use slower,
  higher-quality options:
  <option>subq=6:frameref=15:partitions=all:me=umh</option>
  </para>
</listitem>
<listitem><para>
  <emphasis role="bold">Three pass encoding</emphasis>?
  x264 offers the ability to make an arbitrary number of consecutive
  passes. If you specify <option>pass=1</option> on the first pass,
  then use <option>pass=3</option> on a subsequent pass, the subsequent
  pass will both read the statistics from the previous pass, and write
  its own statistics. An additional pass following this one will have
  a very good base from which to make highly accurate predictions of
  frame sizes at a chosen quantizer. In practice, the overall quality
  gain from this is usually close to zero, and quite possibly a third
  pass will result in slightly worse global PSNR than the pass before
  it. In typical usage, three passes help if you get either bad bitrate
  prediction or bad looking scene transitions when using only two passes.
  This is somewhat likely to happen on extremely short clips. There are
  also a few special cases in which three (or more) passes are handy
  for advanced users, but for brevity, this guide omits discussing those
  special cases.
</para></listitem>
<listitem><para>
  <emphasis role="bold">qcomp</emphasis>:
  <option>qcomp</option> trades off the number of bits allocated
  to "expensive" high-motion versus "cheap" low-motion frames. At
  one extreme, <option>qcomp=0</option> aims for true constant
  bitrate. Typically this would make high-motion scenes look completely
  awful, while low-motion scenes would probably look absolutely
  perfect, but would also use many times more bitrate than they
  would need in order to look merely excellent. At the other extreme,
  <option>qcomp=1</option> achieves nearly constant quantization parameter
  (QP). Constant QP does not look bad, but most people think it is more
  reasonable to shave some bitrate off of the extremely expensive scenes
  (where the loss of quality is not as noticeable) and reallocate it to
  the scenes that are easier to encode at excellent quality.
  <option>qcomp</option> is set to 0.6 by default, which may be slightly
  low for many peoples' taste (0.7-0.8 are also commonly used).
</para></listitem>
<listitem><para>
  <emphasis role="bold">keyint</emphasis>:
  <option>keyint</option> is solely for trading off file seekability against
  coding efficiency. By default, <option>keyint</option> is set to 250. In
  25fps material, this guarantees the ability to seek to within 10 seconds
  precision. If you think it would be important and useful to be able to
  seek within 5 seconds of precision, set <option>keyint=125</option>;
  this will hurt quality/bitrate slightly. If you care only about quality
  and not about seekability, you can set it to much higher values
  (understanding that there are diminishing returns which may become
  vanishingly low, or even zero). The video stream will still have seekable
  points as long as there are some scene changes.
</para></listitem>
<listitem>
  <para>
  <emphasis role="bold">deblock</emphasis>:
  This topic is going to be a bit controversial.
  </para>
  <para>
  H.264 defines a simple deblocking procedure on I-blocks that uses
  pre-set strengths and thresholds depending on the QP of the block
  in question.
  By default, high QP blocks are filtered heavily, and low QP blocks
  are not deblocked at all.
  The pre-set strengths defined by the standard are well-chosen and
  the odds are very good that they are PSNR-optimal for whatever
  video you are trying to encode.
  The <option>deblock</option> allow you to specify offsets to the preset
  deblocking thresholds.
  </para>
  <para>
  Many people seem to think it is a good idea to lower the deblocking
  filter strength by large amounts (say, -3).
  This is however almost never a good idea, and in most cases,
  people who are doing this do not understand very well how
  deblocking works by default.
  </para>
  <para>
  The first and most important thing to know about the in-loop
  deblocking filter is that the default thresholds are almost always
  PSNR-optimal.
  In the rare cases that they are not optimal, the ideal offset is
  plus or minus 1.
  Adjusting deblocking parameters by a larger amount is almost
  guaranteed to hurt PSNR.
  Strengthening the filter will smear more details; weakening the
  filter will increase the appearance of blockiness.
  </para>
  <para>
  It is definitely a bad idea to lower the deblocking thresholds if
  your source is mainly low in spacial complexity (i.e., not a lot
  of detail or noise).
  The in-loop filter does a rather excellent job of concealing
  the artifacts that occur.
  If the source is high in spacial complexity, however, artifacts
  are less noticeable.
  This is because the ringing tends to look like detail or noise.
  Human visual perception easily notices when detail is removed,
  but it does not so easily notice when the noise is wrongly
  represented.
  When it comes to subjective quality, noise and detail are somewhat
  interchangeable.
  By lowering the deblocking filter strength, you are most likely
  increasing error by adding ringing artifacts, but the eye does
  not notice because it confuses the artifacts with detail.
  </para>
  <para>
  This <emphasis role="bold">still</emphasis> does not justify
  lowering the deblocking filter strength, however.
  You can generally get better quality noise from postprocessing.
  If your H.264 encodes look too blurry or smeared, try playing with
  <option>-vf noise</option> when you play your encoded movie.
  <option>-vf noise=8a:4a</option> should conceal most mild
  artifacts.
  It will almost certainly look better than the results you
  would have gotten just by fiddling with the deblocking filter.
  </para>
</listitem>
</itemizedlist>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-x264-example-settings">
<title>Encoding setting examples</title>

<para>
The following settings are examples of different encoding
option combinations that affect the speed vs quality tradeoff
at the same target bitrate.
</para>

<para>
All the encoding settings were tested on a 720x448 @30000/1001 fps
video sample, the target bitrate was 900kbps, and the machine was an
AMD-64 3400+ at 2400 MHz in 64 bits mode.
Each encoding setting features the measured encoding speed (in
frames per second) and the PSNR loss (in dB) compared to the "very
high quality" setting.
Please understand that depending on your source, your machine type
and development advancements, you may get very different results.
</para>

<informaltable frame="all">
<tgroup cols="4">
<thead>
<row>
  <entry>Description</entry>
  <entry>Encoding options</entry>
  <entry>speed (in fps)</entry>
  <entry>Relative PSNR loss (in dB)</entry>
</row>
</thead>
<tbody>
<row>
  <entry>Very high quality</entry>
  <entry><option>subq=6:partitions=all:8x8dct:me=umh:frameref=5:bframes=3:b_pyramid=normal:weight_b</option></entry>
  <entry>6fps</entry>
  <entry>0dB</entry>
</row>
<row>
  <entry>High quality</entry>
  <entry><option>subq=5:8x8dct:frameref=2:bframes=3:b_pyramid=normal:weight_b</option></entry>
  <entry>13fps</entry>
  <entry>-0.89dB</entry>
</row>
<row>
  <entry>Fast</entry>
  <entry><option>subq=4:bframes=2:b_pyramid=normal:weight_b</option></entry>
  <entry>17fps</entry>
  <entry>-1.48dB</entry>
</row>
</tbody>
</tgroup>
</informaltable>
</sect2>
</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-video-for-windows">
<title>
  Encoding with the <systemitem class="library">Video For Windows</systemitem>
  codec family
</title>

<para>
Video for Windows provides simple encoding by means of binary video codecs.
You can encode with the following codecs (if you have more, please tell us!)
</para>

<para>
Note that support for this is very experimental and some codecs may not work
correctly. Some codecs will only work in certain colorspaces, try
<option>-vf format=bgr24</option> and <option>-vf format=yuy2</option>
if a codec fails or gives wrong output.
</para>

<!-- ********** -->

<sect2 id="menc-feat-enc-vfw-video-codecs">
<title>Video for Windows supported codecs</title>

<para>
<informaltable frame="all">
<tgroup cols="4">
<thead>
<row>
  <entry>Video codec file name</entry>
  <entry>Description (FourCC)</entry>
  <entry>md5sum</entry>
  <entry>Comment</entry>
</row>
</thead>
<tbody>
<row>
  <entry>aslcodec_vfw.dll</entry>
  <entry>Alparysoft lossless codec vfw (ASLC)</entry>
  <entry>608af234a6ea4d90cdc7246af5f3f29a</entry>
  <entry></entry>
</row>
<row>
  <entry>avimszh.dll</entry>
  <entry>AVImszh (MSZH)</entry>
  <entry>253118fe1eedea04a95ed6e5f4c28878</entry>
  <entry>needs <option>-vf format</option></entry>
</row>
<row>
  <entry>avizlib.dll</entry>
  <entry>AVIzlib (ZLIB)</entry>
  <entry>2f1cc76bbcf6d77d40d0e23392fa8eda</entry>
  <entry></entry>
</row>
<row>
  <entry>divx.dll</entry>
  <entry>DivX4Windows-VFW</entry>
  <entry>acf35b2fc004a89c829531555d73f1e6</entry>
  <entry></entry>
</row>
<row>
  <entry>huffyuv.dll</entry>
  <entry>HuffYUV (lossless) (HFYU)</entry>
  <entry>b74695b50230be4a6ef2c4293a58ac3b</entry>
  <entry></entry>
</row>
<row>
  <entry>iccvid.dll</entry>
  <entry>Cinepak Video (cvid)</entry>
  <entry>cb3b7ee47ba7dbb3d23d34e274895133</entry>
  <entry></entry>
</row>
<row>
  <entry>icmw_32.dll</entry>
  <entry>Motion Wavelets (MWV1)</entry>
  <entry>c9618a8fc73ce219ba918e3e09e227f2</entry>
  <entry></entry>
</row>
<row>
  <entry>jp2avi.dll</entry>
  <entry>ImagePower MJPEG2000 (IPJ2)</entry>
  <entry>d860a11766da0d0ea064672c6833768b</entry>
  <entry><option>-vf flip</option></entry>
</row>
<row>
  <entry>m3jp2k32.dll</entry>
  <entry>Morgan MJPEG2000 (MJ2C)</entry>
  <entry>f3c174edcbaef7cb947d6357cdfde7ff</entry>
  <entry></entry>
</row>
<row>
  <entry>m3jpeg32.dll</entry>
  <entry>Morgan Motion JPEG Codec (MJPEG)</entry>
  <entry>1cd13fff5960aa2aae43790242c323b1</entry>
  <entry></entry>
</row>
<row>
  <entry>mpg4c32.dll</entry>
  <entry>Microsoft MPEG-4 v1/v2</entry>
  <entry>b5791ea23f33010d37ab8314681f1256</entry>
  <entry></entry>
</row>
<row>
  <entry>tsccvid.dll</entry>
  <entry>TechSmith Camtasia Screen Codec (TSCC)</entry>
  <entry>8230d8560c41d444f249802a2700d1d5</entry>
  <entry>shareware error on windows</entry>
</row>
<row>
  <entry>vp31vfw.dll</entry>
  <entry>On2 Open Source VP3 Codec (VP31)</entry>
  <entry>845f3590ea489e2e45e876ab107ee7d2</entry>
  <entry></entry>
</row>
<row>
  <entry>vp4vfw.dll</entry>
  <entry>On2 VP4 Personal Codec (VP40)</entry>
  <entry>fc5480a482ccc594c2898dcc4188b58f</entry>
  <entry></entry>
</row>
<row>
  <entry>vp6vfw.dll</entry>
  <entry>On2 VP6 Personal Codec (VP60)</entry>
  <entry>04d635a364243013898fd09484f913fb</entry>
  <entry></entry>
</row>
<row>
  <entry>vp7vfw.dll</entry>
  <entry>On2 VP7 Personal Codec (VP70)</entry>
  <entry>cb4cc3d4ea7c94a35f1d81c3d750bc8d</entry>
  <entry><option>-ffourcc VP70</option></entry>
</row>
<row>
  <entry>ViVD2.dll</entry>
  <entry>SoftMedia ViVD V2 codec VfW (GXVE)</entry>
  <entry>a7b4bf5cac630bb9262c3f80d8a773a1</entry>
  <entry></entry>
</row>
<row>
  <entry>msulvc06.DLL</entry>
  <entry>MSU Lossless codec (MSUD)</entry>
  <entry>294bf9288f2f127bb86f00bfcc9ccdda</entry>
  <entry>
  Decodable by <application>Window Media Player</application>,
  not <application>MPlayer</application> (yet).
  </entry>
</row>
<row>
  <entry>camcodec.dll</entry>
  <entry>CamStudio lossless video codec (CSCD)</entry>
  <entry>0efe97ce08bb0e40162ab15ef3b45615</entry>
  <entry>sf.net/projects/camstudio</entry>
</row>
</tbody>
</tgroup>
</informaltable>

The first column contains the codec names that should be passed after the
<literal>codec</literal> parameter,
like: <option>-xvfwopts codec=divx.dll</option>
The FourCC code used by each codec is given in the parentheses.
</para>

<informalexample>
<para>
An example to convert an ISO DVD trailer to a VP6 flash video file
using compdata bitrate settings:
<screen>
mencoder -dvd-device <replaceable>zeiram.iso</replaceable> dvd://7 -o <replaceable>trailer.flv</replaceable> \
-ovc vfw -xvfwopts codec=vp6vfw.dll:compdata=onepass.mcf -oac mp3lame \
-lameopts cbr:br=64 -af lavcresample=22050 -vf yadif,scale=320:240,flip \
-of lavf
</screen>
</para>
</informalexample>
</sect2>

<sect2 id="menc-feat-video-for-windows-bitrate-settings">
<title>Using vfw2menc to create a codec settings file.</title>

<para>
To encode with the Video for Windows codecs, you will need to set bitrate
and other options. This is known to work on x86 on both *NIX and Windows.
</para>
<para>
First you must build the <application>vfw2menc</application> program.
It is located in the <filename class="directory">TOOLS</filename> subdirectory
of the MPlayer source tree.
To build on Linux, this can be done using <application>Wine</application>:
<screen>winegcc vfw2menc.c -o vfw2menc -lwinmm -lole32</screen>

To build on Windows in <application>MinGW</application> or
<application>Cygwin</application> use:
<screen>gcc vfw2menc.c -o vfw2menc.exe -lwinmm -lole32</screen>

To build on <application>MSVC</application> you will need getopt.
Getopt can be found in the original <application>vfw2menc</application>
archive available at:
The <ulink url="http://oss.netfarm.it/mplayer-win32.php">MPlayer on win32</ulink> project.
</para>
<informalexample>
<para>
Below is an example with the VP6 codec.
<screen>
vfw2menc -f VP62 -d vp6vfw.dll -s firstpass.mcf
</screen>
This will open the VP6 codec dialog window.
Repeat this step for the second pass
and use <option>-s <replaceable>secondpass.mcf</replaceable></option>.
</para>
</informalexample>
<para>
Windows users can use
<option>-xvfwopts codec=vp6vfw.dll:compdata=dialog</option> to have
the codec dialog display before encoding starts.
</para>
</sect2>
</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-quicktime-7">
<title>Using <application>MEncoder</application> to create
<application>QuickTime</application>-compatible files</title>


<sect2 id="menc-feat-quicktime-7-why-use-it">
<title>Why would one want to produce <application>QuickTime</application>-compatible Files?</title>

<para>
  There are several reasons why producing
  <application>QuickTime</application>-compatible files can be desirable.
</para>
<itemizedlist>
<listitem><para>
  You want any computer illiterate to be able to watch your encode on
  any major platform (Windows, Mac OS X, Unices &hellip;).
</para></listitem>
<listitem><para>
  <application>QuickTime</application> is able to take advantage of more
  hardware and software acceleration features of Mac OS X than
  platform-independent players like <application>MPlayer</application>
  or <application>VLC</application>.
  That means that your encodes have a chance to be played smoothly by older
  G4-powered machines.
</para></listitem>
<listitem><para>
  <application>QuickTime</application> 7 supports the next-generation codec H.264,
  which yields significantly better picture quality than previous codec
  generations (MPEG-2, MPEG-4 &hellip;).
</para></listitem>
</itemizedlist>
</sect2>

<sect2 id="menc-feat-quicktime-7-constraints">
<title><application>QuickTime</application> 7 limitations</title>

<para>
  <application>QuickTime</application> 7 supports H.264 video and AAC audio,
  but it does not support them muxed in the AVI container format.
  However, you can use <application>MEncoder</application> to encode
  the video and audio, and then use an external program such as
  <application>mp4creator</application> (part of the
  <ulink url="http://mpeg4ip.sourceforge.net/">MPEG4IP suite</ulink>)
  to remux the video and audio tracks into an MP4 container.
</para>

<para>
  <application>QuickTime</application>'s support for H.264 is limited,
  so you will need to drop some advanced features.
  If you encode your video with features that
  <application>QuickTime</application> 7 does not support,
  <application>QuickTime</application>-based players will show you a pretty
  white screen instead of your expected video.
</para>

<itemizedlist>
<listitem><para>
  <emphasis role="bold">B-frames</emphasis>:
  <application>QuickTime</application> 7 supports a maximum of 1 B-frame, i.e.
  <option>-x264encopts bframes=1</option>. This means that
  <option>b_pyramid</option> and <option>weight_b</option> will have no
  effect, since they require <option>bframes</option> to be greater than 1.
</para></listitem>
<listitem><para>
  <emphasis role="bold">Macroblocks</emphasis>:
  <application>QuickTime</application> 7 does not support 8x8 DCT macroblocks.
  This option (<option>8x8dct</option>) is off by default, so just be sure
  not to explicitly enable it. This also means that the <option>i8x8</option>
  option will have no effect, since it requires <option>8x8dct</option>.
</para></listitem>
<listitem><para>
  <emphasis role="bold">Aspect ratio</emphasis>:
  <application>QuickTime</application> 7 does not support SAR (sample
  aspect ratio) information in MPEG-4 files; it assumes that SAR=1. Read
  <link linkend="menc-feat-quicktime-7-scale">the section on scaling</link>
  for a workaround. <application>QuickTime</application> X no longer has this
  limitation.
</para></listitem>
</itemizedlist>

</sect2>

<sect2 id="menc-feat-quicktime-7-crop">
<title>Cropping</title>
<para>
  Suppose you want to rip your freshly bought copy of "The Chronicles of
  Narnia". Your DVD is region 1,
  which means it is NTSC. The example below would still apply to PAL,
  except you would omit <option>-ofps 24000/1001</option> and use slightly
  different <option>crop</option> and <option>scale</option> dimensions.
</para>

<para>
  After running <option>mplayer dvd://1</option>, you follow the process
  detailed in the section <link linkend="menc-feat-telecine">How to deal
  with telecine and interlacing in NTSC DVDs</link> and discover that it is
  24000/1001 fps progressive video. This simplifies the process somewhat,
  since you do not need to use an inverse telecine filter such as
  <option>pullup</option> or a deinterlacing filter such as
  <option>yadif</option>.
</para>

<para>
  Next, you need to crop out the black bars from the top and bottom of the
  video, as detailed in <link linkend="menc-feat-dvd-mpeg4-example-crop">this</link>
  previous section.
</para>

</sect2>

<sect2 id="menc-feat-quicktime-7-scale">
<title>Scaling</title>

<para>
  The next step is truly heartbreaking.
  <application>QuickTime</application> 7 does not support MPEG-4 videos
  with a sample aspect ratio other than 1, so you will need to upscale
  (which wastes a lot of disk space) or downscale (which loses some
  details of the source) the video to square pixels.
  Either way you do it, this is highly inefficient, but simply cannot
  be avoided if you want your video to be playable by
  <application>QuickTime</application> 7.
  <application>MEncoder</application> can apply the appropriate upscaling
  or downscaling by specifying respectively <option>-vf scale=-10:-1</option>
  or <option>-vf scale=-1:-10</option>.
  This will scale your video to the correct width for the cropped height,
  rounded to the closest multiple of 16 for optimal compression.
  Remember that if you are cropping, you should crop first, then scale:

  <screen>-vf crop=720:352:0:62,scale=-10:-1</screen>
</para>

</sect2>

<sect2 id="menc-feat-quicktime-7-avsync">
<title>A/V sync</title>

<para>
  Because you will be remuxing into a different container, you should
  always use the <option>harddup</option> option to ensure that duplicated
  frames are actually duplicated in the video output. Without this option,
  <application>MEncoder</application> will simply put a marker in the video
  stream that a frame was duplicated, and rely on the client software to
  show the same frame twice. Unfortunately, this "soft duplication" does
  not survive remuxing, so the audio would slowly lose sync with the video.
</para>

<para>
  The final filter chain looks like this:
  <screen>-vf crop=720:352:0:62,scale=-10:-1,harddup</screen>
</para>

</sect2>

<sect2 id="menc-feat-quicktime-7-bitrate">
<title>Bitrate</title>

<para>
  As always, the selection of bitrate is a matter of the technical properties
  of the source, as explained
  <link linkend="menc-feat-dvd-mpeg4-resolution-bitrate">here</link>, as
  well as a matter of taste.
  This movie has a fair bit of action and lots of detail, but H.264 video
  looks good at much lower bitrates than XviD or other MPEG-4 codecs.
  After much experimentation, the author of this guide chose to encode
  this movie at 900kbps, and thought that it looked very good.
  You may decrease bitrate if you need to save more space, or increase
  it if you need to improve quality.
</para>

</sect2>

<sect2 id="menc-feat-quicktime-7-example">
<title>Encoding example</title>

<para>
  You are now ready to encode the video. Since you care about
  quality, of course you will be doing a two-pass encode. To shave off
  some encoding time, you can specify the <option>turbo</option> option
  on the first pass; this reduces <option>subq</option> and
  <option>frameref</option> to 1. To save some disk space, you can
  use the <option>ss</option> option to strip off the first few seconds
  of the video. (I found that this particular movie has 32 seconds of
  credits and logos.)  <option>bframes</option> can be 0 or 1.
  The other options are documented in <link
  linkend="menc-feat-x264-encoding-options-speedvquality">Encoding with
  the <systemitem class="library">x264</systemitem> codec</link> and
  the man page.

  <screen>mencoder dvd://1 -o /dev/null -ss 32 -ovc x264 \
-x264encopts pass=1:turbo:bitrate=900:bframes=1:\
me=umh:partitions=all:trellis=1:qp_step=4:qcomp=0.7:direct_pred=auto:keyint=300 \
-vf crop=720:352:0:62,scale=-10:-1,harddup \
-oac faac -faacopts br=192:mpeg=4:object=2 -channels 2 -srate 48000 \
-ofps 24000/1001</screen>

  If you have a multi-processor machine, don't miss the opportunity to
  dramatically speed-up encoding by enabling
  <link linkend="menc-feat-x264-encoding-options-speedvquality-threads">
  <systemitem class="library">x264</systemitem>'s multi-threading mode</link>
  by adding <option>threads=auto</option> to your <option>x264encopts</option>
  command-line.
</para>

<para>
  The second pass is the same, except that you specify the output file
  and set <option>pass=2</option>.

  <screen>mencoder dvd://1 <emphasis role="bold">-o narnia.avi</emphasis> -ss 32 -ovc x264 \
-x264encopts <emphasis role="bold">pass=2</emphasis>:turbo:bitrate=900:frameref=5:bframes=1:\
me=umh:partitions=all:trellis=1:qp_step=4:qcomp=0.7:direct_pred=auto:keyint=300 \
-vf crop=720:352:0:62,scale=-10:-1,harddup \
-oac faac -faacopts br=192:mpeg=4:object=2 -channels 2 -srate 48000 \
-ofps 24000/1001</screen>
</para>

<para>
  The resulting AVI should play perfectly in
  <application>MPlayer</application>, but of course
  <application>QuickTime</application> can not play it because it does
  not support H.264 muxed in AVI.
  So the next step is to remux the video into an MP4 container.
</para>
</sect2>

<sect2 id="menc-feat-quicktime-7-remux">
<title>Remuxing as MP4</title>

<para>
  There are several ways to remux AVI files to MP4. You can use
  <application>mp4creator</application>, which is part of the
  <ulink url="http://mpeg4ip.sourceforge.net/">MPEG4IP suite</ulink>.
</para>

<para>
  First, demux the AVI into separate audio and video streams using
  <application>MPlayer</application>.

  <screen>mplayer narnia.avi -dumpaudio -dumpfile narnia.aac
mplayer narnia.avi -dumpvideo -dumpfile narnia.h264</screen>

  The file names are important; <application>mp4creator</application>
  requires that AAC audio streams be named <systemitem>.aac</systemitem>
  and H.264 video streams be named <systemitem>.h264</systemitem>.
</para>

<para>
  Now use <application>mp4creator</application> to create a new
  MP4 file out of the audio and video streams.

  <screen>mp4creator -create=narnia.aac narnia.mp4
mp4creator -create=narnia.h264 -rate=23.976 narnia.mp4</screen>

  Unlike the encoding step, you must specify the framerate as a
  decimal (such as 23.976), not a fraction (such as 24000/1001).
</para>

<para>
  This <systemitem>narnia.mp4</systemitem> file should now be playable
  with any <application>QuickTime</application> 7 application, such as
  <application>QuickTime Player</application> or
  <application>iTunes</application>. If you are planning to view the
  video in a web browser with the <application>QuickTime</application>
  plugin, you should also hint the movie so that the
  <application>QuickTime</application> plugin can start playing it
  while it is still downloading.  <application>mp4creator</application>
  can create these hint tracks:

  <screen>mp4creator -hint=1 narnia.mp4
mp4creator -hint=2 narnia.mp4
mp4creator -optimize narnia.mp4</screen>

  You can check the final result to ensure that the hint tracks were
  created successfully:

  <screen>mp4creator -list narnia.mp4</screen>

  You should see a list of tracks: 1 audio, 1 video, and 2 hint tracks.

<screen>Track   Type    Info
1       audio   MPEG-4 AAC LC, 8548.714 secs, 190 kbps, 48000 Hz
2       video   H264 Main@5.1, 8549.132 secs, 899 kbps, 848x352 @ 23.976001 fps
3       hint    Payload mpeg4-generic for track 1
4       hint    Payload H264 for track 2
</screen>
</para>

</sect2>

<sect2 id="menc-feat-quicktime-7-metadata">
<title>Adding metadata tags</title>

<para>
  If you want to add tags to your video that show up in iTunes, you can use
  <ulink url="http://atomicparsley.sourceforge.net/">AtomicParsley</ulink>.

  <screen>AtomicParsley narnia.mp4 --metaEnema --title "The Chronicles of Narnia" --year 2005 --stik Movie --freefree --overWrite</screen>

  The <option>--metaEnema</option> option removes any existing metadata
  (<application>mp4creator</application> inserts its name in the
  "encoding tool" tag), and <option>--freefree</option> reclaims the
  space from the deleted metadata.
  The <option>--stik</option> option sets the type of video (such as Movie
  or TV Show), which iTunes uses to group related video files.
  The <option>--overWrite</option> option overwrites the original file;
  without it, <application>AtomicParsley</application> creates a new
  auto-named file in the same directory and leaves the original file
  untouched.
</para>

</sect2>

</sect1>


<!-- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -->


<sect1 id="menc-feat-vcd-dvd">
<title>Using <application>MEncoder</application>
  to create VCD/SVCD/DVD-compliant files</title>

<sect2 id="menc-feat-vcd-dvd-constraints">
<title>Format Constraints</title>

<para>
<application>MEncoder</application> is capable of creating VCD, SCVD
and DVD format MPEG files using the
<systemitem class="library">libavcodec</systemitem> library.
These files can then be used in conjunction with
<ulink url="http://www.gnu.org/software/vcdimager/vcdimager.html">vcdimager</ulink>
or
<ulink url="http://dvdauthor.sourceforge.net/">dvdauthor</ulink>
to create discs that will play on a standard set-top player.
</para>

<para>
The DVD, SVCD, and VCD formats are subject to heavy constraints.
Only a small selection of encoded picture sizes and aspect ratios are
available.
If your movie does not already meet these requirements, you may have
to scale, crop or add black borders to the picture to make it
compliant.
</para>


<sect3 id="menc-feat-vcd-dvd-constraints-resolution">
<title>Format Constraints</title>

<informaltable frame="all">
<tgroup cols="9">
<thead>
<row>
  <entry>Format</entry>
  <entry>Resolution</entry>
  <entry>V. Codec</entry>
  <entry>V. Bitrate</entry>
  <entry>Sample Rate</entry>
  <entry>A. Codec</entry>
  <entry>A. Bitrate</entry>
  <entry>FPS</entry>
  <entry>Aspect</entry>
</row>
</thead>
<tbody>
<row>
  <entry>NTSC DVD</entry>
  <entry>720x480, 704x480, 352x480, 352x240</entry>
  <entry>MPEG-2</entry>
  <entry>9800 kbps</entry>
  <entry>48000 Hz</entry>
  <entry>AC-3,PCM</entry>
  <entry>1536 kbps (max)</entry>
  <entry>30000/1001, 24000/1001</entry>
  <entry>4:3, 16:9 (only for 720x480)</entry>
</row>
<row>
  <entry>NTSC DVD</entry>
  <entry>352x240<footnote id='fn-rare-resolutions'><para>
  These resolutions are rarely used for DVDs because
  they are fairly low quality.</para></footnote></entry>
  <entry>MPEG-1</entry>
  <entry>1856 kbps</entry>
  <entry>48000 Hz</entry>
  <entry>AC-3,PCM</entry>
  <entry>1536 kbps (max)</entry>
  <entry>30000/1001, 24000/1001</entry>
  <entry>4:3, 16:9</entry>
</row>
<row>
  <entry>NTSC SVCD</entry>
  <entry>480x480</entry>
  <entry>MPEG-2</entry>
  <entry>2600 kbps</entry>
  <entry>44100 Hz</entry>
  <entry>MP2</entry>
  <entry>384 kbps (max)</entry>
  <entry>30000/1001</entry>
  <entry>4:3</entry>
</row>
<row>
  <entry>NTSC VCD</entry>
  <entry>352x240</entry>
  <entry>MPEG-1</entry>
  <entry>1150 kbps</entry>
  <entry>44100 Hz</entry>
  <entry>MP2</entry>
  <entry>224 kbps</entry>
  <entry>24000/1001, 30000/1001</entry>
  <entry>4:3</entry>
</row>
<row>
  <entry>PAL DVD</entry>
  <entry>720x576, 704x576, 352x576, 352x288</entry>
  <entry>MPEG-2</entry>
  <entry>9800 kbps</entry>
  <entry>48000 Hz</entry>
  <entry>MP2,AC-3,PCM</entry>
  <entry>1536 kbps (max)</entry>
  <entry>25</entry>
  <entry>4:3, 16:9 (only for 720x576)</entry>
</row>
<row>
  <entry>PAL DVD</entry>
  <entry>352x288<footnoteref linkend='fn-rare-resolutions'/></entry>
  <entry>MPEG-1</entry>
  <entry>1856 kbps</entry>
  <entry>48000 Hz</entry>
  <entry>MP2,AC-3,PCM</entry>
  <entry>1536 kbps (max)</entry>
  <entry>25</entry>
  <entry>4:3, 16:9</entry>
</row>
<row>
  <entry>PAL SVCD</entry>
  <entry>480x576</entry>
  <entry>MPEG-2</entry>
  <entry>2600 kbps</entry>
  <entry>44100 Hz</entry>
  <entry>MP2</entry>
  <entry>384 kbps (max)</entry>
  <entry>25</entry>
  <entry>4:3</entry>
</row>
<row>
  <entry>PAL VCD</entry>
  <entry>352x288</entry>
  <entry>MPEG-1</entry>
  <entry>1152 kbps</entry>
  <entry>44100 Hz</entry>
  <entry>MP2</entry>
  <entry>224 kbps</entry>
  <entry>25</entry>
  <entry>4:3</entry>
</row>
</tbody>
</tgroup>
</informaltable>

<para>
If your movie has 2.35:1 aspect (most recent action movies), you will
have to add black borders or crop the movie down to 16:9 to make a DVD or VCD.
If you add black borders, try to align them at 16-pixel boundaries in
order to minimize the impact on encoding performance.
Thankfully DVD has sufficiently excessive bitrate that you do not have
to worry too much about encoding efficiency, but SVCD and VCD are
highly bitrate-starved and require effort to obtain acceptable quality.
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-constraints-gop">
<title>GOP Size Constraints</title>

<para>
DVD, VCD, and SVCD also constrain you to relatively low
GOP (Group of Pictures) sizes.
For 30 fps material the largest allowed GOP size is 18.
For 25 or 24 fps, the maximum is 15.
The GOP size is set using the <option>keyint</option> option.
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-constraints-bitrate">
<title>Bitrate Constraints</title>

<para>
VCD video is required to be CBR at 1152 kbps.
This highly limiting constraint also comes along with an extremely low vbv
buffer size of 327 kilobits.
SVCD allows varying video bitrates up to 2500 kbps, and a somewhat less
restrictive vbv buffer size of 917 kilobits is allowed.
DVD video bitrates may range anywhere up to 9800 kbps (though typical
bitrates are about half that), and the vbv buffer size is 1835 kilobits.
</para>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-vcd-dvd-output">
<title>Output Options</title>

<para>
<application>MEncoder</application> has options to control the output
format.
Using these options we can instruct it to create the correct type of
file.
</para>

<para>
The options for VCD and SVCD are called xvcd and xsvcd, because they
are extended formats.
They are not strictly compliant, mainly because the output does not
contain scan offsets.
If you need to generate an SVCD image, you should pass the output file to
<ulink url="http://www.gnu.org/software/vcdimager/vcdimager.html">vcdimager</ulink>.
</para>

<para>
VCD:
<screen>-of mpeg -mpegopts format=xvcd</screen>
</para>

<para>
SVCD:
<screen>-of mpeg -mpegopts format=xsvcd</screen>
</para>

<para>
DVD (with timestamps on every frame, if possible):
<screen>-of mpeg -mpegopts format=dvd:tsaf</screen>
</para>

<para>
DVD with NTSC Pullup:
<screen>-of mpeg -mpegopts format=dvd:tsaf:telecine -ofps 24000/1001</screen>
This allows 24000/1001 fps progressive content to be encoded at 30000/1001
fps whilst maintaining DVD-compliance.
</para>


<sect3 id="menc-feat-vcd-dvd-output-aspect">
<title>Aspect Ratio</title>

<para>
The aspect argument of <option>-lavcopts</option> is used to encode
the aspect ratio of the file.
During playback the aspect ratio is used to restore the video to the
correct size.
</para>

<para>
16:9 or "Widescreen"
<screen>-lavcopts aspect=16/9</screen>
</para>

<para>
4:3 or "Fullscreen"
<screen>-lavcopts aspect=4/3</screen>
</para>

<para>
2.35:1 or "Cinemascope" NTSC
<screen>-vf scale=720:368,expand=720:480 -lavcopts aspect=16/9</screen>
To calculate the correct scaling size, use the expanded NTSC width of
854/2.35 = 368
</para>

<para>
2.35:1 or "Cinemascope" PAL
<screen>-vf scale=720:432,expand=720:576 -lavcopts aspect=16/9</screen>
To calculate the correct scaling size, use the expanded PAL width of
1024/2.35 = 432
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-a-v-sync">
<title>Maintaining A/V sync</title>

<para>
In order to maintain audio/video synchronization throughout the encode,
<application>MEncoder</application> has to drop or duplicate frames.
This works rather well when muxing into an AVI file, but is almost
guaranteed to fail to maintain A/V sync with other muxers such as MPEG.
This is why it is necessary to append the
<option>harddup</option> video filter at the end of the filter chain
to avoid this kind of problem.
You can find more technical information about <option>harddup</option>
in the section
<link linkend="menc-feat-dvd-mpeg4-muxing-filter-issues">Improving muxing and A/V sync reliability</link>
or in the manual page.
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-output-srate">
<title>Sample Rate Conversion</title>

<para>
If the audio sample rate in the original file is not the same as
required by the target format, sample rate conversion is required.
This is achieved using the <option>-srate</option> option and
the <option>-af lavcresample</option> audio filter together.
</para>

<para>
DVD:
<screen>-srate 48000 -af lavcresample=48000</screen>
</para>

<para>
VCD and SVCD:
<screen>-srate 44100 -af lavcresample=44100</screen>
</para>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-vcd-dvd-lavc">
<title>Using libavcodec for VCD/SVCD/DVD Encoding</title>

<sect3 id="menc-feat-vcd-dvd-lavc-intro">
<title>Introduction</title>

<para>
<systemitem class="library">libavcodec</systemitem> can be used to
create VCD/SVCD/DVD compliant video by using the appropriate options.
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-lavc-options">
<title>lavcopts</title>

<para>
This is a list of fields in <option>-lavcopts</option> that you may
be required to change in order to make a complaint movie for VCD, SVCD,
or DVD:
</para>

<itemizedlist>
<listitem><para>
  <emphasis role="bold">acodec</emphasis>:
  <option>mp2</option> for VCD, SVCD, or PAL DVD;
  <option>ac3</option> is most commonly used for DVD.
  PCM audio may also be used for DVD, but this is mostly a big waste of
  space.
  Note that MP3 audio is not compliant for any of these formats, but
  players often have no problem playing it anyway.
</para></listitem>
<listitem><para>
  <emphasis role="bold">abitrate</emphasis>:
  224 for VCD; up to 384 for SVCD; up to 1536 for  DVD, but commonly
  used values range from 192 kbps for stereo to 384 kbps for 5.1 channel
  sound.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vcodec</emphasis>:
  <option>mpeg1video</option> for VCD;
  <option>mpeg2video</option> for SVCD;
  <option>mpeg2video</option> is usually used for DVD but you may also use
  <option>mpeg1video</option> for CIF resolutions.
</para></listitem>
<listitem><para>
  <emphasis role="bold">keyint</emphasis>:
  Used to set the GOP size.
  18 for 30fps material, or 15 for 25/24 fps material.
  Commercial producers seem to prefer keyframe intervals of 12.
  It is possible to make this much larger and still retain compatibility
  with most players.
  A <option>keyint</option> of 25 should never cause any problems.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vrc_buf_size</emphasis>:
  327 for VCD, 917 for SVCD, and 1835 for DVD.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vrc_minrate</emphasis>:
  1152, for VCD. May be left alone for SVCD and DVD.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vrc_maxrate</emphasis>:
  1152 for VCD; 2500 for SVCD; 9800 for DVD.
  For SVCD and DVD, you might wish to use lower values depending on your
  own personal preferences and requirements.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vbitrate</emphasis>:
  1152 for VCD;
  up to 2500 for SVCD;
  up to 9800 for DVD.
  For the latter two formats, vbitrate should be set based on personal
  preference.
  For instance, if you insist on fitting 20 or so hours on a DVD, you
  could use vbitrate=400.
  The resulting video quality would probably be quite bad.
  If you are trying to squeeze out the maximum possible quality on a DVD,
  use vbitrate=9800, but be warned that this could constrain you to less
  than an hour of video on a single-layer DVD.
</para></listitem>
<listitem><para>
  <emphasis role="bold">vstrict</emphasis>:
  <option>vstrict</option>=0 should be used to create DVDs.
  Without this option, <application>MEncoder</application> creates a
  stream that cannot be correctly decoded by some standalone DVD
  players.
</para></listitem>
</itemizedlist>
</sect3>


<sect3 id="menc-feat-vcd-dvd-lavc-examples">
<title>Examples</title>

<para>
This is a typical minimum set of <option>-lavcopts</option> for
encoding video:
</para>
<para>
VCD:
<screen>
-lavcopts vcodec=mpeg1video:vrc_buf_size=327:vrc_minrate=1152:\
vrc_maxrate=1152:vbitrate=1152:keyint=15:acodec=mp2
</screen>
</para>

<para>
SVCD:
<screen>
-lavcopts vcodec=mpeg2video:vrc_buf_size=917:vrc_maxrate=2500:vbitrate=1800:\
keyint=15:acodec=mp2
</screen>
</para>

<para>
DVD:
<screen>
-lavcopts vcodec=mpeg2video:vrc_buf_size=1835:vrc_maxrate=9800:vbitrate=5000:\
keyint=15:vstrict=0:acodec=ac3
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-lavc-advanced">
<title>Advanced Options</title>

<para>
For higher quality encoding, you may also wish to add quality-enhancing
options to lavcopts, such as <option>trell</option>,
<option>mbd=2</option>, and others.
Note that <option>qpel</option> and <option>v4mv</option>, while often
useful with MPEG-4, are not usable with MPEG-1 or MPEG-2.
Also, if you are trying to make a very high quality DVD encode, it may
be useful to add <option>dc=10</option> to lavcopts.
Doing so may help reduce the appearance of blocks in flat-colored areas.
Putting it all together, this is an example of a set of lavcopts for a
higher quality DVD:
</para>

<para>
<screen>
-lavcopts vcodec=mpeg2video:vrc_buf_size=1835:vrc_maxrate=9800:vbitrate=8000:\
keyint=15:trell:mbd=2:precmp=2:subcmp=2:cmp=2:dia=-10:predia=-10:cbp:mv0:\
vqmin=1:lmin=1:dc=10:vstrict=0
</screen>
</para>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-vcd-dvd-audio">
<title>Encoding Audio</title>

<para>
VCD and SVCD support MPEG-1 layer II audio, using one of
<systemitem class="library">toolame</systemitem>,
<systemitem class="library">twolame</systemitem>,
or <systemitem class="library">libavcodec</systemitem>'s MP2 encoder.
The libavcodec MP2 is far from being as good as the other two libraries,
however it should always be available to use.
VCD only supports constant bitrate audio (CBR) whereas SVCD supports
variable bitrate (VBR), too.
Be careful when using VBR because some bad standalone players might not
support it too well.
</para>

<para>
For DVD audio, <systemitem class="library">libavcodec</systemitem>'s
AC-3 codec is used.
</para>


<sect3 id="menc-feat-vcd-dvd-audio-toolame">
<title>toolame</title>

<para>
For VCD and SVCD:
<screen>-oac toolame -toolameopts br=224</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-audio-twolame">
<title>twolame</title>

<para>
For VCD and SVCD:
<screen>-oac twolame -twolameopts br=224</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-audio-lavc">
<title>libavcodec</title>

<para>
For DVD with 2 channel sound:
<screen>-oac lavc -lavcopts acodec=ac3:abitrate=192</screen>
</para>

<para>
For DVD with 5.1 channel sound:
<screen>-channels 6 -oac lavc -lavcopts acodec=ac3:abitrate=384</screen>
</para>

<para>
For VCD and SVCD:
<screen>-oac lavc -lavcopts acodec=mp2:abitrate=224</screen>
</para>
</sect3>
</sect2>

<!-- ********** -->

<sect2 id="menc-feat-vcd-dvd-all">
<title>Putting it all Together</title>

<para>
This section shows some complete commands for creating VCD/SVCD/DVD
compliant videos.
</para>


<sect3 id="menc-feat-vcd-dvd-all-pal-dvd">
<title>PAL DVD</title>

<para>
<screen>
mencoder -oac lavc -ovc lavc -of mpeg -mpegopts format=dvd:tsaf \
  -vf scale=720:576,harddup -srate 48000 -af lavcresample=48000 \
  -lavcopts vcodec=mpeg2video:vrc_buf_size=1835:vrc_maxrate=9800:vbitrate=5000:\
keyint=15:vstrict=0:acodec=ac3:abitrate=192:aspect=16/9 -ofps 25 \
  -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-ntsc-dvd">
<title>NTSC DVD</title>

<para>
<screen>
mencoder -oac lavc -ovc lavc -of mpeg -mpegopts format=dvd:tsaf \
  -vf scale=720:480,harddup -srate 48000 -af lavcresample=48000 \
  -lavcopts vcodec=mpeg2video:vrc_buf_size=1835:vrc_maxrate=9800:vbitrate=5000:\
keyint=18:vstrict=0:acodec=ac3:abitrate=192:aspect=16/9 -ofps 30000/1001 \
  -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-pal-ac3-copy">
<title>PAL AVI Containing AC-3 Audio to DVD</title>

<para>
If the source already has AC-3 audio, use -oac copy instead of re-encoding it.
<screen>
mencoder -oac copy -ovc lavc -of mpeg -mpegopts format=dvd:tsaf \
  -vf scale=720:576,harddup -ofps 25 \
  -lavcopts vcodec=mpeg2video:vrc_buf_size=1835:vrc_maxrate=9800:vbitrate=5000:\
keyint=15:vstrict=0:aspect=16/9 -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-ntsc-ac3-copy">
<title>NTSC AVI Containing AC-3 Audio to DVD</title>

<para>
If the source already has AC-3 audio, and is NTSC @ 24000/1001 fps:
<screen>
mencoder -oac copy -ovc lavc -of mpeg -mpegopts format=dvd:tsaf:telecine \
  -vf scale=720:480,harddup -lavcopts vcodec=mpeg2video:vrc_buf_size=1835:\
  vrc_maxrate=9800:vbitrate=5000:keyint=15:vstrict=0:aspect=16/9 -ofps 24000/1001 \
  -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-pal-svcd">
<title>PAL SVCD</title>

<para>
<screen>
mencoder -oac lavc -ovc lavc -of mpeg -mpegopts format=xsvcd -vf \
    scale=480:576,harddup -srate 44100 -af lavcresample=44100 -lavcopts \
    vcodec=mpeg2video:mbd=2:keyint=15:vrc_buf_size=917:vrc_minrate=600:\
vbitrate=2500:vrc_maxrate=2500:acodec=mp2:abitrate=224:aspect=16/9 -ofps 25 \
    -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
  </screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-ntsc-svcd">
<title>NTSC SVCD</title>

<para>
<screen>
mencoder -oac lavc -ovc lavc -of mpeg -mpegopts format=xsvcd  -vf \
    scale=480:480,harddup -srate 44100 -af lavcresample=44100 -lavcopts \
    vcodec=mpeg2video:mbd=2:keyint=18:vrc_buf_size=917:vrc_minrate=600:\
vbitrate=2500:vrc_maxrate=2500:acodec=mp2:abitrate=224:aspect=16/9 -ofps 30000/1001 \
    -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-pal-vcd">
<title>PAL VCD</title>

<para>
<screen>
mencoder -oac lavc -ovc lavc -of mpeg -mpegopts format=xvcd -vf \
    scale=352:288,harddup -srate 44100 -af lavcresample=44100 -lavcopts \
    vcodec=mpeg1video:keyint=15:vrc_buf_size=327:vrc_minrate=1152:\
vbitrate=1152:vrc_maxrate=1152:acodec=mp2:abitrate=224:aspect=16/9 -ofps 25 \
    -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>


<sect3 id="menc-feat-vcd-dvd-all-ntsc-vcd">
<title>NTSC VCD</title>

<para>
<screen>
mencoder -oac lavc -ovc lavc -of mpeg -mpegopts format=xvcd -vf \
    scale=352:240,harddup -srate 44100 -af lavcresample=44100 -lavcopts \
    vcodec=mpeg1video:keyint=18:vrc_buf_size=327:vrc_minrate=1152:\
vbitrate=1152:vrc_maxrate=1152:acodec=mp2:abitrate=224:aspect=16/9 -ofps 30000/1001 \
    -o <replaceable>movie.mpg</replaceable> <replaceable>movie.avi</replaceable>
</screen>
</para>
</sect3>
</sect2>
</sect1>
</chapter>
