### 2.3.1 Video output devices

#### 2.3.1.1 Setting up MTRR

It is VERY recommended to check if the MTRR registers are set up properly, because they can give a big performance boost.

Do a '`cat /proc/mtrr`':

`--($:~)-- cat /proc/mtrr
reg00: base=0xe4000000 (3648MB), size= 16MB: write-combining, count=9
reg01: base=0xd8000000 (3456MB), size= 128MB: write-combining, count=1`

It's right, shows my Matrox G400 with 16MB memory. I did this from XFree 4.x.x , which sets up MTRR registers automatically.

If nothing worked, you have to do it manually. First, you have to find the base address. You have 3 ways to find it:

- from X11 startup messages, for example:

  `(--) SVGA: PCI: Matrox MGA G400 AGP rev 4, Memory @ 0xd8000000, 0xd4000000
  (--) SVGA: Linear framebuffer at 0xD8000000`

- from /proc/pci (use lspci -v command):

  `01:00.0 VGA compatible controller: Matrox Graphics, Inc.: Unknown device 0525` `Memory at d8000000 (32-bit, prefetchable)`

- from mga_vid kernel driver messages (use dmesg):

  `mga_mem_base = d8000000`

Then let's find the memory size. This is very easy, just convert video ram size to hexadecimal, or use this table:

| 1 MB |  | 0x100000
| 2 MB |  | 0x200000
| 4 MB |  | 0x400000
| 8 MB |  | 0x800000
| 16 MB |  | 0x1000000
| 32 MB |  | 0x2000000

You know base address and memory size, let's setup MTRR registers! For example, for the Matrox card above (base=0xd8000000) with 32MB ram (size=0x2000000) just execute:

`echo "base=0xd8000000 size=0x2000000 type=write-combining" >| /proc/mtrr`

Not all CPUs support MTRRs. For example older K6-2's [around 266MHz, stepping 0] doesn't support MTRR, but stepping 12's do ('`cat /proc/cpuinfo`' to check it').

#### 2.3.1.2 Xv

Under XFree86 4.0.2 or newer, you can use your card's hardware YUV routines using the XVideo extension. This is what the option '-vo xv' uses. Also, this is driver supports adjusting brightness/contrast/hue/etc (unless you use the old, slow DirectShow DivX codec, which supports it everywhere), see the man page.

In order to make this work, be sure to check the following:

- You have to use XFree86 4.0.2 or newer (former versions don't have XVideo)
- Your card actually supports hardware acceleration (modern cards do)
- X loads the XVideo extension, it's something like this:

  `(II) Loading extension XVideo`

  in /var/log/XFree86.0.log

  NOTE: this loads only the XFree86's extension. In a good install, this is always loaded, and doesn't mean that the card's XVideo support is loaded!

- Your card has Xv support under Linux. To check, try 'xvinfo', it is the part of the XFree86 distribution. It should display a long text, similar to this:

      	X-Video Extension version 2.2
      	screen #0
      	  Adaptor #0: "Savage Streams Engine"
      	    number of ports: 1
      	    port base: 43
      	    operations supported: PutImage
      	    supported visuals:
      	      depth 16, visualID 0x22
      	      depth 16, visualID 0x23
      	    number of attributes: 5
      	(...)
      	    Number of image formats: 7
      	      id: 0x32595559 (YUY2)
      	        guid: 59555932-0000-0010-8000-00aa00389b71
      	        bits per pixel: 16
      	        number of planes: 1
      	        type: YUV (packed)
      	      id: 0x32315659 (YV12)
      	        guid: 59563132-0000-0010-8000-00aa00389b71
      	        bits per pixel: 12
      	        number of planes: 3
      	        type: YUV (planar)
      	(...etc...)

  It must support YUY2 packed, and YV12 planar pixel formats to be usable with MPlayer.

- And finally, check if MPlayer was compiled with 'xv' support. ./configure prints this.

##### 2.3.1.2.1 3dfx cards

Older 3dfx drivers were known to have problems with XVideo acceleration, it didn't support either YUY2 or YV12, and so. Verify that you have XFree86 version 4.2.0 or greater, it works OK with YV12 and YUY2. Previous versions, including 4.1.0, crash with YV12. If you experience strange effects using -vo xv, try SDL (it has XVideo too) and see if it helps. Check the SDL section for details.

OR, try the NEW -vo tdfxfb driver! See the tdfxfb section.

##### 2.3.1.2.2 S3 cards

S3 Savage3D's should work fine, but for Savage4, use XFree86 version 4.0.3 or greater (in case of image problems, try 16bpp). As for S3 Virge.. there is xv support, but the card itself is very slow, so you better sell it.

NOTE: Savage cards have a slow YV12 image displaying capability (it needs to do YV12 to YUY2 conversion, because the Savage hardware can't display YV12). So when this documentation says at some point "this has YV12 output use this, it's faster", it's not sure. Try this driver, it uses MMX2 for this task and is faster than the native X driver.

##### 2.3.1.2.3 nVidia cards

nVidia isn't a very good choice under Linux (according to nVidia, this is not true).. You'll have to use the binary closed-source nVidia driver, available at nVidia's web site. The standard XFree86 driver doesn't support XVideo for these cards, due to nVidia's closed sources/specifications.

As far as I know the latest XFree86 driver contains XVideo support for GeForce 2 and 3.

Riva128 cards don't have XVideo support even with the nVidia driver :( Complain to nVidia.

##### 2.3.1.2.4 ATI cards

- The GATOS driver (which you should use, unless you have Rage128 or Radeon) has VSYNC enabled by default. It means that decoding speed (!) is synced to the monitor's refresh rate. If playing seems to be slow, try disabling VSYNC somehow, or set refresh rate to n*(fps of the movie) Hz.
- Radeon VE - currently only XFree86 CVS has driver for this card, version 4.1.0 doesn't. And no TV out support. Of course with MPlayer you can happily get accelerated display, with or without TV output, and no libraries or X are needed. Read Vidix section.

##### 2.3.1.2.5 NeoMagic cards

These cards can be found in many laptops. Unfortunately, the driver in X 4.2.0 can't do Xv, but we have a modified, Xv-capable driver for you. Download from here. Driver provided by Stefan Seyfried.

To allow playback of DVD sized content change your XF86Config like this:

Section "Device"
[...]
Driver "neomagic"
Option "OverlayMem" "829440"
[...]
EndSection

##### 2.3.1.2.6 Trident cards

If you want to use xv with a trident card, provided that it doesn't work with 4.1.0, try the latest CVS of XFree or wait for XFree 4.2.0. The latest CVS adds support for fullscreen xv support with the Cyberblade XP card.

#### 2.3.1.3 DGA

##### 2.3.1.3.1 Summary

This document tries to explain in some words what DGA is in general and what the DGA video output driver for MPlayer can do (and what it can't).

##### 2.3.1.3.2 What is DGA

DGA is short for Direct Graphics Access and is a means for a program to bypass the X-Server and directly modifying the framebuffer memory. Technically spoken this happens by mapping the framebuffer memory into the memory range of your process. This is allowed by the kernel only if you have superuser privileges. You can get these either by logging in as root or by setting the SUID bit on the MPlayer executable (not recommended).

There are two versions of DGA: DGA1 is used by XFree 3.x.x and DGA2 was introduced with XFree 4.0.1.

DGA1 provides only direct framebuffer access as described above. For switching the resolution of the video signal you have to rely on the XVidMode extension.

DGA2 incorporates the features of XVidMode extension and also allows switching the depth of the display. So you may, although basically running a 32 bit depth X server, switch to a depth of 15 bits and vice versa.

However DGA has some drawbacks. It seems it is somewhat dependent on the graphics chip you use and on the implementation of the X server's video driver that controls this chip. So it does not work on every system ...

##### 2.3.1.3.3 Installing DGA support for MPlayer

First make sure X loads the DGA extension, see in /var/log/XFree86.0.log:

`(II) Loading extension XFree86-DGA`

See, XFree86 4.0.x or greater is VERY RECOMMENDED! MPlayer's DGA driver is autodetected on ./configure, or you can force it with --enable-dga.

If the driver couldn't switch to a smaller resolution, experiment with switches -vm (only with X 3.3.x), -fs, -bpp, -zoom to find a video mode that the movie fits in. There is no converter right now :(

Become root. DGA needs root access to be able to write directly to video memory. If you want to run it as user, then install MPlayer SUID root:

`chown root /usr/local/bin/mplayer
chmod 750 /usr/local/bin/mplayer
chmod +s /usr/local/bin/mplayer`

Now it works as a simple user, too.

> Warning: security risk
> This is a big security risk! Never do this on a server or on a computer that can be accessed by other people because they can gain root privileges through SUID root MPlayer.

Now use the `-vo dga` option, and there you go (hope so :))! You should also try if the `-vo sdl:dga` option works for you. It's much faster.

##### 2.3.1.3.4 Resolution switching

The DGA driver allows for switching the resolution of the output signal. This avoids the need for doing (slow) software scaling and at the same time provides a fullscreen image. Ideally it would switch to the exact resolution (except for honoring aspect ratio) of the video data, but the X server only allows switching to resolutions predefined in `/etc/X11/XF86Config` (`/etc/X11/XF86Config-4` for XFree 4.0.X respectively). Those are defined by so-called modelines and depend on the capabilities of your video hardware. The X server scans this config file on startup and disables the modelines not suitable for your hardware. You can find out which modes survive with the X11 log file. It can be found at: `/var/log/XFree86.0.log`.

See appendix A for some sample modeline definitions.

##### 2.3.1.3.5 DGA & MPlayer

DGA is used in two places with MPlayer: The SDL driver can be made to make use of it (-vo sdl:dga) and within the DGA driver (-vo dga). The above said is true for both; in the following sections I'll explain how the DGA driver for MPlayer works.

##### 2.3.1.3.6 Features of the DGA driver

The DGA driver is invoked by specifying -vo dga at the command line. The default behavior is to switch to a resolution matching the original resolution of the video as close as possible. It deliberately ignores the -vm and -fs switches (enabling of video mode switching and fullscreen) - it always tries to cover as much area of your screen as possible by switching the video mode, thus refraining to use a single additional cycle of your CPU to scale the image. If you don't like the mode it chooses you may force it to choose the mode matching closest the resolution you specify by -x and -y. By providing the -v option, the DGA driver will print, among a lot of other things, a list of all resolutions supported by your current XF86-Config file. Having DGA2 you may also force it to use a certain depth by using the -bpp option. Valid depths are 15, 16, 24 and 32. It depends on your hardware whether these depths are natively supported or if a (possibly slow) conversion has to be done.

If you should be lucky enough to have enough offscreen memory left to put a whole image there, the DGA driver will use doublebuffering, which results in much smoother movie replaying. It will tell you whether double- buffering is enabled or not.

Doublebuffering means that the next frame of your video is being drawn in some offscreen memory while the current frame is being displayed. When the next frame is ready, the graphics chip is just told the location in memory of the new frame and simply fetches the data to be displayed from there. In the meantime the other buffer in memory will be filled again with new video data.

Doublebuffering may be switched on by using the option -double and may be disabled with -nodouble. Current default option is to disable doublebuffering. When using the DGA driver, onscreen display (OSD) only works with doublebuffering enabled. However, enabling doublebuffering may result in a big speed penalty (on my K6-II+ 525 it used an additional 20% of CPU time!) depending on the implementation of DGA for your hardware.

##### 2.3.1.3.7 Speed issues

Generally spoken, DGA framebuffer access should be at least as fast as using the X11 driver with the additional benefit of getting a fullscreen image. The percentage speed values printed by MPlayer have to be interpreted with some care, as for example, with the X11 driver they do not include the time used by the X-Server needed for the actual drawing. Hook a terminal to a serial line of your box and start top to see what is really going on in your box...

Generally spoken, the speedup done by using DGA against 'normal' use of X11 highly depends on your graphics card and how well the X-Server module for it is optimized.

If you have a slow system, better use 15 or 16bit depth since they require only half the memory bandwidth of a 32 bit display.

Using a depth of 24bit is even a good idea if your card natively just supports 32 bit depth since it transfers 25% less data compared to the 32/32 mode.

I've seen some AVI files already be replayed on a Pentium MMX 266. AMD K6-2 CPUs might work at 400 MHZ and above.

##### 2.3.1.3.8 Known bugs

Well, according to some developers of XFree, DGA is quite a beast. They tell you better not to use it. Its implementation is not always flawless with every chipset driver for XFree out there.

- With XFree 4.0.3 and nv.o there is a bug resulting in strange colors.
- ATI driver requires to switch mode back more than once after finishing using of DGA.
- Some drivers simply fail to switch back to normal resolution (use Ctrl-Alt-Keypad +, - to switch back manually).
- Some drivers simply display strange colors.
- Some drivers lie about the amount of memory they map into the process's address space, thus vo_dga won't use doublebuffering (SIS?).
- some drivers seem to fail to report even a single valid mode. In this case the DGA driver will crash telling you about a nonsense mode of 100000x100000 or the like ...
- OSD only works with doublebuffering enabled.

##### 2.3.1.3.9 Future work

- use of the new X11 render interface for OSD
- where is my TODO list ???? :-(((

##### 2.3.1.3.A Some modelines

      Section "Modes"
        Identifier    "Modes[0]"
        Modeline	"800x600"  40     800 840 968 1056  600 601 605 628
        Modeline	"712x600"  35.0   712 740 850 900   400 410 412 425
        Modeline	"640x480"  25.175 640 664 760 800   480 491 493 525
        Modeline 	"400x300"  20     400 416 480 528   300 301 303 314 Doublescan
        Modeline	"352x288"  25.10  352 368 416 432   288 296 290 310
        Modeline	"352x240"  15.750 352 368 416 432   240 244 246 262 Doublescan
        Modeline	"320x240"  12.588 320 336 384 400   240 245 246 262 Doublescan
      EndSection

These entries work fine with my Riva128 chip, using nv.o X server driver module.

##### 2.3.1.3.B Bug Reports

If you experience troubles with the DGA driver please feel free to file a bug report to me (e-mail address below). Please start MPlayer with the -v option and include all lines in the bug report that start with vo_dga:

Please do also include the version of X11 you are using, the graphics card and your CPU type. The X11 driver module (defined in XF86-Config) might also help. Thanks!

Acki (acki@acki-netz.de, www.acki-netz.de)

#### 2.3.1.4 SDL

SDL (Simple Directmedia Layer) is basically a unified video/audio interface. Programs that use it know only about SDL, and not about what video or audio driver does SDL actually use. For example a Doom port using SDL can run on svgalib, aalib, X, fbdev, and others, you only have to specify the (for example) video driver to use with the SDL_VIDEODRIVER environment variable. Well, in theory.

With MPlayer, we used its X11 driver's software scaler ability for cards/drivers that doesn't support XVideo, until we made our own (faster, nicer) software scaler. Also we used its aalib output, but now we have ours which is more comfortable. Its DGA mode was better than ours, until recently. Get it now? :)

It also helps with some buggy drivers/cards if the video is jerky (not slow system problem), or audio is lagging.

SDL video output supports displaying subtitles under the movie, on the (if present) black bar.

Here are some notes about SDL out in MPlayer.

There are several command line switches for SDL:
| `-vo sdl:name` |  | specifies sdl video driver to use (i.e.. aalib, dga, x11)
| `-ao sdl:name` |  | specifies sdl audio driver to use (i.e.. dsp, esd, arts)
| `-noxv` |  | disables XVideo hardware acceleration
| `-forcexv` |  | tries to force XVideo acceleration
SDL Keys:
| `F` |  | toggles fullscreen/windowed mode
| `C` |  | cycles available fullscreen modes
| `W/S` |  | mappings for * and / (mixer control)

#### KNOWN BUGS:

- Keys pressed under sdl:aalib console driver repeat forever. (use -vo aa!) It's bug in SDL, I can't change it (tested with SDL 1.2.1).

#### 2.3.1.5 SVGAlib

#### Installation

You'll have to install svgalib and its development package in order for MPlayer build its SVGAlib driver (autodetected, but can be forced), and don't forget to edit /etc/vga/libvga.config to suit your card & monitor.

#### Notes

Be sure not to use the -fs switch, since it toggles the usage of the software scaler, and it's slow. If you really need it, use the `-sws 4` option which will produce bad quality, but is somewhat faster.

#### EGA (4bpp) support

SVGAlib incorporates EGAlib, and MPlayer has the possibility to display any movie in 16 colors, thus usable in the following sets:

- EGA card with EGA monitor: 320x200x4bpp, 640x200x4bpp, 640x350x4bpp
- EGA card with CGA monitor: 320x200x4bpp, 640x200x4bpp

The bpp (bits per pixel) value must be set to 4 by hand:
`-bpp 4`
The movie probably must be scaled down to fit in EGA mode:
`-vop scale=640:350` or
`-vop scale=320:200`
For that we need fast but bad quality scaling routine:
`-sws 4`
Maybe automatic aspect correction has to be shut off:
`-noaspect`

#### 2.3.1.6 Framebuffer output (FBdev)

Whether to build the FBdev target is autodetected during ./configure . Read the framebuffer documentation in the kernel sources (Documentation/fb/*) for more information.

If your card doesn't support VBE 2.0 standard (older ISA/PCI cards, such as S3 Trio64), only VBE 1.2 (or older?): Well, VESAfb is still available, but you'll have to load SciTech Display Doctor (formerly UniVBE) before booting Linux. Use a DOS boot disk or whatever. And don't forget to register your UniVBE ;))

The FBdev output takes some additional parameters above the others:

| `-fb` |  | specify the framebuffer device to use (/dev/fb0)
| `-fbmode` |  | mode name to use (according to /etc/fb.modes)
| `-fbmodeconfig` |  | config file of modes (default /etc/fb.modes)
| `-monitor_hfreq` |  | IMPORTANT values, see example.conf
| `-monitor_vfreq` |
| `-monitor_dotclock` |

If you want to change to a specific mode, then use

`mplayer -vm -fbmode (NameOfMode) filename`

- -vm alone will choose the most suitable mode from /etc/fb.modes. Can be used together with -x and -y options too. The -flip option is supported only if the movie's pixel format matches the video mode's pixel format. Pay attention to the bpp value, fbdev driver tries to use the current, or if you specify the -bpp option, then that.
- -zoom option isn't supported (software scaling is slow). -fs option isn't supported. You can't use 8bpp (or less) modes.
- you possibly want to turn the cursor off: `echo -e '\033[?25l'` or `setterm -cursor off`
  and the screen saver: `setterm -blank 0`
  To turn the cursor back on: `echo -e '\033[?25h'` or `setterm -cursor on`

NOTE: FBdev video mode changing _does not work_ with the VESA framebuffer, and don't ask for it, since it's not an MPlayer limitation.

#### 2.3.1.7 Matrox framebuffer (mga_vid)

This section is about the Matrox G200/G400/G450/G550 BES (Back-End Scaler) support, the mga_vid kernel driver. It's active developed by me (A'rpi), and it has hardware VSYNC support with triple buffering. It works on both framebuffer console and under X.

WARNING: on non-Linux systems, use VIDIX for mga_vid!

To use it, you first have to compile mga_vid.o:

`cd drivers
make`

Then create /dev/mga_vid device:

`mknod /dev/mga_vid c 178 0`

and load the driver with

`insmod mga_vid.o`

You should verify the memory size detection using the 'dmesg' command. If it's bad, use the mga_ram_size option (rmmod mga_vid first), specify card's memory size in MB:

`insmod mga_vid.o mga_ram_size=16`

To make it load/unload automatically when needed, first insert the following line at the end of /etc/modules.conf:

`alias char-major-178 mga_vid`

Then copy the `mga_vid.o` module to the appropriate place under `/lib/modules/<kernel version>/somewhere`.

Then run

`depmod -a`

Now you have to (re)compile MPlayer, ./configure will detect /dev/mga_vid and build the 'mga' driver. Using it from MPlayer goes by '-vo mga' if you have matroxfb console, or '-vo xmga' under XFree86 3.x.x or 4.x.x.

The mga_vid driver cooperates with Xv.

The `/dev/mga_vid` device file can be read (for example by `cat /dev/mga_vid`) for some info, and written for brightness change: `echo "brightness=120" > /dev/mga_vid`

#### 2.3.1.8 SiS 6326 framebuffer (sis_vid)

SiS 6326 YUV Framebuffer driver -> sis_vid kernel driver

Its interface should be compatible with the mga_vid, but the driver was not updated after the mga_vid changes, so it's outdated now. Volunteers needed to test it and bring the code up-to-date.

#### 2.3.1.9 3dfx YUV support (tdfxfb)

This driver uses the kernel's tdfx framebuffer driver to play movies with YUV acceleration. You'll need a kernel with tdfxfb support, and recompile with `./configure --enable-tdfxfb`

#### 2.3.1.10 OpenGL output

MPlayer supports displaying movies using OpenGL, but if your platform/driver supports xv as should be the case on a PC with Linux, use xv instead, OpenGL performance is considerably worse. If you have an X11 implementation without xv support, OpenGL is a viable alternative.

Unfortunately not all drivers support this feature. The Utah-GLX drivers (for XFree86 3.3.6) support it for all cards. See http://utah-glx.sourceforge.net for details about how to install it.

XFree86(DRI) 4.0.3 or later supports OpenGL with Matrox and Radeon cards, 4.2.0 or later supports Rage128. See http://dri.sourceforge.net for download and installation instructions.

#### 2.3.1.11 AAlib - text mode displaying

AAlib is a library for displaying graphics in text mode, using powerful ASCII renderer. There are LOTS of programs already supporting it, like Doom, Quake, etc. MPlayer contains a very usable driver for it. If ./configure detects aalib installed, the aalib libvo driver will be built.

You can use some keys in the AA Window to change rendering options:
| `1` |  | decrease contrast
| `2` |  | increase contrast
| `3` |  | decrease brightness
| `4` |  | increase brightness
| `5` |  | switch fast rendering on/off
| `6` |  | set dithering mode (none, error distribution, Floyd Steinberg)
| `7` |  | invert image
| `a` |  | toggles between aa and MPlayer control)
The following command line options can be used:
| `-aaosdcolor=V` |  | change OSD color
| `-aasubcolor=V` |  | change subtitle color
| where V can be: (0/normal, 1/dark, 2/bold, 3/bold font, 4/reverse, 5/special)
AAlib itself provides a large sum of options. Here are some important:
| `-aadriver` |  | set recommended aa driver (X11, curses, Linux)
| `-aaextended` |  | use all 256 characters
| `-aaeight` |  | use eight bit ASCII
| `-aahelp` |  | prints out all aalib options

NOTE: the rendering is very CPU intensive, especially when using AA-on-X (using aalib on X), and it's least CPU intensive on standard, non-framebuffer console. Use SVGATextMode to set up a big textmode, then enjoy! (secondary head Hercules cards rock :)) (anyone can enhance fbdev to do conversion/dithering to hgafb? Would be neat :)

Use the `-framedrop` option if your computer isn't fast enough to render all frames!

Playing on terminal you'll get better speed and quality using the Linux driver, not curses (`-aadriver linux`). But therefore you need write access on `/dev/vcsa<terminal>`. That isn't autodetected by aalib, but vo_aa tries to find the best mode. See http://aa-project.sourceforge.net/tune/ for further tuning issues.

#### 2.3.1.12 VESA - output to VESA BIOS

This driver was designed and introduced as a generic driver for any video card which has VESA VBE 2.0 compatible BIOS. Another advantage of this driver is that it tries to force TV output on.
VESA BIOS EXTENSION (VBE) Version 3.0 Date: September 16, 1998 (Page 70) says:

> Dual-Controller Designs
> VBE 3.0 supports the dual-controller design by assuming that since both controllers are typically provided by the same OEM, under control of a single BIOS ROM on the same graphics card, it is possible to hide the fact that two controllers are indeed present from the application. This has the limitation of preventing simultaneous use of the independent controllers, but allows applications released before VBE 3.0 to operate normally. The VBE Function 00h (Return Controller Information) returns the combined information of both controllers, including the combined list of available modes. When the application selects a mode, the appropriate controller is activated. Each of the remaining VBE functions then operates on the active controller.

So you have chances to get working TV-out by using this driver.
(I guess that TV-out frequently is standalone head or standalone output at least.)

#### Advantages:

- You have the possibility to watch movies even if Linux doesn't know your video hardware.
- You don't need to have installed any graphics' related things on your Linux (like X11 (aka XFree86), fbdev and so on). This driver can be run from text-mode.
- You have chances to get working TV-out. (It's known at least for ATI's cards).
- This driver calls int 10h handler thus it's not an emulator - it calls real things of real BIOS in real-mode. (Finely - in vm86 mode).
- You can use Vidix with it, thus getting accelerated video display AND TV output at the same time! (recommended for ATI cards)

#### Disadvantages:

- It works only on x86 systems.
- It can be used only by root.
- Currently it's available only for Linux.

Don't use this driver with GCC 2.96! It won't work!

These switches of command line currently are available for VESA:
| `-vo vesa:opts` |  | currently recognized: dga to force dga mode and nodga to disable dga mode. Note: you may omit these parameters to enable autodetect of dga mode. (In the future also will specify mode parameters such as refresh rate, interlacing, doublescan and so on. Samples: i43, 85, d100)
| `-screenw, -screenh, -bpp` |  | force userdefined mode
| `-x, -y` |  | set userdefined prescaling
| `-zoom` |  | enables userdefined prescaling
| `-fs` |  | scales image to fullscreen
| `-fs -zoom` |  | scales userdefined prescaling to fullscreen
| `-double` |  | enables double buffering mode. (Available only in DGA mode). Should be slower of single buffering, but has no flickering effects.

#### Known problems and workaround:

- If you have installed NLS font on your Linux box and run VESA driver from text-mode then after terminating MPlayer you will have ROM font loaded instead of national. You can load national font again by using setsysfont utility from the Mandrake distribution for example.
  (Hint: The same utility is used for the localization of fbdev).
- Some Linux graphics drivers don't update active BIOS mode in DOS memory. So if you have such problem - always use VESA driver only from text-mode. Otherwise text-mode (#03) will be activated anyway and you will need restart your computer.
- Often after terminating VESA driver you get black screen. To return your screen to original state - simply switch to other console (by pressing Alt-Fx) then switch to your previous console by the same way.
- To get working TV-out you need have plugged TV-connector in before booting your PC since video BIOS initializes itself only once during POST procedure.

#### 2.3.1.13 X11

Avoid if possible. Outputs to X11 (uses shared memory extension), with no hardware acceleration at all. Supports (MMX/3DNow/SSE accelerated, but still slow) software scaling, use the options `-fs -zoom`. Most cards have hardware scaling support, use the `-vo xv` output for them, or `-vo xmga` for Matroxes.

The problem is that most cards' driver doesn't support hardware acceleration on the second head/TV. In those cases, you see green/blue colored window instead of the movie. This is where this driver comes in handy, but you need powerful CPU to use software scaling. Don't use the SDL driver's software output+scaler, it has worse image quality!

Software scaling is very slow, you better try changing video modes instead. It's very simple. See the DGA section's modelines, and insert them into your XF86Config.

- If you have XFree86 4.x.x - use the `-vm` option. It will change to a resolution your movie fits in. If it doesn't:
- With XFree86 3.x.x - you have to cycle through available resolutions with the CTRL-ALT-plus and minus keys.

If you can't find the modes you inserted, browse XFree86's output. Some drivers can't use low pixelclocks that are needed for low resolution video modes.

#### 2.3.1.14 VIDIX

#### WHAT IS VIDIX?

VIDIX is the abbreviation for VIDeo Interface for *niX.
VIDIX was designed and introduced as an interface for fast user-space drivers providing such video performance as mga_vid does for Matrox cards. It's also very portable.

This interface was designed as an attempt to fit existing video acceleration interfaces (known as mga_vid, rage128_vid, radeon_vid, pm3_vid) into a fixed scheme. It provides highlevel interface to chips which are known as BES (BackEnd scalers) or OV (Video Overlays). It doesn't provide lowlevel interface to things which are known as graphics servers. (I don't want to compete with X11 team in graphics mode switching). I.e. main goal of this interface is to maximize the speed of video playback.

#### USAGE

- You can use standalone video output driver: `-vo xvidix`
  This driver was developed as X11's front end to VIDIX technology. It requires X server and can work only under X server.
- You can use VIDIX subdevice which was applied to several video output drivers, such as:
  `-vo vesa:vidix` (Linux only) and `-vo fbdev:vidix`

Indeed it doesn't matter which video output driver is used with VIDIX.

#### REQUIREMENTS

- video card should be in graphics mode (I write should simply because I tested it in text mode - it works but has awful output ;) Use AAlib for that).
  Note: Everyone can try this trick by commenting out mode switching in vo_vesa driver.
- MPlayer's video output driver should know active video mode and be able to tell to VIDIX subdevice some video characteristics of server.

I hope that probably every video output driver of MPlayer will recognize `:vidix` subdevice.

#### USAGE METHODS

When VIDIX is used as subdevice (`-vo vesa:vidix`) then video mode configuration is performed by video output device (vo_server in short). Therefore you can pass into command line of MPlayer the same keys as for vo_server. In addition it understands `-double` key as globally visible parameter. (I recommend using this key with VIDIX at least for ATI's card).
As for `-vo xvidix`: currently it recognizes the following options: `-fs -zoom -x -y -double`.

Also you can specify VIDIX's driver directly as third subargument in command line:
`mplayer -vo xvidix:mga_vid.so -fs -zoom -double file.avi`
or
`mplayer -vo vesa:vidix:radeon_vid.so -fs -zoom -double -bpp 32 file.avi`
But it's dangerous, and you shouldn't do that. In this case given driver will be forced and result is unpredictable (it may freeze your computer). You should do that ONLY if you are absolutely sure it will work, and MPlayer doesn't do it automatically. Please tell about it to the developers. The Right Way is to use VIDIX without arguments to enable driver autodetection.

VIDIX is very new technology and it's extremely possible that on your system (OS=abc CPU=xyz) it won't work. In this case only solution for you it's port it (mainly libdha). But there is hope that it will work on those systems where X11 does.

> Warning: security risk
> Unfortunately you must have root privileges to use VIDIX due to direct hardware access. At least the SUID bit on the MPlayer executable must be set.

#### VIDEO EQUALIZER

This is a video equalizer implemented especially for VIDIX. You can use it either with 1-8 keys as described in the man page, or by command line arguments. MPlayer recognizes the following options:

| `-brightness` |  | Adjust BRIGHTNESS of video output. It's not equal to brightness adjusting on monitor panel or on TV. It changes intensity of RGB components of video signal from black to white screen.
| `-contrast` |  | Adjust CONTRAST of video output. Works in similar manner as brightness.
| `-saturation` |  | Adjust SATURATION of video output. You can get grayscale output with this option.
| `-hue` |  | Adjust HUE of video signal. You can get colored negative of image with this option.
| `-red_intensity` |  | Adjust intensity of RED component of video signal.
| `-green_intensity` |  | Adjust intensity of GREEN component of video signal.
| `-blue_intensity` |  | Adjust intensity of BLUE component of video signal.

Each parameter can accept values from -1000 to +1000.
Default value for each parameter is 0.

Note: Not every driver provides support for each of those parameters. Currently only radeon_vid.so provides full support for video equalizing. Other drivers only partly support these options.

Examples:
`mplayer -vo vesa:vidix -brightness -300 -contrast 200 filename.avi`
or
`mplayer -vo xvidix -red_intensity -50 -saturation 400 -hue 300 filename.vob`

#### 2.3.1.15 Zr

This is a display-driver (`-vo zr`) for a number of MJPEG capture/playback cards (tested for DC10+ and Buz, and it should work for the LML33, the DC10). The driver works by encoding the frame to jpeg and then sending it to the card. For the jpeg encoding libavcodec is used, and required.

This driver talks to the kernel driver available at http://mjpeg.sourceforge.net, so you must get it working first. Then recompile MPlayer with `--enable-zr`.

Some remarks:

- don't start or stop XawTV on the playback device during playback, it will crash your computer. It is, however, fine to FIRST start XawTV, THEN start MPlayer, wait for MPlayer to finish and THEN stop XawTV.
- this driver adds `-zr*` command line options. The explanation of these options can be viewed with `-zrhelp`. It is possible to crop the input frame (cut borders to make it fit or to enhance performance) and to do other things.
- the driver takes data in YV12 and YUY2 format, this means that some codecs won't work. Some old VfW (Video for Windows) codecs, for example, are incompatible with this driver. The error message that you will see is: `Sorry, selected video_out device is incompatible with this codec.`
- OSD is currently not supported, so you won't see subtitles.

#### 2.3.1.16 DVB

MPlayer supports cards with the Siemens DVB chipset from vendors like Siemens, Technotrend, Galaxis or Hauppauge. The latest DVB drivers are available from the Linux TV site. If you want to do software transcoding you should have at least a 1GHz CPU.

Configure should detect your DVB card. If it did not, force detection with

      ./configure --enable-dvb

If you have ost headers at a non-standard path, set the path with

      ./configure --with-extraincdir=<DVB source directory>/ost/include

Then compile and install as usual.

#### USAGE

Hardware decoding (playing standard MPEG1/2 files) can be done with this command:

      mplayer -ao mpegpes -vo mpegpes file.mpg|vob

Software decoding or transcoding different formats to MPEG1 can be achieved using a command like this:

      mplayer -ao mpegpes -vo mpegpes -vop lavc yourfile.ext
      mplayer -ao mpegpes -vo mpegpes -vop fame,expand yourfile.ext

Note that DVB cards only support heights 288 and 576 for PAL or 240 and 480 for NTSC. You must rescale for other heights by adding `scale=width:height` with the width and height you want to the `-vop` option. DVB cards accept various widths, like 720, 704, 640, 512, 480, 352 etc and do hardware scaling in horizontal direction, so you do not need to scale horizontally in most cases. For a 512x384 (aspect 4:3) DivX try:

      mplayer -ao mpegpes -vo mpegpes -vop lavc,scale=512:576

If you have a widescreen movie and you do not want to scale it to full height, you can use the `expand=w:h` plugin to add black bands. To view a 640x384 DivX, try:

      mplayer -ao mpegpes -vo mpegpes -vop lavc,expand=640:576 file.avi

If your CPU is too slow for a full size 720x576 DivX, try downscaling:

      mplayer -ao mpegpes -vo mpegpes -vop lavc,scale=352:576 file.avi

If speed does not improve, try vertical downscaling, too:

      mplayer -ao mpegpes -vo mpegpes -vop lavc,scale=352:288 file.avi

For OSD and subtitles use the expand feature of the OSD plugin. So, instead of `expand=w:h` or `expand=w:h:x:y`, use `expand=w:h:x:y:1` (the 5th parameter `:1` at the end will enable OSD rendering). You may want to move the image up a bit to get a bigger black zone for subtitles. You may also want to move subtitles up, if they are outside your TV screen, use the `-subpos <0-100>` switch to adjust this (`-subpos 80` is a good choice).

In order to play non-25fps movies on a PAL TV or with a slow CPU, add the `-framedrop` option.

To keep the aspect ratio of DivX files and get the optimal scaling parameters (hardware horizontal scaling and software vertical scaling while keeping the right aspect ratio), use the new dvbscale plugin:

    for  3:4 TV:  -vop lavc,expand=-1:576:-1:-1:1,scale=-1:0,dvbscale
    for 16:9 TV:  -vop lavc,expand=-1:576:-1:-1:1,scale=-1:0,dvbscale=1024

#### FUTURE

If you have questions or want to hear feature announcements and take part in discussions on this subject, join our MPlayer-DVB mailing list. Please remember that the list language is English.

In the future you may expect the ability to display OSD and subtitles using the native OSD feature of DVB cards, as well as more fluent playback of non-25fps movies and realtime transcoding between MPEG2 and MPEG4 (partial decompression).

#### 2.3.1.17 DXR3

MPlayer supports hardware accelerated playback with the Creative DXR3 and Sigma Designs Hollywood Plus cards.

First of all you will need properly installed DXR3/H+ drivers, version 0.12.0 or later. You can find the drivers and installation instructions at the DXR3 & Hollywood Plus for Linux site. Configure should detect your card automatically, compilation should go without any problems.

#### USAGE

| `-vo dxr3:<noprebuf>:<codec>:<device>` |  | Where `<noprebuf>` specifies turning off prebuffering. This is done automatically on Athlons. If playback is out of sync try disabling prebuffering. If noprebuf is left out prebuffering is enabled (except on Athlons). `<codec>` = fame/avcodec, avcodec produces better quality output, but fame is faster for those of you with slow machines. The default is to use libavcodec. Note that you need libavcodec properly installed (read DOCS/codecs.html). `<device>` = device number to use if you have more than one em8300 card. Any of these options may be left out, but they must be specified in this order, i.e. `dxr3:fame` works, `dxr3:1` works, but `dxr3:1:avcodec` will not.
| `-ao oss:/dev/em8300_ma-X` |  | For audio output, where `X` is the device number (0 if one card).
| `-ac hwac3` |  | For digital instead of analog audio output.
| `-vc mpegpes` |  | Force hardware acceleration, only works with MPEG1/2.
| `-aop list=resample:fout=xxxxx` |  | If sample rate is below 44100Hz, select either 44100Hz or 48000Hz depending on which one matches closest. I.e. if the movie uses 22050Hz use 44100Hz as 44100 / 2 = 22050, if it is 24000Hz use 48000Hz as 48000 / 2 = 24000 and so on. This does not work with digital audio output (`-ac hwac3`).

#### Overlay

To get overlay run dxr3view that comes with the em8300 package before starting MPlayer. You can set various options in dxr3view by pressing `T` while holding the mouse cursor above the window.

#### MPEG1, MPEG2, VCD and DVD Notes

MPEG1/2 content should now automatically be detected by MPlayer and it will use the hardware acceleration of the DXR3 to play it. If not, you can force it to hardware acceleration with `-vc mpegpes`. Also, if you plan to use any postprocessing filters you must use `-vc mpeg12`.

In some instances, subtitles may not appear properly in sync with the A/V stream when using hardware decoding (`-vc mpegpes`). This is a known bug. The em8300 will also improperly handle subtitles that are too big, and may hang for a second or two. At this time, the only workaround is to use `-vc mpeg12` when viewing DVDs with subtitles.

#### 2.3.1.A TV-out support

##### 2.3.1.A.1 Matrox G400 cards

Under Linux you have 2 methods to get G400 TV out working:

IMPORTANT: Only Matrox G400DH/G400MAX has TV-out support under Linux, others (G450, G550) have not!

- XFree86: using the driver and the HAL module, available from Matrox's site. This will give you X on the TV.
  This method doesn't give you accelerated playback as under Windoze! The second head has only YUV framebuffer, the BES (Back End Scaler, the YUV scaler on G200/G400/G450/G550 cards) doesn't work on it! The Windows driver somehow works around this, probably by using the 3D engine to zoom, and the YUV framebuffer to display the zoomed image. If you really want to use X, use the `-vo x11 -fs -zoom` options, but it will be SLOW, and has Macrovision copy protection enabled (you can "workaround" Macrovision using this perl script.
- Framebuffer: using the matroxfb modules in the 2.4 kernels. 2.2 kernels don't have the TVout feature in them, thus unusable for this. You have to enable ALL matroxfb-specific feature during compilation (except MultiHead), and compile them into modules! You'll also need I2C enabled.
  - Enter `TVout/matroxset` and type `make`. Install `matroxset` into somewhere in your PATH.
  - If you don't have `fbset` installed, enter `TVout/fbset` and type `make`. Install `fbset` into somewhere in your PATH.
  - Then enter into the `TVout/` directory in the MPlayer source, and execute `./modules` as root. Your text-mode console will enter into framebuffer mode (no way back!).
  - Next, run the `./matroxtv` script. This will present you to a very simple menu. Press 2 and ENTER. Now you should have the same picture on your monitor, and TV. The 3. option will turn on independent display, but then you can't use X! If the TV (PAL) picture has some weird stripes on it, the script wasn't able to set the resolution correctly (to 640x512 by default). Use other menu items randomly and it'll be OK :)

  Yoh. Next task is to make the cursor on tty1 (or whatever) to disappear, and turn off screen blanking. Execute the following commands:

  `echo -e '\033[?25l'` or `setterm -cursor off
  setterm -blank 0`

  You possibly want to put the above into a script, and also clear the screen.. To turn the cursor back:
  `echo -e '\033[?25h'` or `setterm -cursor on`

  Yeah kewl. Start movie playing with `mplayer -vo mga -fs -screenw 640 -screenh 512 <filename>`
  (if you use X, now change to matroxfb with for example CTRL-ALT-F1!)
  Change 640x512 if you set the resolution to other.
  Enjoy the ultra-fast ultra-featured Matrox TV output (better than Xv)!

##### 2.3.1.A.2 ATI cards

##### PREAMBLE

Currently ATI doesn't want to support any of its TV-out chips under Linux, because of their licensed Macrovision technology.

##### ATI CARDS TV-OUT STATUS ON LINUX

- ATI Mach64: supported by gatos.
- ASIC Radeon VIVO: supported by gatos.
- Radeon and Rage128: supported by MPlayer! Check VESA driver and VIDIX sections.

On other cards, just use the VESA driver, without VIDIX. Powerful CPU is needed, though.

Only thing you need to do - have TV connector plugged in before booting your PC since video BIOS initializes itself only once during POST procedure.

##### 2.3.1.A.3 Voodoo 3

Check this URL.