## UPNP_CONTROL_ACTION_REQUEST

> Received by a device when a control point issues a control request.

## Documentation

> Received by a device when a control point issues a control request. The Event parameter contains a pointer to a Upnp_Action_Request structure containing the action. The application stores the results of the action in this structure.

Alphabetic index

This page was generated with the help of DOC++.