## Initialization and Registration

UpnpInit
  Initializes the Linux SDK for UPnP Devices.
UpnpFinish
  Terminates the Linux SDK for UPnP Devices.
UpnpGetServerPort
  If '0' is used as the port number in UpnpInit, then this function can be used to retrieve the actual port allocated to the SDK.
UpnpGetServerIpAddress
  If `NULL` is used as the IP address in UpnpInit, then this function can be used to retrieve the actual interface address on which device is running.
UpnpRegisterClient
  UpnpRegisterClient registers a control point application with the SDK.
UpnpRegisterRootDevice
  UpnpRegisterRootDevice registers a device application with the SDK.
UpnpRegisterRootDevice2
  UpnpRegisterRootDevice2 is similar to UpnpRegisterRootDevice, except that it also allows the description document to be specified as a file or a memory buffer.
UpnpUnRegisterClient
  UpnpUnRegisterClient unregisters a control point application, unsubscribing all active subscriptions.
UpnpUnRegisterRootDevice
  Unregisters a root device registered with UpnpRegisterRootDevice or UpnpRegisterRootDevice2.
UpnpSetContentLength
  OBSOLETE METHOD : use UpnpSetMaxContentLength instead.
UpnpSetMaxContentLength
  Sets the maximum content-length that the SDK will process on an incoming SOAP requests or responses.

Alphabetic index

This page was generated with the help of DOC++.