## enum UPnP_EventType

> The reason code for an event callback.

> The Event parameter will be different depending on the reason for the callback. The descriptions for each event type describe the contents of the Event parameter.

UPNP_CONTROL_ACTION_REQUEST
  Received by a device when a control point issues a control request.
UPNP_CONTROL_ACTION_COMPLETE
  A UpnpSendActionAsync call completed.
UPNP_CONTROL_GET_VAR_REQUEST
  Received by a device when a query for a single service variable arrives.
UPNP_CONTROL_GET_VAR_COMPLETE
  A UpnpGetServiceVarStatus call completed.
UPNP_DISCOVERY_ADVERTISEMENT_ALIVE
  Received by a control point when a new device or service is available.
UPNP_DISCOVERY_ADVERTISEMENT_BYEBYE
  Received by a control point when a device or service shuts down.
UPNP_DISCOVERY_SEARCH_RESULT
  Received by a control point when a matching device or service responds.
UPNP_DISCOVERY_SEARCH_TIMEOUT
  Received by a control point when the search timeout expires.
UPNP_EVENT_SUBSCRIPTION_REQUEST
  Received by a device when a subscription arrives.
UPNP_EVENT_RECEIVED
  Received by a control point when an event arrives.
UPNP_EVENT_RENEWAL_COMPLETE
  A UpnpRenewSubscriptionAsync call completed.
UPNP_EVENT_SUBSCRIBE_COMPLETE
  A UpnpSubscribeAsync call completed.
UPNP_EVENT_UNSUBSCRIBE_COMPLETE
  A UpnpUnSubscribeAsync call completed.
UPNP_EVENT_AUTORENEWAL_FAILED
  The auto-renewal of a client subscription failed.
UPNP_EVENT_SUBSCRIPTION_EXPIRED
  A client subscription has expired.

Alphabetic index

This page was generated with the help of DOC++.