


CVTMT(4)            UNIX Programmer's Manual             CVTMT(4)



NNAAMMEE
     cvt_meta_tbl - Meta key conversion table of Input Manager of
     the X Window System Version 11 (xwnmo(1X))

SSYYNNOOPPSSIISS
     //uussrr//llooccaall//lliibb//wwnnnn//ccvvtt__mmeettaa__ttbbll (Default)

DDEESSCCRRIIPPTTIIOONN
     Converts a meta key code(_K_e_y_S_y_m) generated by _X_L_o_o_k_u_p_-
     _S_t_r_i_n_g() to a one-byte character(_W_n_n _c_o_d_e) according to
     preset data.

     CCooddiinngg ffoorrmmaatt::
             [ _K_e_y_S_y_m-_e_n_t_r_y <space_character> _W_n_n-_c_o_d_e ]

     Lines that start with a semicolon (;) are comments.

     CCooddee nnoottaattiioonn::
             0??             ---> Octal
             0x?? or 0X??    ---> Hexadecimal
             ??              ---> Decimal

EEXXAAMMPPLLEE
     Left            0x9A
     Up              0x99
     Right           0x9B
     Down            0x9C
     F11             0x95
     F12             0x96
     F13             0x97
     F14             0x98
     minus           0x81
     asciicircum     0x82
     backslash       0x83

NNOOTTEESS
     Codes converted according to this table will be evaluated by
     _2_A__C_T_R_L (default), which is an alphanumeric-phonetic conver-
     sion automation table. After which, they are evaluated by
     _u_u_m_k_e_y.

SSEEEE AALLSSOO
     xwnmo(1X), 2A_CTRL(4_JT), uumkey(4_JT), cvt_xim_tbl(4X),
     cvt_fun_tbl(4X)

CCOOPPYYRRIIGGHHTT
     Copyright 1991 by OMRON Corporation
     Copyright 1991 by Massachusetts Institute of Technology

AAUUTTHHOORR
     Seiji Kuwari (OMRON Corporation)



Printed 12/1/92             Release 5                           1






































































