## UPNP_DISCOVERY_SEARCH_RESULT

> Received by a control point when a matching device or service responds.

## Documentation

> Received by a control point when a matching device or service responds. The Event parameter contains a pointer to a Upnp_Discovery structure containing the information about the reply to the search request.

Alphabetic index

This page was generated with the help of DOC++.